Skip to content

# SP750

- Next Product

## SP750

⦁ 80 PLUS GOLD Efficiency
⦁ Fully modular braided cables for a clean look
⦁ Japanese electrolytic capacitors for high durability
⦁ ZERO RPM mode under 40% load for silent operation
⦁ Sleek and classic exterior with brushed aluminum housing

Category: Power supply Tags: Aluminum PSU, braided cables, LIAN LI PSU, Modular cabler, O11D MINI PSU, SFF Build PSU, SFX PSU

- Description

The SP750 is a stylish high-performance PSU that perfectly fits small-form-factor PCs while supporting power-hungry components.

# Available in two color

Sleek Black Look with Aluminum Housing Completely White Designing.

# 80 PLUS Gold Certificate

SP750 guarantees up to 92% efficiency, ensuring less power wastage.

# SP750 Composition

# Cooling in Silence

The SP750 features a 92mm hydraulic bearing fan that operates at zero RPM mode until 40% load in order to achieve minimal acoustic levels.

ACOUSTIC NOISE (Ambient Temperature is 25°C)

Note : Internal components reach 60°C will also trigger fan to operate

# Japanese Electrolytic Capacitors

Premium Japanese electrolytic capacitors provide great durability and long-term reliability, as well as offering the highest stability.

# Fully Modular Connection and Included Braided Cables

The fully modular power supply provides all necessary braided cables right out of the box, ensuring less cable clutter and more aesthetics.

CPU / ATX12V Connector x1

2 x 8 PIN PCIe Connector x1

1 x 8 PIN PCIe Connector x1

Motherboard Connector x1

SATA Connector x2

Peripheral Connector x1

# SP750 Connector Type for Custom Cables

Note: Damage caused by custom cables doesn’t include in the warranty.

# Multi Power Cord Types

# Five Years Warranty

LIAN LI offers a 5-year limited warranty for the SP750, reflecting our confidence in the quality of our performance SFX PSU.

### SPECIFICATIONS

MODEL | SP750 BLACK / SP750 WHITE
Dimensions | (D)100 mm X (W)63.5mm X (H)125 mm
Power supply design | Fully modular
Color | Black / White
Material | Steel/brushed aluminum housing
Form factor | SFX
Certification | 80 PLUS Gold
Max. DC Output | 750W
Combined +3.3V & +5V | 100W
Combined +12V | 744W
Input Voltage | 100 – 240 Vrms
Input Frequency Range | 50Hz – 60 Hz
PFC | Active PFC (PF)>0.90 at full load
Efficiency | 91.89% Max
Protective Circuit | OCP/ OPP/ UVP/ OVP/ OTP/ SCP
Connectors | 1 x 24 / 20-Pin motherboard connector (300mm) x 1pcs 2 x 8 / 4-Pin CPU / ATX 12V connector (450mm-70mm) x 1 pcs 1 x 8 / 6+2 Pin PCIe connector (400mm) x 1pcs 2 x 8 / 6+2 Pin PCIe connector (400mm-120mm) x 1pcs 4 x SATA connector (120mm-120mm-120mm-120mm) x 2pcs 4 x 4-Pin Peripheral connector (120mm-120mm-120mm-120mm) x 1pcs
750W FAN RPM | 1000-2800 RPM
Noise Level | 17.1-43.1 DBA
Bearing Type | 31.Fluid Dynamic Bearing (FDB)
Warranty | 5 years

Search this website Type then hit enter to search
×

By continuing to use this website, you consent to the use of cookies in accordance with our Cookie Policy.