AS350 PANTHER SATA III

SATA III SSD

AS350 PANTHER SATA III

SATA III SSD

AS350 PANTHER SATA III

 Compatible with SATA III 6.0 Gb/s Interface

 Sequential Read/Write Speed up to 560/540MB/s

 Supports SATA Power Management

                                    Explore the Peaks of High Speed
                                

                                        AS350X is Apacer's latest mid-to-high-end SSD. It uses a new generation of SATA III interface and provides 6Gb/s transmission speeds, enabling it to reach read/write speeds of up to 560/540 MB/s.
                                    

                                    First Choice for Computer Upgrades
                                

                                        The high-speed access performance of the AS350X offers users a superior computing experience. Bootups and program runtimes will take place in just a few seconds. The AS350X offers options including 128GB, 256GB, 512GB and 1TB. Thanks to Apacer's SSD Utility software, users are able to monitor all the relevant information about the status of their drives without extra cost.
                                    

                                    Excellent Performance with Optimized Durability and Stability
                                

                                        AS350X has an extended lifespan with improved operation stability, maintaining consistent performance even after years of use.
                                    

Spec

Product Name

AS350 PANTHER

Capacity

128GB~1TB

Interface

SATA III

NAND Flash

3D NAND

Sequential Read Performance

128GB：Up to 560MB/s

256GB：Up to 560MB/s

512GB：Up to 560MB/s

1TB：Up to 560MB/s

Sequential Write Performance

128GB：Up to 540MB/s

256GB：Up to 540MB/s

512GB：Up to 540MB/s

1TB：Up to 540MB/s

*The performance may vary due to host hardware, software , usage and storage capacity.

IOPs (4K Random Write)

Up to 30,176IOPs

ECC Support

Up to 72bit/1KB

Shock

1,500G/0.5msec

Vibration

5~2000Hz/20G

Low Power Consumption (Active/Idle)

275/80mA

MTBF

1,500,000 hours

Humidity

5% ~95%

Standard Operating Temperature

0°C ~ +70°C

Storage Temperature

-40 ~ +85°C

Dimensions

(L)100 x (W)69.9 x (H)7 mm

Certificate

CE, FCC, VCCI, BSMI, RoHS

Warranty

3 Years

*The SSD is based on the TBW or Warranty period.