# Polaris Vac-Sweep 280

## Our most popular automatic pool cleaner

SKU #F5

Our most popular pressure pool cleaner, the Polaris Vac-Sweep 280 pressure-side pool cleaner works in all in-ground pools and requires a booster pump. It is powered by double jets, providing greater vacuum power and faster cleaning (3 hours or less). The Polaris 280 easily connects to a dedicated pressure line and sweeps, scrubs, and vacuums all surfaces of the pool. The pressure cleaner is equipped with a single chamber filter bag where it captures large debris such as leaves, acorns, pebbles, and other small to large debris. Its unique filter bag removes debris before it reaches your pump basket or filter, prolonging the life of your filtration system.

Buy Now

View Specifications

# Greater Vacuum Power and Faster Cleaning

- Powered by double jets, cleans a pool faster (3 hours or less)
- Works in all in-ground pools of any size and shape
- Sweeps, scrubs, and vacuums the bottom and walls of your pool
- Runs off a separate booster pump
- Includes 31-feet of feed hose, and equipped with single chamber filter bag for capturing larger debris
- Available in a Black Max™ model to complement dark-bottom pools
- Available in a TankTrax model to get to those hard-to-reach places

## Polaris Vac-Sweep 280 Specifications

## Polaris Vac-Sweep 280 User Guides

Document ID TL-1013
Description Polaris Hose Connector Replacement Instructions
File Size 478.49 KB
|
File Type PDF
Document ID SL825
Description Polaris Inground Cleaner Family Brochure
File Size 1.42 MB
|
File Type PDF
Document ID TL-200
Description Polaris 280 I/O Manual
File Size 493.7 KB
|
File Type PDF
Document ID SL200
Description Polaris 280 Data Sheet
File Size 502.74 KB
|
File Type PDF
Document ID TL-205
Description Polaris 280 Factory Rebuild Kit
File Size 136.04 KB
|
File Type PDF
Document ID TL-206
Description Polaris 280 TankTrax Conversion Kit Installation
File Size 654.23 KB
|
File Type PDF
Document ID H0409800
Description Polaris 280 Quick Start Guide
File Size 1.09 MB
|
File Type PDF

## Polaris Vac-Sweep 280 Frequently asked questions

Verify that the wheel RPM's are in the correct range and adjust the thrust jet. If the cleaner isn't climbing well then ensure the thrust jet is in the 11 o'clock position. If it is going in circles then angle the thrust jet so it is pointing opposite of the way the cleaner is turning. For example, if the cleaner is turning right then point the thrust jet to the left.

1. Turn the appliance over and check the suction by making sure that all the jets located in the central pipework are working correctly. If they aren’t, make sure they are not blocked.
2. Fit the special tires for smooth tiled surfaces (Ref. C-13).

1. Check the wheel RPM.
2. Verify the back-up valve is cycling.
3. Adjust the thrust jet.
4. Remove unnecessary pool hardware or install a Ladder Guard Kit (order part #G21 from a Polaris dealer).

Check swivels and make sure they are spinning freely. Lay the hose out in the sun for 24 hours to eliminate any potential hose memory.

Hold the back up valve out of the water and verify that it cycles on and off. A complete cycle takes about three minutes. If it stays on all the time or doesn't come on at all then replace the back up valve.

1. Check the wheel RPM. If more than 32 RPM, unscrew the pressure relief valve to decrease water flow to cleaner.
2. Confirm that the blue restrictor disc is installed in the UWF to decrease water flow. Or, install the red restrictor disc to decrease water flow even more.
3. Verify the back-up valve is cycling. Hold the valve out of the water and watch the jet. It should come on and go off.

1. Check the filter screen in the Quick Disconnect and clean, if necessary.
2. Clean the skimmer basket, pump basket, and pool filter.
3. Check all of the hoses, connections, and swivels for leaks that cause loss of water pressure.
4. Check the wheel RPM.

1. Adjust the thrust jet.
2. Make sure feed hose is floating.

1. Make sure the opening at the end of the sweep hose is not blocked by the sweep hose scrubber.
2. Adjust the sweep hose to a gentle sweeping motion.

1. Adjust the speed of the sweep hose by tightening the adjustment screw.
2. Replace the sweep hose scrubber if it is worn or missing.
3. Add a sweep hose weight (Part No. B2) to keep the sweep hose from spraying.

1. Verify that feed hose reaches within 6" of the farthest point of the pool. If not, order a new hose section from your Polaris dealer.
2. Check the thrust jet for straight back position that optimizes random turning.
3. While the cleaner is operating, hold it upside down and look into the vacuum tube. There should be two distinct, even jets of water. If there are not, contact Customer Service or a Polaris authorized Service Center for assistance.

1. Check the filter bag, if full it can weigh the cleaner down on one side.
2. Remove the head float and shake it. If there is water in the float, order a new one.
3. Check the hose floats to make sure they are spaced evenly.

1. Use the Polaris pressure tester to check the booster pump pressure.
2. Check that the metal pre-filter is present and not clogged.
3. Make sure that the hose weight adjustment nut is screwed down correctly.
4. Make sure the hoses have been cut as indicated in the instructions.
5. Make sure that the blue reducing disk has not been installed in the quick disconnect.
6. Check that the booster pump is working normally.
7. Clean the skimmer baskets, sand filter, and pump basket.

1. Unscrew the hose-weight adjustment nut until the desired setting is obtained.
2. Fit the flow limiter (red or blue) into the quick disconnect.

Verify the wheel RPM's are in range. If they are low or the wheels are not spinning then check the in-line filter for debris. If clear and the wheels still aren't spinning then check the water management system for clogs. If the RPM's are slightly below the prescribed range then remove the restrictor disc from the wall connector. If the wheels are moving too quickly then install the red restrictor disc.

Verify the wheel RPM's are in range. Ensure that the head float is not filled with water. Try running the cleaner without the bag and if it fixes the issue then clean the bag with soap and warm water. This will remove any biofilm/oils that may have accumulated in the bag.

## Polaris Vac-Sweep 280 Related Products

### Polaris PB4SQ

4.9 Stars (77 Reviews)

The PB4SQ is an energy-efficient, multistage booster pump
that operates quietly and is easy to install and service.

View details

### Polaris PB4-60

4.9 Stars (1000 Reviews)

The PB4-60 delivers the best combination of high-performance power, quiet operation, and durability.

View details

### Polaris TR28P Pressure Pool Cleaner

4.7 Stars (68 Reviews)

The Polaris® TR28P vacuums and effectively sweeps and scrubs with the TailSweep PRO®, collecting debris into an attached debris bag to help prolong the longevity of your pool’s filtration system.

View details

### Polaris Vac-Sweep 380

4.7 Stars (458 Reviews)

Powered by triple jets and a separate booster pump, the Polaris 380 is one of our most powerful, durable cleaners, is suitable for all in-ground pools, and requires a booster pump.

View details

### Polaris Vac-Sweep 360

4.7 Stars (1000 Reviews)

Our most advanced pressure-side automatic pool cleaner that operates without a separate booster pump.

View details

## Polaris Vac-Sweep 280 Spare Parts & Accessories

K13

### K13 All-Purpose Debris Bag With Zippered Closure

K14

### K14 Sand/Silt Debris Bag

K16

### K16 All-Purpose Debris Bag

K17

### K17 All-Purpose Debris Bag

G52

### G52 Back-Up Valve

9-100-9001

### 9-100-9001 Universal Wall Fitting

C10

### C10 Max Trax Tire

Compatible Models
Polaris 380, 360, 280, 180

C60

### C60 Ball Bearing for Wheel

C6

### C6 Large Wheel

B5

### B5 Sweep Hose

G5

### G5 Feed Hose w/ UWF®

C86

### C86 Drive Shaft Assembly

A49

### A49 Factory Tune-Up Kit