Remove Product?
Are you sure you want to remove the following product from the cart?

Remove Coupon?
Are you sure you want to remove the following coupon from the cart?

Forgot your Password

Provide your account email address to receive an email to reset your password.

Email

# WRT3200ACM AC3200 Gigabit Wi-Fi Router

https://www.linksys.com/ca/wrt3200acm-ac3200-gigabit-wi-fi-router/WRT3200ACM-CA.html

# WRT3200ACM AC3200 Gigabit Wi-Fi Router

SKU: WRT3200ACM-CA
5 out of 5 Customer Rating

# WRT3200ACM AC3200 Gigabit Wi-Fi Router

SKU: WRT3200ACM-CA
5 out of 5 Customer Rating

Bring ultra-fast AC Wi-Fi to your home with the one and only WRT3200ACM Wi-Fi Router. Equipped with Tri-Stream 160, this open-source router delivers blazing-fast, uninterrupted dual-band Wi-Fi speeds to multiple devices at the same time.

Find a Retailer
Warranty Information: 1

- Tri-Stream 160 technology
- Open source ready with OpenWrt® and DD-WRT®

Number of Ethernet Ports

- 1x Gigabit WAN port
- 4x Gigabit LAN ports

Certified Operating Systems

- MacOS (10.X or higher), Windows 7, Windows 8.1 (Works with Windows 10)

Wi-Fi Range

- Very Large Household

LEDs

- Power, Internet, 2.4 GHz, 5 GHz, eSATA, USB1 (USB 2.0), USB2 (USB 3.0), LAN 1–4 (activity/10/100 Mbps), LAN 1–4 (1 Gbps), WPS

Dimensions (LxWxH)

- 245.87 x 193.80 x 51.82 mm(9.68 x 7.63 x 2.04 in.) without antennas

Weight

- 798.32 g(28.16 oz)

Operation Modes

- Access Point
- Wired Bridge
- Wireless Bridge
- Wireless Repeater
- Wireless Router

Minimum System Requirements

- Firefox® 8
- Google Chrome™
- Internet Explorer® 8
- Safari® 5 (for Mac®)

Wi-Fi Speed

- AC3200 (N600 + AC2600)

Storage File System Support

- FAT, NTFS, and HFS+

Operating Humidity

- 10 to 80% Noncondensing

Operating Temperature

- 32 to 104 F (0 to 40 C)

Security Features

- 128 bit AES link encryption
- WPA/WPA2

Wi-Fi Technology

- AC3200 Dual-band Gigabit, 600+2600 Mbps

Easy Setup

- Browser-based Setup
- Linksys Smart Wi-Fi Setup

Storage Temperature

- -4 to 140 F (-20 to 60 C)

Additional Information

- Open Source ready for OpenWrt, DD-WRT

Key Features

- 802.11a
- 802.11ac
- 802.11g
- 802.11n

VPN Support

- IPSec pass‐through
- PPTP

Power Supply

- Input: 100-240V ~ 50-60Hz; Output: 12V, 3.0A

Antennas

- 4x external, dual-band, detachable antennas

Wireless Encryption

- WPA2 Personal, WPA2 Enterprise

Regulatory Compliance

- FCC class B

Other Ports

- One(1) Combo eSATA/USB 2.0 port
- One(1) USB 3.0 port
- Power

Processor

- 1.8 GHz dual-core

Wi-Fi Bands

- 2.4 and 5 GHz (simultaneous dual-band)

Other Certifications

- FCC DFS Certified

- Linksys WRT3200ACM
- Quick Start Guide
- CD-ROM with Documentation
- 4 Antennas
- Ethernet Cable
- Power Adapter

*Fastest 5 GHz band claim is made as of August 26, 2016 (ex-factory date). Tri-Stream 160 with 2x bandwidth for 5 GHz band is based on achieving 3x 160 MHz at 867 Mbps = 2.6 Gbps, which is up to 2x more bandwidth when compared to an AC1900 router with 3x 80 MHz at 433 Mbps = 1.3 Gbps.

†While Linksys fully embraces the open source community and is providing open source use capabilities, they do not offer technical support on using open source firmware. Installing 3rd party firmware is done at your own risk and replacing factory-installed firmware with open source firmware will void your warranty. Please always seek the advice of more experienced users via open source community forums if you’re unsure.