Smooth starting KOHLER® XT675 149cc engine with Easy-Pull™ technology for ease of engine starting
Maintenance-free OEM Technologies™ vertical axial cam pump
Powder-coated steel frame for corrosion resistance and 12'' never-flat wheels for portability

Kärcher® FATMAX® gas powered premium pressure washers are designed to provide maximum performance with professional quality.

Ergonomic spray gun designed for comfort and control with adjustable pressure regulator (M22 connectors)
35' MorFlex™ poly-braided abrasion resistant high pressure hose
Four spray nozzles; 0 °, 15 °, 40 ° and soap