







































375 Series T4F Portable Diesel Compressors | Sullair
































































































Contact Us


Search


















Search














































Contact Us


























Hitachi Global Air Power US, LLC














Skip to main content


 
















 
Language: English






English
Español
Français












 
Region: Americas






Americas


Asia


Australia


EMEA/CIS


Global










Header Submenu








About






News






Events






Careers






Channel Partners






Suppliers










Find A Local Rep


1-800-SULLAIR
1-219-879-5451


























 








Search














Find A Local Rep


1-800-SULLAIR


1-800-785-5247 or 1-219-879-5451
























Main navigation












Menu
















Products






Industrial Air Compressors






Oil Free Air Compressors






Portable Diesel Air Compressors






Portable Electric Air Compressors






Compressed Air Dryers






Filters, Separators, & Drains






Air Systems Management










Industry






Parts & Fluids






Genuine Air Compressor Parts










OEM






Services






Air Compressor Service & Repair










Blog






Contact




































Home






Products





                  375 Series T4F Portable Diesel Compressors
              
















375 Series T4F Portable Diesel Compressors
























400HH
DESIGNED TO GET THE JOB DONE


Sullair 375 Series portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the 375 compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.


Compact design


Easy pressure change


Extended runtime


Available with your choice of a reliable Caterpillar or Perkins engine!






Models vary by region. Please contact your Sullair sales representative for more details.




Jump To:


Specs


Contact Us








 
































Flow







           375 – 425
      
 cfm





           10.6 – 12
      
 m³/min




 










Pressure







           150 – 200
       psi





           10.3 – 13.8
       bar


 












Power







           122 – 157
       hp





           91 – 117
       kW


 




























Features & Benefits 


 


Options


 


Models & Specs


 








Features & Benefits 




Multiple Engine Options
	
Caterpillar C4.4 (T4F)


Perkins 1204F (T4F)




Compact Design
	
Easier towing to and from the job site


Improved maneuverability — fits more easily in smaller space


More convenient storage — on the job site or at the yard




Easy Pressure Change
	
Select models shift from low to high pressure with the turn of a switch




Quiet Operation
	
74 decibels at 23 feet operating at full load




Extended Runtime
	
Oversized 65 gallon tank


Up to 10 hours of runtime at full load
		
5–7% improvement in fuel consumption at full load compared to previous models






Easy Service and Maintenance
	
Swing doors with slam latches to ensure doors stay open


Easy access to key components including:
		
Cooler; aftercooler (if equipped)


Compressor fluid and air filters


Engine filters


Battery and battery disconnect






Legendary Sullair 16-Series Air End


Low Fuel Shutdown


Discharge Temperature Sensor


Electric Brakes


LED Tail Lights


LED Turn Lights


Clearance Lights


Sullair AWF® All Weather Fluid — Factory Fill Lubricant




 




Options




Cold weather package


Jack caster with wheels


Mechanical parking brake


Single or dual hose reels


Aftercooled and filtered




 




Models & Specs




Performance by Model


375H


Actual Delivery
 
cfm (m³/min):
 375 (10.6)


Rated Pressure
 
psig (bar):
 150 (10.3)


Pressure Range
 
min/max (bar):
 80 (5.5) / 175 (12.1)


Fuel Consumption Full Load
 
gal/h (l/h):
 5.9 (22.3)


Maximum Operating Altitude
 
ft (m):
 9000 (2743)


Makes & Models:
 CAT C4.4 & Perkins 1204F (T4F)


Operating Speed
 
rpm:
 2100


Available Power
 
bhp (kW):
 122 (91)


Displacement
 
in³/l:
 269 (4.4)


Cooling System Capacity
 
gal (l):
 6.9 (26)


Engine Oil Capacity
 
qts (l):
 8.5 (8)


Fuel Tank Capacity
 
gal (l):
 65 (246)


Electrical System Voltage:
 12


Battery Rating
 
CCA:
 1125


DEF Consumption
 
% of Fuel:
 2.3%


DEF Capacity
 
gal (l):
 5 (19)


Service Valves
 
No. & (Size):
 2 (¾")


Compressor Oil Capacity
 
gal (l):
 8 (30)


400HH


Actual Delivery
 
cfm (m³/min):
 400 (11.3)


Rated Pressure
 
psig (bar)
: 200 (13.8)


Pressure Range
 
min/max (bar):
 80 (5.5) / 225 (15.5)


Fuel Consumption Full Load
 
gal/h (l/h):
 7.4 (28)


Maximum Operating Altitude
 
ft (m):
 9000 (2743)


Makes & Models:
 CAT C4.4 & Perkins 1204F (T4F)


Operating Speed
 
rpm:
 1900


Available Power
 
bhp (kW):
 157 (117)


Displacement
 
in³/l:
 269 (4.4)


Cooling System Capacity
 
gal (l):
 6.9 (26)


Engine Oil Capacity
 
qts (l):
 12 (11.5)


Fuel Tank Capacity
 
gal (l):
 65 (246)


Electrical System Voltage:
 12


Battery Rating
 
CCA
: 1125


DEF Consumption
 
% of Fuel:
 2.3%


DEF Capacity
 
gal (l):
 5 (19)


Service Valves
 
No. & (Size):
 1 (1 ½ ")


Compressor Oil Capacity
 
gal (l):
 8 (30)


425H


Actual Delivery
 
cfm (m³/min):
 425 (112)


Rated Pressure
 
psig (bar):
 150 (10.3)


Pressure Range
 
min/max (bar):
 80 (5.5) / 175 (12.1)


Fuel Consumption Full Load
 
gal/h (l/h):
 7.7 (29.1)


Maximum Operating Altitude
 
ft (m):
 9000 (2743)


Makes & Models:
 CAT C4.4 & Perkins 1204F (T4F)


Operating Speed
 
rpm:
 2100


Available Power
 
bhp (kW):
 157 (117)


Displacement
 
in³/l:
 269 (4.4)


Cooling System Capacity
 
gal (l):
 6.9 (26)


Engine Oil Capacity
 
qts (l):
 ;12 (11.5)


Fuel Tank Capacity
 
gal (l):
 65 (246)


Electrical System Voltage:
 12


Battery Rating
 
CCA:
 1125


DEF Consumption
 
% of Fuel:
 2.3%


DEF Capacity
 
gal (l):
 5 (19)


Service Valves
 
No. & (Size):
 2 (¾ ")


Compressor Oil Capacity
 
gal (l):
 8 (30)


Weights & Dimensions for 375H, 400HH, 425H


DPQ Package — Includes Running Gear


Working weight
 
lbs (kg):
 4840 (2195)


Dry weight
 
lbs (kg):
 4200 (1905)


Length
 
in (mm):
 156 (3962)


Width
 
in (mm):
 78 (1958)


Height
 
in (mm):
 76 (1921)


Track Width
 
in (mm):
 67 (1702)


Max Towing Speed
 
mph (km/h):
 55 (89)


Axle Rating
 
lbs (kg):
 5000 (2268)


Tire Size
: 225/75R15


DLQ Package — Less Running Gear


Working weight
 
lbs (kg):
 4610 (2092)


Dry weight
 
lbs (kg):
 3970 (1801)


Length
 
in (mm):
 101 (2577)


Width
 
in (mm):
 59 (1506)


Height
 
in (mm):
 64 (1619)




*Non-aftercooled 






 




















How to Buy












Get More Info












Download the Brochure




 












On


Off


Off


Off
















Related Products


















 




185 Series T4F Portable Diesel Compressors


View Product




 




Sullair Certified Glider Program for Towable Air Compressors 


View Product




 




AWF® Compressor Fluid


View Product


































Related Products 2






















International 185 T3 Portable Diesel Compressors
View Product














SULLAIR RECON PROGRAM
View Product














Customer Fleet Management Parts Program (C.F.M)
View Product






































NEED HELP FINDING THE
RIGHT SOLUTION




INTERACTIVE GUIDE   


































Hitachi Global Air Power US, LLC




North America Operations

1 Sullair Way

Michigan City, IN 46360






























SULLAIR






About






Brand Promise






Quality & Value






Sustainability






News






Events






Careers






Blog










Equipment






Stationary






Portable


















Parts






Fluid Filters






Air Filters






Downstream Filters






Fluids






Fluid Analysis






Separators










Services






Air System Management










OEM






Drill Compressors






Process Gas Compressors






Receiver Tanks


















Industry






Automotive






Chemical & Petrochemical






Construction & Mining






Food & Beverage






Gas Compression






General Manufacturing






Life Sciences






Oil & Gas






Power Generation










Contact






Find a Local Representative










Channel Partners






Suppliers






























This site uses 
essential cookies
 for core functionality and 
analytics cookies
 to collect anonymous usage data. Click “Accept Cookies” to accept all cookies or “Cookie Settings” to choose which types of cookies you wish to accept. 
View our Privacy Policy.


Accept Cookies
 
Cookie Settings






Use the checkboxes to select the types of cookies you want to accept, then press the “Save Settings” button. 
View our Privacy Policy.


Essential cookies
 enable core functionality of the site. These cannot be disabled.


Analytics cookies
 collect anonymous usage data to help us understand how visitors interact with the site and improve their experience.




Save Settings






















Hitachi Global Website






Terms of Use


Privacy Policy


Privacy Settings


Terms & Conditions of Sale




© 2017—2024 Hitachi Global Air Power US, LLC. All rights reserved. Information and specifications may change without notice.

















