Skip to main content
English

# Fluke 417D Laser Distance Meter

- bvseo_sdk, p_sdk, 3.2.1
- CLOUD, getAggregateRating, 23.22ms
- REVIEWS, PRODUCT
- bvseo-msg: HTTP status code of 404 was returned; HTTP status code of 404 was returned;

## Key features

- The Fluke 417D laser meter is accurate, durable, and easy to use—just point and shoot
- Instantly measure up to 40 m (131 ft.) with 1-button point-and-click
- Continuous measurement capable: adjusting as you move closer and farther from your target
- Quickly calculate area (sq feet/meters)
- 1-meter drop tested and IP54 rated: built to withstand rainy or dusty conditions
- Great for interior and exterior applications

Manuals + resources
Buy now

## Product overview: Fluke 417D Laser Distance Meter

The Fluke 417D is accurate, durable, and easy to use—just point and shoot. The simple design and easy, one-button measurement operation allows you to minimize time spent measuring and maximize the reliability of measurements.

Additional Product Features:

- Large, 2-line illuminated LCD screen.
- Three different measurement tasks can be completed quickly and easily with one hand.
- The bright laser is clearly visible, so you can always see your target point even from a hard-to-reach spot or long distance.
- Designed for both indoor and outdoor applications.
- Operates with the Fluke durability and quality you expect.
- Protected by a 3-year warranty.

## Specifications: Fluke 417D Laser Distance Meter

417D
Typical range [1] | 0.2-40 m/0.6-131 ft
Typical measuring tolerance* [1] | 2.0 mm ± 1.5 mm/± 0.06 in ***
Maximum measuring tolerance [2] | ± 3.0 mm/0.12 in ***
Accuracy up to 10m (+/-) | ± 2 mm
Display | 2 line/1 mm/1/32 in
Display illumination | Yes
Laser point at distance | 6/30/60 mm (10/40/100 m)
Area | Yes
Units setting (smallest units displayed) | 0,000m, 0' 00'' 1/32, 0 in 1/32
Auto laser switch off | 90 sec
Auto power switch off | 180 sec
General
Laser class | II
Laser type | 635 nm, <1 mW
Protection class | IP54
Battery life (2 x AAA) 1.5 V NEDA 24A/IEC LR03 | Up to 3,000 measurements
Size (Hx W x D) | 11.9 x 3.8 x 2.6 cm
Drop test | 1 meter
Weight (with batteries) | 95g (3.35 oz)
Temperature range: Storage | -25 °C to 70 °C (-13 °F to 158 °F)
Temperature range: Operation | -10 °C to 50 °C (14 °F to 122 °F)
Calibration cycle | Not applicable
Maximum relative humidity | 85 % @ 20°F to 120 °F (-7 °C to 50 °C)
Safety | CAN/CSA-C22.2 No. 61010-1-04, UL Std. No. 61010-1 (2nd Edition), ISA-82.02.01, IEC Standard No. 61010-1:2001, EN60825-1:2007 (Class II)
EMC | 61326-1:2006

[1] Applies for 100 % target reflectivity (white painted wall), low background illumination, 25 °C (13 °F).

[2] Applies for 10 % to 500 % target reflectivity, high background illumination, -10 °C to +50 °C (14 °F to +122 °F).

[3] Tolerances apply from 0.05 m to 10 m (0.001 ft to 32.8 ft) with a confidence level of 95 %. The maximum tolerance may deteriorate to 0.1 mm/m (0.003 in/ft) between 10 m to 30 m (32.8 ft to 98.4 ft) and to 0.15 mm/m (0.005 in/ft) for distances above 30 m (98.4 ft).

[4] Applies for 100 % target reflectivity, background illumination between 10,000 lux and 30,000 lux.

[5] After user calibration. Additional angle related deviation of ± 0.01° per degree up to ± 45° in each quadrant. Applies at room temperature. For the whole operating temperature range the maximum deviation increases by ± 0.1°.

## Models: Fluke 417D Laser Distance Meter

Fluke 417D

Fluke 417D Laser Distance Measurer (Meter)

Buy it

Includes:

- Two AAA batteries
- Users manual (17 languages)
- Quick reference guide
- Lanyard
- Three-year warranty

- bvseo_sdk, p_sdk, 3.2.1
- CLOUD, getContent, 22.05ms
- QUESTIONS, PRODUCT
- bvseo-msg: HTTP status code of 404 was returned;

- bvseo_sdk, p_sdk, 3.2.1
- CLOUD, getReviews, 21.97ms
- REVIEWS, PRODUCT
- bvseo-msg: HTTP status code of 404 was returned;

## Manuals + resources: Fluke 417D Laser Distance Meter

#### Manuals (3)

- 417D/424D | Users manual
- 417D/424D | Quick reference guide
- 417D/424D | Safety sheet

#### Data sheet (1)

- Fluke 417D Laser Distance Measurer Technical Data

#### Price (1)

- Price list

#### Register products

- Register product

## Related products

- ### 62 MAX Mini Infrared Thermometer

  Designed with your on-the-job needs in mind, the Fluke 62 MAX, 62 MAX+ Mini Infrared Thermometers are everything you'd expect from the experts in measurement tools. Small in size, extremely accurate and very easy to use.

  62 MAX Mini Infrared Thermometer is rated 3.5 out of 5 by 26.
  - bvseo_sdk, p_sdk, 3.2.1
  - CLOUD, getAggregateRating, 22.74ms
  - REVIEWS, PRODUCT

- ### Fluke 323 True RMS Clamp Meter

  Fluke 320 Series Clamp Meters for electrical troubleshooting

  Fluke 323 True RMS Clamp Meter is rated 4.3 out of 5 by 34.
  - bvseo_sdk, p_sdk, 3.2.1
  - CLOUD, getAggregateRating, 23.18ms
  - REVIEWS, PRODUCT

#### Tech support

service.uk@fluke.com

800-44-FLUKE (800-873-5853)

##### Repairs

service.uk@fluke.com

How to repair and replace Fluke products

##### Distributor questions

+44 (0)20 7942 0708