Visiting us from ?

# Dream Machine

Dream Machine
UDM
$299.00
All-in-one UniFi Gateway and access point designed to support LAN and WiFi networks.

Built-in WiFi 5 AP

Includes UniFi Network for device management

Full Gigabit routing

(4) GbE RJ45 LAN ports

Installation Guide
Technical Specifications

Mechanical
Dimensions | Ø110 x 184.1 mm (Ø4.3 x 7.3")
Weight | 1.1 kg (2.3 lb)
Enclosure material | Polycarbonate
Hardware
Processor | Quad-core Arm® Cortex® A57 at 1.7 GHz
System memory | 2 GB DDR RAM
Management interface | Ethernet Bluetooth
Networking interface | LAN: (4) GbE RJ45 ports WAN: (1) GbE RJ45 port
Power method | Universal AC input, 100—240V AC, 0.6A Max., 50/60 Hz
Power supply | AC/DC, internal, 50W
Supported voltage range | 100—240V AC
Max. power consumption | 26W
Max. TX power 2.4 GHz 5 GHz | 23 dBm 26 dBm
MIMO 2.4 GHz 5 GHz | 2 x 2 4 x 4
Throughput rate 2.4 GHz 5 GHz | 300 Mbps 1.7 Gbps
Antenna gain 2.4 GHz 5 GHz | 3 dBi 4.5 dBi
Antenna | (1) Internal, dual-band, quad-polarity antenna
Button | Factory reset
LEDs | White/blue
Ambient operating temperature | -10 to 45° C (14 to 113° F)
Ambient operating humidity | 5 to 95% Noncondensing
Certifications | CE, FCC, IC
Gateway Features
Performance | WiFi QoS with UniFi APs Application, domain, and country-based QoS Application and device type identification Additional internet failover with LTE Backup Internet quality and outage reporting
Next-generation security | Application-aware firewall rules Signature-based IPS/IDS threat detection Content, country, domain, and ad filtering VLAN/subnet-based traffic segmentation Full stateful firewall
Advanced networking | License-free SD-WAN WireGuard, L2TP and OpenVPN server OpenVPN client OpenVPN and IPsec site-to-site VPN One-click Teleport and Identity VPN Policy-based WAN and VPN routing DHCP relay Customizable DHCP server IGMP proxy IPv6 ISP support
Software
WiFi standards | 802.11a/b/g/n/ac
Wireless security | WEP, WPA-PSK, WPA-Enterprise (WPA/WPA2, TKIP/AES), 802.11w/PMF
BSSID | Up to 8 per radio
VLAN | 802.1Q
Advanced QoS | Per-user rate limiting
Guest traffic isolation | Supported
Concurrent clients | 100+
Supported Data Rates
802.11a | 6, 9, 12, 18, 24, 36, 48, 54 Mbps
802.11b | 1, 2, 5.5, 11 Mbps
802.11g | 6, 9, 12, 18, 24, 36, 48, 54 Mbps
802.11n (WiFi 4) | 6.5 Mbps to 300 Mbps (MCS0 - MCS15, HT 20/40)
802.11ac (WiFi 5) | 6.5 Mbps to 1.7 Gbps (MCS0 - MCS9 NSS1/2/3/4, VHT 20/40/80/160)