The leica disto d1 features Leica Lithium-ion battery and green beam laser technology. This laser is debris and water resistant with an IP65 rating and with an over-molded housing, it can withstand harsh conditions found on the worksite.

Full-time pulse mode allows use with detector, maintains full brightness for visibility, and extends range
Overmolded housing and IP65 debris/water resistance
Locking pendulum helps prevent damage to internal components

Applications:
- Framing
- Drywall
- Extended Ceiling Bracket
- Kitchen Installation
- Interior Finishing
- Layout
- Plumbing Walls
- Squaring Corners
- LEVELING Walls to Foundation
- Laying Steel track
- Railing install
- Laying Boards
- Digging Footings
- Retaining Wall
- Patio
- Tile Backsplash
- Fireplace
- Bathroom tile
- Digging Consistent Depths
- Laying Tile/Linoleum
- Cuts outs
- Level Countertops
- Cabinet Install
- Backsplash
- Drywall Cutouts
- Interior Can Lights
- Use as baseline
- Trim
- Crown Molding

Inc