CD-1002-3MUH

This electric series is lightweight and a perfect option for effectively washing wooden surfaces, driveways, sidewalks and siding.

Pump
Forged brass manifold · Thermal and safety relief valves · Built-in low pressure detergent injector

Motor
Totally enclosed fan-cooled electric motor with magnetic circuit breaker · 35-foot, 15-amp power cord with GFCI

Frame
Powder coated steel mounting plate with center balanced lift and four rubber isolators

Unit Includes
Variable high/low pressure nozzle · 25-foot x 3⁄8-inch non-marking hose · Two-piece, 36-inch lance with insulated trigger gun

Specifications

PSI

1000

GPM

2.0

Horsepower/Motor

1.5 HP, 120V, 1Ø, 13.2A

Pump

AR

Unloader

Adjustable Pressure

Plug Type

NEMA 5-15P

Weights & Dimensions

Net Weight

67.00 lbs.

Shipping Weight

78.00 lbs.

Length

22.00 in.

Width

11.50 in.

Height

14.50 in.

Options

CX-0030 High Pressure Hose - 50-Foot

For when you need extra hose for added mobility

Warranty Information

1 Year Electric Motor

7 Year AR Pump