Skip to main content
DCD771C2
20V MAX* Compact Drill/Driver Kit
DCD771C2

# 20V MAX* Compact Drill/Driver Kit

DCD771C2

# 20V MAX* Compact Drill/Driver Kit

- Compact, lightweight design fits into tight areas
- High performance motor delivers 300 unit watts out (UWO) of power ability completing a wide range of applications
- High speed transmission delivers two speeds (0-450 & 1,500 rpm) for a range of fastening and drilling applications

View more features

## Product Overview

Complete jobs in tight spots with the lightweight 20V MAX* Compact Drill/Driver. Featuring a high-performance motor and a 2-speed transmission, this drill delivers up to 300 UWO for a wide range of applications. For convenience this kit includes (2) 20V MAX* batteries, a charger, and a durable storage bag for portability.

## Additional Features

- 1/2" single sleeve ratcheting chuck provides tight bit gripping strength
- Ergonomic handle delivers comfort and control
- New 18V XR Li-Ion compact drill driver featuring XR 1.3Ah Li-Ion battery technology

## Includes

- (2) 20V MAX* Compact Li-ion battery packs
- (1) Compact charger
- (1) Contractor bag
- (1) DCD771 1/2" Drill driver

## Specifications

Battery Capacity | 1.3 Ah
Battery Chemistry | XR Li-ion
Chuck Capacity | 1.5-13 mm
Chuck size | 13 mm
Chuck size | 1/2 in
Clutch Positions | 16
Depth | 53 mm
Max. Drilling Capacity (Metal) | 13 mm
Max. Drilling Capacity (Wood) | 30 mm
No Load Speed (RPM) | 0-450-1500
Number of Pieces | 1
Power Output | 300 W
Product Height | 191 mm
Product Length | 219 mm
Product Weight | 2 Kg
Tool Weight | 3.6 lbs
Uncertainty K1 (Vibration) | 1.5 m/s2
Uncertainty K2 (Vibration) | 1.5 m/s2
Voltage | 20 V
Weight (Including Battery) | 4 lbs

## Support

### Warranty

- 3 Year Limited Warranty, 1 Year Free Service, 90 Days Satisfaction Guaranteed

We’re confident of the quality of our products, and we’ll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.

Learn More

### Service

We take extensive measures to ensure all our products are made to the very highest standards and meet all relevant industry regulations.

Learn More

### Support Manual

## Disclaimer(s)

- * Maximum initial battery voltage (measured without a workload) is 20 volts. Nominal voltage is 18.

DEWALT® Support

####

Hi there 👋Welcome to DeWalt! Stanley Black & Decker and its vendors use your communications here to provide technical support services and improve customer support. This chat uses an automated bot to respond. By continuing, you consent to the collection, use and sharing of the communications in this chat for the purposes mentioned above and as provided in our Privacy Policy.

I agree to the terms above and want to proceed

### Notice

You are now leaving our website and will be directed to an external website. Would you like to continue?

Continue Go Back