Motion activation variable speed and reversing control for precise fastening control
Motion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal
Adjustable two-position handle allows for operation in either in-line or pistol-grip
The MCF680N1 Automotive Ratcheting 13-in-1 Screwdriver 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional's needs.
Allows control when completing light fastening applications
LED provides illumination in confined areas without shadowing
Battery charge status on tool notifies when to charge packs
1/4" hex allows for quick screwdriver bit change and holds 1" bit tips
Automotive Ratcheting 13-in-1 Screwdriver battery pack allows for longer run-time and charges in one hour
#8x1 5/8" Drywall Screw into 2" x 4" SPF
#8 & #6 Machine screw insertion and removal
#6 & #8 Cabinet hardware screws
Electrical switch and outlet wall plate screws
Ideal tool fo