Contact Us

- Contact Us

Hitachi Global Air Power US, LLC
Skip to main content

# 375 Series T4F Portable Diesel Compressors

400HH

DESIGNED TO GET THE JOB DONE

Sullair 375 Series portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the 375 compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.

- Compact design
- Easy pressure change
- Extended runtime

Available with your choice of a reliable Caterpillar or Perkins engine!

Models vary by region. Please contact your Sullair sales representative for more details.

Jump To:

Specs Contact Us

### Flow

375 – 425 cfm
10.6 – 12 m³/min

### Pressure

150 – 200 psi
10.3 – 13.8 bar

### Power

122 – 157 hp
91 – 117 kW

##
Features & Benefits

- Multiple Engine Options
  - Caterpillar C4.4 (T4F)
  - Perkins 1204F (T4F)
- Compact Design
  - Easier towing to and from the job site
  - Improved maneuverability — fits more easily in smaller space
  - More convenient storage — on the job site or at the yard
- Easy Pressure Change
  - Select models shift from low to high pressure with the turn of a switch
- Quiet Operation
  - 74 decibels at 23 feet operating at full load
- Extended Runtime
  - Oversized 65 gallon tank
  - Up to 10 hours of runtime at full load
    - 5–7% improvement in fuel consumption at full load compared to previous models
- Easy Service and Maintenance
  - Swing doors with slam latches to ensure doors stay open
  - Easy access to key components including:
    - Cooler; aftercooler (if equipped)
    - Compressor fluid and air filters
    - Engine filters
    - Battery and battery disconnect
- Legendary Sullair 16-Series Air End
- Low Fuel Shutdown
- Discharge Temperature Sensor
- Electric Brakes
- LED Tail Lights
- LED Turn Lights
- Clearance Lights
- Sullair AWF® All Weather Fluid — Factory Fill Lubricant

##
Options

- Cold weather package
- Jack caster with wheels
- Mechanical parking brake
- Single or dual hose reels
- Aftercooled and filtered

##
Models & Specs

### Performance by Model

#### 375H

- Actual Delivery cfm (m³/min): 375 (10.6)
- Rated Pressure psig (bar): 150 (10.3)
- Pressure Range min/max (bar): 80 (5.5) / 175 (12.1)
- Fuel Consumption Full Load gal/h (l/h): 5.9 (22.3)
- Maximum Operating Altitude ft (m): 9000 (2743)
- Makes & Models: CAT C4.4 & Perkins 1204F (T4F)
- Operating Speed rpm: 2100
- Available Power bhp (kW): 122 (91)
- Displacement in³/l: 269 (4.4)
- Cooling System Capacity gal (l): 6.9 (26)
- Engine Oil Capacity qts (l): 8.5 (8)
- Fuel Tank Capacity gal (l): 65 (246)
- Electrical System Voltage: 12
- Battery Rating CCA: 1125
- DEF Consumption % of Fuel: 2.3%
- DEF Capacity gal (l): 5 (19)
- Service Valves No. & (Size): 2 (¾")
- Compressor Oil Capacity gal (l): 8 (30)

#### 400HH

- Actual Delivery cfm (m³/min): 400 (11.3)
- Rated Pressure psig (bar): 200 (13.8)
- Pressure Range min/max (bar): 80 (5.5) / 225 (15.5)
- Fuel Consumption Full Load gal/h (l/h): 7.4 (28)
- Maximum Operating Altitude ft (m): 9000 (2743)
- Makes & Models: CAT C4.4 & Perkins 1204F (T4F)
- Operating Speed rpm: 1900
- Available Power bhp (kW): 157 (117)
- Displacement in³/l: 269 (4.4)
- Cooling System Capacity gal (l): 6.9 (26)
- Engine Oil Capacity qts (l): 12 (11.5)
- Fuel Tank Capacity gal (l): 65 (246)
- Electrical System Voltage: 12
- Battery Rating CCA: 1125
- DEF Consumption % of Fuel: 2.3%
- DEF Capacity gal (l): 5 (19)
- Service Valves No. & (Size): 1 (1 ½ ")
- Compressor Oil Capacity gal (l): 8 (30)

#### 425H

- Actual Delivery cfm (m³/min): 425 (112)
- Rated Pressure psig (bar): 150 (10.3)
- Pressure Range min/max (bar): 80 (5.5) / 175 (12.1)
- Fuel Consumption Full Load gal/h (l/h): 7.7 (29.1)
- Maximum Operating Altitude ft (m): 9000 (2743)
- Makes & Models: CAT C4.4 & Perkins 1204F (T4F)
- Operating Speed rpm: 2100
- Available Power bhp (kW): 157 (117)
- Displacement in³/l: 269 (4.4)
- Cooling System Capacity gal (l): 6.9 (26)
- Engine Oil Capacity qts (l): ;12 (11.5)
- Fuel Tank Capacity gal (l): 65 (246)
- Electrical System Voltage: 12
- Battery Rating CCA: 1125
- DEF Consumption % of Fuel: 2.3%
- DEF Capacity gal (l): 5 (19)
- Service Valves No. & (Size): 2 (¾ ")
- Compressor Oil Capacity gal (l): 8 (30)

### Weights & Dimensions for 375H, 400HH, 425H

#### DPQ Package — Includes Running Gear

- Working weight lbs (kg): 4840 (2195)
- Dry weight lbs (kg): 4200 (1905)
- Length in (mm): 156 (3962)
- Width in (mm): 78 (1958)
- Height in (mm): 76 (1921)
- Track Width in (mm): 67 (1702)
- Max Towing Speed mph (km/h): 55 (89)
- Axle Rating lbs (kg): 5000 (2268)
- Tire Size: 225/75R15

#### DLQ Package — Less Running Gear

- Working weight lbs (kg): 4610 (2092)
- Dry weight lbs (kg): 3970 (1801)
- Length in (mm): 101 (2577)
- Width in (mm): 59 (1506)
- Height in (mm): 64 (1619)

*Non-aftercooled

### How to Buy

### Get More Info

### Download the Brochure

On
Off
Off
Off

## Related Products

### 185 Series T4F Portable Diesel Compressors

View Product

### Sullair Certified Glider Program for Towable Air Compressors

View Product

### AWF® Compressor Fluid

View Product

## Related Products 2

International 185 T3 Portable Diesel Compressors
View Product
SULLAIR RECON PROGRAM
View Product
Customer Fleet Management Parts Program (C.F.M)
View Product

## NEED HELP FINDING THE
RIGHT SOLUTION

INTERACTIVE GUIDE
This site uses essential cookies for core functionality and analytics cookies to collect anonymous usage data. Click “Accept Cookies” to accept all cookies or “Cookie Settings” to choose which types of cookies you wish to accept. View our Privacy Policy.
Accept Cookies Cookie Settings

Use the checkboxes to select the types of cookies you want to accept, then press the “Save Settings” button. View our Privacy Policy.

- Essential cookies enable core functionality of the site. These cannot be disabled.
- Analytics cookies collect anonymous usage data to help us understand how visitors interact with the site and improve their experience.

Save Settings
Hitachi Global Website
Terms of Use Privacy Policy Privacy Settings Terms & Conditions of Sale
© 2017—2024 Hitachi Global Air Power US, LLC. All rights reserved. Information and specifications may change without notice.