HUSQVARNA 125B
 
 
 
12.5 N
Blowing Force
9.4 lbs
Weight
Powerful, Lightweight Design*
Ergonomic Balanced Design
Quick Start with Air Purge
View all features
 
 
 
 
 
 
 
 
What's Included
HUSQVARNA 125B - 952 71 19‑25
Included
Nozzle type
Round+ Flat
Not Included
Harness
Vacuum Kit
125B
Comfort meets performance with the Husqvarna 125B. With unbeatable performance of 470 CFM at only 9.4 lbs*, this gas blower also features a state-of-the-art ergonomic design to minimize strain on your arms and wrists. And you'll enjoy easier starting with the auto return stop switch and air purge.
Features
Powerful, Lightweight Design*
470 CFM for maximum blowing performance at only 9.4 lbs
View more
Ergonomic Balanced Design
Balanced for less strain on your arms, shoulders and back
View more
Quick Start with Air Purge
Air purge removes air from carburetor and fuel system for easy starting
View more
Simple Starting
Stop switch automatically resets to ON so blower is ready for next use
View more
Adjustable Tube Length
Easily adjust the blowing tube length for maximum performance
View more
Multi-Speed Control
Variable speed throttle with cruise control option for easier handling
View more
Specifications
Compare specifications and features with similar Husqvarna products.
Compare
28cc, handheld blower
SKU: 952 71 19‑25
Equipment
28cc, handheld blower
SKU: 952 71 19‑25
Nozzle type
Round+ Flat
Harness
Not included
Vacuum Kit
No
Emission
Exhaust emissions (CO2 EU V)
1,392 g/kWh
Engine
Cylinder displacement
1.7 cu.inch
Power output
1.1 hp
Fuel tank volume
16.91 fl oz
Fuel consumption
575 g/kWh
Maximum power speed
8,000 rpm
Idling speed
3,000 rpm
Electrode gap
0.024 in
Engine Family CARB
Not Certified for CARB
Capacity
Air flow in housing
470 cfm
Air flow in pipe
425 cfm
Air speed (flat nozzle)
170 mph
Air speed (round nozzle)
130 mph
Blowing Force
12.5 N
Air speed
170 mph
Dimensions
Weight
9.4 lbs
Product size height
13.4 in
Product size length
14.9 in
Product size width
8.1 in
Tube diameter
2.559 in
Tube length
25.236 in
Sound and noise
Sound pressure level at operators ear
94 dB(A)
Sound power level, measured
109 dB(A)
Sound power level, guaranteed (LWA)
112 dB(A)
Vibration
Equivalent vibration level (ahv, eq) handle
11.1 m/s²