P750GM

Compliance with ATX 12V V2.52 & EPS 12 V2.92 standards
Conformal Coating Application
Global Safety Approved
High efficiency ≧ 92%
Powerful +12V single rail design
Quiet and durable cooling
Japanese electrolytic capacitors
Intelligent fan speed control circuit design
Full protections OCP,OVP, SCP,OPP,OTP, UVP
High Wattages with 80PLUS® Platinum Certification
Unique product ID with changeable side stickers for DIY enthusiasts and gamers

Conformal Coating Application
Off-Wet, Off-Dust and Off-Stain
The conformal coating which protects the power supply and its internal components from dust, humidity, stains. The P750GM series are covered with conformal coating to guarantee reliable performance in a harsh environment and tested to work perfectly even in 95% relative humidity.

LLC Full-Bridge Topology with DC-DC Module Design
P750GM Pro series features extremely tight voltage regulation to make the output voltage regulation under +/- 1% above 10% load change a