Open modal

# Redirect

Hello, we see you are visiting this site from North America. Click here to be redirected to Buffalo Americas.

# TeraStation™ 5810DN

High Performance, reliable storage. With built-in 10GBE Port, 3 USB 3.0 ports and 4 GB RAM.

Product Data Sheet

# TeraStation™ 5810DN

High Performance, reliable storage. With built-in 10GBE Port, 3 USB 3.0 ports and 4 GB RAM.

Buffalo’s TeraStation 5810DN is a high performance 8-bay network storage solution ideal for businesses and demanding users requiring a reliable RAID-based network storage solution for business critical applications. Increased speed and reliability is achieved with a 10GbE connection and hard drives built for always-on NAS devices. With the powerful Annapurna Labs® Alpine AL314 1.7Ghz Quad-Core processor, TeraStation 5810DN provides exceptional performance during file transfers and everyday NAS functions. The TS5810DN model is available in partially-populated units with 16 TB or 32 TB, and fully-populated units with 32TB and 64 TB. Partially populated models are ideal for users needing a small start with less initial investment. Populated with same size Buffalo OP-HD** only, for full support and warranty.

CPU Speed

1.7GHz

RAM

DDR3 ECC 4GB

Number of Bays

8

Supported RAID Levels

JBOD, 0, 1, 5, 6, 10

# High transmission speed

The 10GbE connectivity impresses with exceptional speed.

# VMware-ready

With this device you are supported by VMware if you have an ESX problem because this NAS device is VM-ready for NFS and iSCSI.

# Rsynch Feature

Users can make backup copies from TeraStation to a rsync-compatible device from another manufacturer. This function also allows backups to be made from another manufacturer’s rsync-compatible NAS to the TeraStation NAS.

# Active Directory

TeraStation functions as a client of an Active Directory domain, so that domain users and groups can be used. This means that they can be used in domain environments of companies with up to 10,000 users and groups.

# Including Buffalo VIP service

Replacement of defective hard disks within 24 hours

If you want to replace a defective hard disk, just let us know. If your order is in the system before 12 noon and the hard drives are in stock, they will be replaced within 24 hours. Applies within the 3 year warranty for each TeraStation and LinkStation NVR sold in the EU. (Outside the EU it can take longer).

More info

# 3 year warranty

This product has a standard warranty of 3 years. Check for other possibilities of warranty extension.

# Cloud-ready!

Buffalo’s TeraStation Series features B-Sync, which allows users to easily synchronize files between their TeraStation and 3rd party cloud services to make backups. The Buffalo NAS supports Amazon S3 Cloud Services, Dropbox, OneDrive and Azure.

# Intuitive web management interface

The web interface has a dashboard that offers the user more effective views of system status, the ability to resize windows (even on the phone) and a more comfortable button layout.

4 GB fast DDR3 ECC memory installed.

# iSCSI target support

Works simultaneously as NAS and iSCSI target.

# Replication with TeraStation

By replication, a folder in two separate TeraStations™ is synchronized almost in real time. This only happens in one direction (not bi-directional) – from the source to the destination. This function can be set up in LAN and WAN. WAN setup includes remote connection via port forwarding and VPN setup.

# Hot-swap function increases data security

With the hot swap function, the TeraStation™ automatically switches off the defective hard disk even if one hard disk fails, so that it can be replaced safely without interrupting work or losing data.

# With Annapurna Lab’s quad-core processor

Faster transfer of large files, faster file access from multiple computers.

# NovaStor Backup

Including 11 licenses NovaBACKUP® Buffalo Edition software. NovaBACKUP® provides small and medium-sized companies that value the protection of their digital data with a complete data security solution in one package.

# Allocation of disk quota

Hard disk quotas prevent the misuse of storage space by allocating appropriate amounts of storage to users.

#### TeraStation™ 51210RH

High performance, reliable storage. With built-in 10 Gigabit Ethernet Port, enterprise nearline HDD and 8GB RAM. Awarded several times!

more details

#### TeraStation™ 5410RN

High performance, reliable storage. With built-in 10Gigabit Ethernet Port.

more details

#### BS-MP2008 - 8 ports

Finally, a value Switch scalable to 10 GbE. 10Gigabit Layer2 Switches.

more details

Hardware System

Form factor
Desktop
CPU Type
Annapurna Labs Quad Core
CPU Speed
1.7GHz
RAM
DDR3 ECC 4GB
Drive Interface
SATA 6Gb/s
Installed OS
Linux

Internal Hard Drives

Number of Drives
8, 4
Type of Drive
NAS HDD
Number of Bays
8
Total Capacity
16TB, 32TB, 64TB
Supported HDD Capacities
4, 8TB

LAN Interface

Standard Compliance
(10BASE-T) IEEE802.3, (100BASE-TX) IEEE802.3u, (1000BASE-T) IEEE802.3ab, (10GBASE-T) IEEE802.3an, (NBASE-T) IEEE802.3bz
Connector Type
RJ-45
LAN Ports
1 x 10GbE, 2 x 1GbE
Max Transmission Rate
10/100/1000 Mbps / 2.5/5/10Gbps

USB Interface

Connector Type
Type A
USB 2.0 Ports
0
USB 3.0 Ports
3
Max Transmission Rate
480 Mbps / 5 Gbps

Other

Client OS
Windows 10 / 8.1 / 7; Windows Server 2016 / 2012 R2 / 2012 / 2008 R2 / 2008; Mac OS X 10.9 or later
Support
Standard Warranty 3 years, 24 hour HDD exchange, Technical Support Hotline
Power Consumption (max.)
150 W
Power Consumption (operation, typical)
108 W
Power Consumption (idle state, typical)
87 W
Power Consumption (standby)
4.5 W

Software System

Supported RAID Levels
JBOD, 0, 1, 5, 6, 10
Hot Swap
Yes
iSCSI
iSCSI Target

Protocol Support

Active Directory support
Yes
Active Directory users
10000

Backup

Failover
Failover solution with other Buffalo NAS devices
Realtime Backup
Folder Replication, Failover
Replication
Yes
Apple Time Machine®
Yes
Backup Software
NovaBACKUP Buffalo Edition
Cloud Support
Yes

Remote Access

WebAccess
Yes
FTP/SFTP
Yes

Product Part Numbers

Product Code
TS5810DN1604-EU - 16TB, TS5810DN3204-EU - 32TB, TS5810DN3208-EU - 32TB, TS5810DN6408-EU - 64TB
Note
1TB = 1, 000, 000, 000, 000 Bytes. Actual data throughput will vary depending upon environment factor.

# Downloads

Product Data Sheet Product images

Manuals / Setup / Latest Product Information
Documentation & Software |  |  |  | 24-04-2017
Firmware
Release notes | 4.68 | Windows | English | 28-09-2020
Release notes | 4.68 | Windows | Française | 28-09-2020
Release notes | 4.68 | Intel Mac | English | 28-09-2020
Release notes | 4.68 | Intel Mac | Française | 28-09-2020
Firmware updater | 4.68 | Intel Mac |  | 28-09-2020
Firmware updater | 4.68 | Windows |  | 28-09-2020
Utilities
B-Sync release notes | 1.02 | Windows | English | 11-11-2019
B-Sync release notes | 1.02 | Windows | Française | 11-11-2019
B-Sync | 1.02 | Windows |  | 11-11-2019
MIB files for SNMP software |  |  |  | 28-02-2018
Boot Authentication release notes | 1.00 | Windows |  | 16-11-2016
Boot Authentication Tool for TeraStation | 1.00 | Windows |  | 16-11-2016
NAS Navigator |  | Intel Mac 10.9 to 10.12 | Mac OS 10.13 or later, use the Mac App Store | --
NAS Navigator |  | Windows |  | --