Dream Machine - Ubiquiti Store United States
Visiting us from 
?
Continue to United States Store
Select Other Country / Region
Cloud Gateways
WiFi
Switching
Camera Security
Door Access
New Integrations
Accessory Tech
Identity
Support
Store
Dream Machine
Dream Machine
UDM
$299.00
All-in-one UniFi Gateway and access point designed to support LAN and WiFi networks.
 Built-in WiFi 5 AP


  Includes UniFi Network for device management


 Full Gigabit routing


 (4) GbE RJ45 LAN ports


Add to Cart
Installation Guide
Technical Specifications










Mechanical






Dimensions


Ø110 x 184.1 mm (Ø4.3 x 7.3")






Weight


1.1 kg (2.3 lb)






Enclosure material
Polycarbonate






Hardware






Processor


Quad-core Arm® Cortex® A57 at 1.7 GHz






System memory


2 GB DDR RAM






Management interface


Ethernet
Bluetooth






Networking interface


LAN: 
(4) GbE RJ45 ports
WAN: 
(1) GbE RJ45 port







Power method


 Universal AC input, 100—240V AC, 0.6A Max., 50/60 Hz






Power supply


AC/DC, internal, 50W






Supported voltage range


100—240V AC






Max. power consumption


26W






Max. TX power
2.4 GHz
5 GHz


23 dBm
26 dBm






MIMO
2.4 GHz
5 GHz
2 x 2
4 x 4






Throughput rate
2.4 GHz
5 GHz
300 Mbps
1.7 Gbps






Antenna gain
2.4 GHz
5 GHz


3 dBi
4.5 dBi






Antenna


(1) Internal, dual-band, quad-polarity antenna






Button


Factory reset






LEDs
White/blue






Ambient operating temperature


-10 to 45° C (14 to 113° F)






Ambient operating humidity


5 to 95% Noncondensing






Certifications


CE, FCC, IC






Gateway Features






Performance 

WiFi QoS with UniFi APs

Application, domain, and country-based QoS

Application and device type identification

Additional internet failover with LTE Backup

Internet quality and outage reporting






Next-generation security
Application-aware firewall rules

Signature-based IPS/IDS threat detection

Content, country, domain, and ad filtering

VLAN/subnet-based traffic segmentation

Full stateful firewall






Advanced networking
License-free SD-WAN
WireGuard, L2TP and OpenVPN server

OpenVPN client

OpenVPN and IPsec site-to-site VPN

One-click Teleport and Identity VPN

Policy-based WAN and VPN routing

DHCP relay

Customizable DHCP server

IGMP proxy

IPv6 ISP support







Software






WiFi standards


802.11a/b/g/n/ac






Wireless security


WEP, WPA-PSK, WPA-Enterprise (WPA/WPA2, TKIP/AES), 802.11w/PMF






BSSID


Up to 8 per radio






VLAN
802.1Q






Advanced QoS
Per-user rate limiting






Guest traffic isolation
Supported






Concurrent clients
100+






Supported Data Rates






802.11a
6, 9, 12, 18, 24, 36, 48, 54 Mbps






802.11b
1, 2, 5.5, 11 Mbps






802.11g
6, 9, 12, 18, 24, 36, 48, 54 Mbps






802.11n (WiFi 4)
6.5 Mbps to 300 Mbps (MCS0 - MCS15, HT 20/40)






802.11ac (WiFi 5)
6.5 Mbps to 1.7 Gbps (MCS0 - MCS9 NSS1/2/3/4, VHT 20/40/80/160)






 
Company
Careers
Contact Us
Investors
 
Training
Courses
Calendar
Trainers
Become a Trainer
 
Buy Now
Find a Distributor
Stock Locator Tool
Become a Distributor
 
Tools
WiFiman
UISP
UniFi Design Center
UISP Design Center
Stay in Touch
Subscribe
Terms and Conditions
|
Terms of Service
|
Privacy Policy
|
Return Policy
|
Cookies Settings
© 2024 Ubiquiti Inc. All rights reserved.