Dream Machine
Dream Machine
UDM
$299.00
All-in-one UniFi Gateway and access point designed to support LAN and WiFi networks.
 Built-in WiFi 5 AP

  Includes UniFi Network for device management

 Full Gigabit routing

 (4) GbE RJ45 LAN ports

Add to Cart
Installation Guide
Technical Specifications

Mechanical

Dimensions

Ø110 x 184.1 mm (Ø4.3 x 7.3")

Weight

1.1 kg (2.3 lb)

Enclosure material
Polycarbonate

Hardware

Processor

Quad-core Arm® Cortex® A57 at 1.7 GHz

System memory

2 GB DDR RAM

Management interface

Ethernet
Bluetooth

Networking interface

LAN: 
(4) GbE RJ45 ports
WAN: 
(1) GbE RJ45 port

Power method

 Universal AC input, 100—240V AC, 0.6A Max., 50/60 Hz

Power supply

AC/DC, internal, 50W

Supported voltage range

100—240V AC

Max. power consumption

26W

Max. TX power
2.4 GHz
5 GHz

23 dBm
26 dBm

MIMO
2.4 GHz
5 GHz
2 x 2
4 x 4

Throughput rate
2.4 GHz
5 GHz
300 Mbps
1.7 Gbps

Antenna gain
2.4 GHz
5 GHz

3 dBi
4.5 dBi

Antenna

(1) Internal, dual-band, quad-polarity antenna

Button

Factory reset

LEDs
White/blue

Ambient operating temperature

-10 to 45° C (14 to 113° F)

Ambient operating humidity

5 to 95% Noncondensing

Certifications

CE, FCC, IC

Gateway Features

Performance 

WiFi QoS with UniFi APs

Application, domain, and country-based QoS

Application and device type identification

Additional internet failover with LTE Backup

Internet quality and outage reporting

Next-generation security
Application-aware firewall rules

Signature-based IPS/IDS threat detection

Content, country, domain, and ad filtering

VLAN/subnet-based traffic segmentation

Full stateful firewall

Advanced networking
License-free SD-WAN
WireGuard, L2TP and OpenVPN server

OpenVPN client

OpenVPN and IPsec site-to-site VPN

One-click Teleport and Identity VPN

Policy-based WAN and VPN routing

DHCP relay

Customizable DHCP server

IGMP proxy

IPv6 ISP support

Software

WiFi standards

802.11a/b/g/n/ac

Wireless security

WEP, WPA-PSK, WPA-Enterprise (WPA/WPA2, TKIP/AES), 802.11w/PMF

BSSID

Up to 8 per radio

VLAN
802.1Q

Advanced QoS
Per-user rate limiting

Guest traffic isolation
Supported

Concurrent clients
100+

Supported Data Rates

802.11a
6, 9, 12, 18, 24, 36, 48, 54 Mbps

802.11b
1, 2, 5.5, 11 Mbps

802.11g
6, 9, 12, 18, 24, 36, 48, 54 Mbps

802.11n (WiFi 4)
6.5 Mbps to 300 Mbps (MCS0 - MCS15, HT 20/40)

802.11ac (WiFi 5)
6.5 Mbps to 1.7 Gbps (MCS0 - MCS9 NSS1/2/3/4, VHT 20/40/80/160)