Chicago Pneumatic homepage

Your browser is not supported

You are using a browser we do not support any longer. To continue visiting our website, please choose one of the following supported browsers.

Google Chrome

Mozilla Firefox

Safari

Microsoft Edge

Chicago Pneumatic homepage

Close

## Not quite sure about what you are looking for?

Use the links below to jump directly to the most searched topics

###### Most search keywords

#### Dealers locator

Find you closest dealer

#### More

Find your local contact

# CP3850 Series - Industrial angle grinders & sanders

The ultimate material removal tool. Ideal for grinding, sanding, cutting, contouring, deburring, finishing and weld cleaning.

Get in touch Download leaflet

#### A 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.

The CP3850 series grinders and sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.

Loading...

## Our CP3850 angle grinders and sanders feature:

#### A highly durable spiral bevel gear

that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.

#### A spindle lock feature

that allows for quick and easy abrasive replacement to reduce tool downtime.

#### A 360° adjustable air exhaust

with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).

#### A streamlined and ergonomic two-position safety trigger

that can be adapted to an operator’s grip above or below the housing.

#### An ergonomic handle

to promote a good operating position by maintaining the operator’s wrist straight.

#### A multi-position 360° anti-vibration side handle

for greater operator comfort. It can be positioned for left-hand or right-hand use.

## Feature highlight:

### A governed air motor of 2.8 hp / 2100 W

for constant air flow and abrasive wear. It delivers its maximum torque close to the free speed of the tool, prevents overspeed and reduces air consumption. The higher speed of the abrasive allows more material to be removed therefore increasing productivity. Read more

## Explore the CP3850 series:

## 7 angle grinders

High productivity with more comfort

Find your CP3850 angle grinders

Loading...

## 4 angle sanders

Find your CP3850 angle sanders

Loading...

## Air line accessories:

#### Filters, regulators, lubricators (FRL)

Why should you use a filter, regulator and lubricator ? The use of a filter, regulator and lubricator (in that order) for pretool air preparation is strongly recommended by Chicago Pneumatic.

#### Air fuses

## The CP3850 industrial grinders & sanders series is ideal for:

#### Metalworking

#### Foundries and casting plants

#### Oil, gas and petrochemical

#### Mining

#### Rolling stock

#### Shipyards

### Learn more from our experts