Compact, lightweight design fits into tight areas
High performance motor delivers 300 unit watts out (UWO) of power ability completing a wide range of applications
High speed transmission delivers two speeds (0-450 & 1,500 rpm) for a range of fastening and drilling applications
Complete jobs in tight spots with the lightweight 20V MAX* Compact Drill/Driver. Featuring a high-performance motor and a 2-speed transmission, this drill delivers up to 300 UWO for a wide range of applications. For convenience this kit includes (2) 20V MAX* batteries, a charger, and a durable storage bag for portability.
1/2" single sleeve ratcheting chuck provides tight bit gripping strength
Ergonomic handle delivers comfort and control
New 18V XR Li-Ion compact drill driver featuring XR 1.3Ah Li-Ion battery technology
Includes
(2) 20V MAX* Compact Li-ion battery packs
(1) Compact charger
(1) Contractor bag
(1) DCD771 1/2" Drill driver
Battery Capacity
1.3 Ah
Battery Chemistry
XR Li-ion
Chuck Capacity
1.5-13 mm
Chuck size
13 mm
Chuck size
1/2 in
Clutch Positions
16
Depth
53 mm
Max. Drilling Capacity (Metal)
13 mm
Max. Drilling Capacity (Wood)
30 mm
No Load Speed (RPM)
0-450-1500
Number of Pieces
1
Power Output
300 W
Product Height
191 mm
Product Length
219 mm
Product Weight
2 Kg
Tool Weight
3.6 lbs
Uncertainty K1 (Vibration)
1.5 m/s2
Uncertainty K2 (Vibration)
1.5 m/s2
Voltage
20 V
Weight (Including Battery)
4 lbs