































Cisco RV260 VPN Routers Data Sheet - Cisco














































































































Skip to content


Skip to search


Skip to footer














Cisco.com Worldwide


Products and Services


Solutions


Support


Learn


Explore Cisco


How to Buy


Partners Home


Partner Program


Support


Tools


Find a Cisco Partner


Meet our Partners


Become a Cisco Partner


















Products & Services
Routers
End-of-Sale and End-of-Life Products
Data Sheets








Cisco RV260 VPN Routers Data Sheet




































Save








Log in
 to Save Content
    








Download


Print












Available Languages












Download Options








PDF


(362.6 KB)




View with Adobe Reader on a variety of devices
















Updated:
October 24, 2018


Document ID:
1540240291900374










Bias-Free Language








Bias-Free Language


The documentation set for this product strives to use bias-free language. For the purposes of this documentation set, bias-free is defined as language that does not imply discrimination based on age, disability, gender, racial identity, ethnic identity, sexual orientation, socioeconomic status, and intersectionality. Exceptions may be present in the documentation due to language that is hardcoded in the user interfaces of the product software, language used based on RFP documentation, or language that is used by a referenced third-party product. 
Learn more
 about how Cisco is using Inclusive Language.




















 
 
 
 
 
The Cisco
®
 Small Business RV260, RV260P, and RV260W VPN routers are high-performance models combining business-class features with performance, security, reliability, and overall value at a great price point. These models are perfect for the small business, small enterprise, branch, or small home office network.
 
Product overview
 
Easy to configure and install, the RV260 routers can be remotely deployed using Plug and Play (PnP), are supported by the Cisco FindIT network platform, and feature a new user interface.
 
These models have a dual-core processor that provides performance usually found only in more expensive solutions. A Small Form-Factor Pluggable (SFP) WAN port provides flexible connectivity and investment protection. Like the other models in the portfolio, the RV260, 260P, and 260W include standard features such as a business-grade Stateful Packet Inspection (SPI) firewall, VPN security (IP Security [IPsec], Point-to-Point Tunneling Protocol [PPTP], and OpenVPN), content filtering, and device wizards to make an easy setup even easier.
 
The wired RV260 offers a high-performance user experience at an attractive cost point. The RV260P adds Power over Ethernet (PoE) to four of the eight ports. The RV260W adds 3x3 wireless 802.11ac. Like the RV160W but with better performance and more ports, this network-in-a-box offers fantastic wireless performance and range for the small business and teleworker network solution.
 
These models come with one year of web filtering service. This feature provides the ability to categorize different types of websites at different levels, and keeps your business users away from harmful websites.
 
Prominent feature/Differentiator/Capability
 
The Cisco Small Business RV260 VPN routers are high-performance models combining business-class features with performance, security, reliability, and overall value at a great price point. They are perfect for the small business, small enterprise, branch, or small home office network.
 
A new graphical user interface helps you get your VPN router up and running in minutes. Your business will enjoy reliable, highly secure connectivity that is so transparent you may not be aware of it.
 
Features and benefits
 
●
   
The RV260 provides wired connectivity with eight Gigabit Ethernet ports
 
●
   
The RV260P has eight Gigabit Ethernet ports with four ports of PoE and a 60W power budget
 
●
   
The RV260W is a wireless VPN router with 3x3 802.11ac Wave 2 wireless and a switch with eight Gigabit Ethernet ports 
 
●
   
Flexible SFP/RJ-45 combination WAN ports
 
●
   
High-performance Gigabit Ethernet ports, enabling large file transfers and multiple users 
 
 
●
   
Includes one year of web filtering to keep users and the business away from harmful websites and maintain a high level of productivity
 
●
   
IPsec, PPTP, and OpenVPN server enable secure connectivity for remote employees and multiple office sites
 
●
   
Strong security: Proven SPI firewall and hardware encryption
 
●
   
New user interface design for easier configuration and device management
 
●
   
Simple setup with wizard-based configuration 
 
 
●
   
Updated with a new hardware enclosure design
 
●
   
FindIT network management support
 
Product specifications
 
 
 
 
 
 
Description
 
 
 
Specification
 
 
 
 
 
 
 
Ethernet WAN 
 
 
 
1 RJ-45 SFP Gigabit combination port
 
 
 
 
 
Ethernet LAN
 
 
 
8 RJ-45 Gigabit Ethernet ports
 
RV260P has 4 PoE ports with a 60W power budget
 
 
 
 
 
Console port
 
 
 
1 RJ-45 port
 
 
 
 
 
Switch
 
 
 
Power on/off
 
 
 
 
 
Cabling type
 
 
 
Category 5 or better
 
 
 
 
 
LEDs
 
 
 
Power, VPN, WAN, LAN
 
 
 
 
 
Operating system
 
 
 
Linux
 
 
 
 
 
LAN
 
 
 
 
 
VLANs
 
 
 
16
 
 
 
 
 
Port security
 
 
 
Yes, 802.1X
 
 
 
 
 
IPv6
 
 
 
Dual stack, 6rd,6in4
 
 
 
 
 
WAN
 
 
 
Dynamic Host Configuration Protocol (DHCP) client, static IP, Point-to-Point Protocol over Ethernet (PPPoE), PPTP, Layer 2 Tunneling Protocol (L2TP)
 
 
 
 
 
WLAN
 
 
 
3x3 802.11ac Wave 2
 
 
 
 
 
Security
 
 
 
 
 
Firewall
 
 
 
SPI firewall
 
Port forwarding and triggering
 
Denial-of-Service prevention (DoS)
 
 
 
 
 
Access control
 
 
 
IP access control lists
 
 
 
 
 
Secure management
 
 
 
HTTPS, username/password complexity
 
 
 
 
 
User privileges
 
 
 
Two levels of access: Admin and guest
 
 
 
 
 
Network
 
 
 
 
 
Network protocols
 
 
 
 
●
  
Dynamic Host Configuration Protocol (DHCP) server      
 
 
●
  
Point-to-Point Protocol over Ethernet (PPPoE)      
 
 
●
  
Point-to-Point Tunneling Protocol (PPTP)      
 
 
◦
   
Layer 2 Tunneling Protocol (L2TP)       
 
 
●
  
DNS proxy      
 
 
●
  
DHCP relay agent      
 
 
●
  
Internet Group Management Protocol (IGMP) proxy and multicast forwarding      
 
 
●
  
Rapid Spanning Tree Protocol (RSTP)      
 
 
●
  
Dynamic DNS (DynDNS, No-IP, ChangeIP)      
 
 
●
  
Network Address Translation (NAT), Port Address Translation (PAT)      
 
 
●
  
One-to-one NAT      
 
 
●
  
Port management      
 
 
●
  
Port mirroring      
 
 
●
  
Software-configurable DMZ to any LAN IP address      
 
 
◦
   
Session Initiation Protocol (SIP) Application Layer Gateways (ALG)       
 
 
 
 
 
Routing protocols
 
 
 
 
●
  
Static routing, IGMP proxy      
 
 
●
  
Dynamic routing      
 
 
●
  
Routing Information Protocol (RIP) v1 and v2      
 
 
●
  
RIP for IPv6 (RIPng)      
 
 
◦
   
Inter-VLAN routing       
 
 
 
 
 
NAT protocol
 
 
 
Port Address Translation (PAT), Network Address Port Translation (NAPT) 
 
 
 
 
 
Port forwarding, One-to-one NAT, VPN NAT Traversal, Session Initiation Protocol (SIP), ALG, FTP ALG
 
 
 
 
 
VPN
 
 
 
 
 
Gateway-to-gateway IPsec VPN
 
 
 
20 IPsec tunnels
 
 
 
 
 
Client-to-gateway IPsec VPN
 
 
 
20 IPsec tunnels
 
 
 
 
 
IPsec VPN
 
 
 
Internet Key Exchange (IKE) v2, Generic Routing Encapsulation (GRE), hub and spoke supported
 
 
 
 
 
PPTP VPN
 
 
 
20 PPTP VPN tunnels
 
 
 
 
 
OpenVPN
 
 
 
Support for the OpenVPN server
 
 
 
 
 
Encryption
 
 
 
Triple Data Encryption Standard (3DES), Advanced Encryption Standard (AES) with 128, 192, and 256-bit keys encryption
 
 
 
 
 
VPN pass-through
 
 
 
IPsec, PPTP, and L2TP pass-through
 
 
 
 
 
Quality of Service (QoS)
 
 
 
 
 
QoS
 
 
 
 
●
  
802.1p port-based priority on LAN port, application-based priority on WAN port      
 
 
●
  
4 queues
 
 
 
 
●
  
Differentiated Services Code Point (DSCP) support
 
 
 
 
●
  
Class of Service (CoS)      
 
 
●
  
Bandwidth management for service prioritization      
 
 
 
 
 
Jumbo frame support
 
 
 
Supports jumbo frames on Gigabit ports – at least 1536B
 
 
 
 
 
Performance
 
 
 
 
 
NAT throughput
 
 
 
800+ Mbps
 
 
 
 
 
Concurrent sessions
 
 
 
25,000
 
 
 
 
 
IPsec VPN throughput
 
 
 
75+ Mbps
 
 
 
 
 
Configuration
 
 
 
 
 
Web-based user interface
 
 
 
Browser-based configuration (HTTP/HTTPS)
 
 
 
 
 
Management
 
 
 
Web-based user interface, Simple Network Management Protocol (SNMP) v3, Bonjour, PnP
 
Command-line interface via console – limited configuration command support
 
FindIT support for monitoring and management
 
 
 
 
 
Event logging
 
 
 
Local, syslog, email alerts
 
 
 
 
 
Network diagnostics
 
 
 
Ping, traceroute, DNS lookup
 
 
 
 
 
Upgradability
 
 
 
Firmware upgradable via browser UI, imported/exported file, USB, Cisco FindIT
 
 
 
 
 
System time
 
 
 
Network Time Protocol (NTP), Daylight Savings, manual entry
 
 
 
 
 
Language support
 
 
 
User interface support for English
 
 
 
 
 
Environmental
 
 
 
 
 
Power
 
 
 
RV260: 12VDC/2A
 
RV260P: 54VDC/1.67A
 
RV260W: 12VDC/2.5A
 
 
 
 
 
Operating temperature
 
 
 
0° to 40°C (32° to 104°F)
 
 
 
 
 
Storage temperature
 
 
 
-20° to 70°C (-4° to 158°F)
 
 
 
 
 
Operating humidity
 
 
 
10% to 85% noncondensing
 
 
 
 
 
Storage humidity
 
 
 
5% to 90% noncondensing
 
 
 
 
 
Certifications
 
 
 
Safety:
 
 
●
  
UL 60950-1      
 
 
●
  
CAN/CSA-C22.2 No. 60950-1      
 
 
●
  
IEC 60950-1      
 
 
●
  
EN 60950-1      
 
Radio approvals:
 
 
●
  
FCC Part 15.247, 15.407      
 
 
●
  
RSS-210 (Canada)      
 
 
●
  
EN 300.328, EN 301.893 (Europe)      
 
 
●
  
AS/NZS 4268.2003 (Australia and New Zealand)      
 
EMI and susceptibility:
 
 
●
  
FCC Part 15.107 and 15.109      
 
 
●
  
ICES-003 (Canada)      
 
 
●
  
EN 301.489-1 and -17 (Europe)      
 
 
◦
   
RV260/RV260P rackmount: Class A       
 
 
 
 
 
 
Ordering Information
 
 
 
 
 
 
Part number
 
 
 
Product description
 
 
 
 
 
 
 
RV260 and RV260P
 
 
 
 
 
RV260-K9-NA, RV260P-K9-NA
 
 
 
United States, Canada, Columbia, Mexico, Chile, Taiwan
 
 
 
 
 
RV260-K9-G5, RV260P-K9-G5
 
 
 
EU (CE Mark) 32 countries, Ukraine, Hong Kong, Singapore, Thailand, Vietnam, Philippines, Indonesia, Malaysia, Saudi Arabia, UAE, South Africa 
 
 
 
 
 
RV260-K9-AU, RV260P-K9-AU
 
 
 
Australia, New Zealand
 
 
 
 
 
RV260-K9-AR, RV260P-K9-AR
 
 
 
Argentina
 
 
 
 
 
RV260-K9-BR, RV260P-K9-BR
 
 
 
Brazil
 
 
 
 
 
RV260-K9-CN, RV260P-K9-CN
 
 
 
China
 
 
 
 
 
RV260-K9-IN, RV260P-K9-IN
 
 
 
India
 
 
 
 
 
RV260-K9-JP, RV260P-K9-JP
 
 
 
Japan
 
 
 
 
 
R260-K9-KR, R260P-K9-KR
 
 
 
Korea
 
 
 
 
 
RV260-K8-RU, RV260P-K8-RU
 
 
 
Russian Federation
 
 
 
 
 
RV260W
 
 
 
 
 
RV260W-A-K9-NA
 
 
 
United States, Canada, Columbia, Mexico
 
 
 
 
 
RV260W-E-K9-G5
 
 
 
EU (CE Mark) 32 countries, Hong Kong, Singapore, Thailand, Vietnam, Philippines
 
 
 
 
 
RV260W-A-K9-AU
 
 
 
Australia, New Zealand
 
 
 
 
 
RV260W-A-K9-AR
 
 
 
Argentina
 
 
 
 
 
RV260W-A-K9-BR
 
 
 
Brazil
 
 
 
 
 
RV260W-C-K9-CN
 
 
 
China
 
 
 
 
 
RV260W-I-K9-IN
 
 
 
India
 
 
 
 
 
RV260W-E-K9-JP
 
 
 
Japan
 
 
 
 
 
RV260W-R-K8-RU
 
 
 
Russian Federation
 
 
 
 
 
 
Dimensions
 
 
 
 
 
 
 
 
 
 
RV260
 
 
 
RV260W
 
 
 
RV260P
 
 
 
 
 
Device Dimension/Weight
 
 
 
Size L x W x H:
 279.4x170x38.5 mm
 
 
 
Size L x W x H:
 279x170x38.5 mm
 
 
 
Size L x W x H:
 279.4x170x38.5mm
 
 
 
 
 
 
 
 
 
Weight: 1230 g
 
 
 
Weight: 1360 g
 
 
 
Weight: 1260 g
 
 
 
 
 
Single Box Dimension/Weight
 
 
 
Size L x W x H: 376x266x127 mm
 
 
 
Size L x W x H: 388x271x126 mm
 
 
 
Size L x W x H: 261x453x106 mm
 
 
 
 
 
 
 
 
 
Weight: 2.33 kg
 
 
 
Weight: 2.18 kg
 
 
 
Weight: 2.72 kg
 
 
 
 
 
 
For more information 
 
For more information on the Cisco RV260, RV260P, and RV260W VPN routers, visit 
https://www.cisco.com/go/rv260
.
 
Warranty Information
 
Cisco limited lifetime warranty for Cisco products
 
This Cisco product comes with a limited lifetime hardware warranty. Product warranty terms and other information applicable to Cisco products are available at 
https://www.cisco.com/go/warranty
.
 
Cisco Support Service
 
Cisco Support Service offers an affordable, subscription-based support service that helps protect your investment and derive maximum value from Cisco products. Delivered and backed by Cisco, this comprehensive service includes software updates, extended access to the Cisco Support Center, and expedited hardware replacement, if required.
 
Cisco Capital
 
Flexible payment solutions to help you achieve your objectives
 
Cisco Capital
 
makes it easier to get the right technology to achieve your objectives, enable business transformation and help you stay competitive. We can help you reduce the total cost of ownership, conserve capital, and accelerate growth. In more than 100 countries, our flexible payment solutions can help you acquire hardware, software, services and complementary third-party equipment in easy, predictable payments. 
Learn more
.
 
For more information
 
For more information on the Cisco RV260, RV260P, and RV260W VPN routers, visit 
https://www.cisco.com/go/rv160
.
 
Firmware
 
To download firmware for the routers, visit Cisco Software Central.
 
 
 
 
 
 
 


































Contact Cisco
























Get a call from Sales








Call Sales:







                            
                            1-800-553-6387
                            
                        




US/CAN | 5am-5pm PT






Product / Technical Support










Training & Certification






























Was this Document Helpful?




Yes


No








Feedback















































