Fujitsu Storage ETERNUS AF250 S3

Entry-level all-flash storage for all Tier-1 applications in small and mid-sized companies

Max No. of controllers: 2

Max No. of drives: 264

Maximum storage capacity of up to 8,110 TB

Random access performance of up to 600,000 IOPS

Flexible and flash optimized storage

Selective use of deduplication / compression

Automated Quality-of-Service

Transparent failover and Storage Cluster

Ultra-low response times for all applications and a massive increase of IOPS without complicated tuning measures as well as scalable capacity and connectivity.

Data reduction at the volume level to improve storage efficiency and increase the lifespan of flash

Control applications priorities according to business needs, minimize admin efforts, automate monitoring and adjustment to guarantee service levels

High redundancies enable business critical computing, data processing and real-time data mirroring at the highest level and a system availability of up to 99.9999%.

Tech Specs

Type

All-Flash Array

Latency

140µsec (Read), 60µsec (Write)

Sequential access performance

11,000 MB/s (128KB Read) 5,300 MB/s (128KB Write)

Random access performance

600,000 IOPS (8KB Read) 480,000 IOPS (8KB Write)

Host Interfaces

Fibre Channel (16 Gbit/s, 32Gbit/s) iSCSI (10 Gbit/s [10GBase-SR, 10GBase-CR, 10GBase-T], 1 Gbit/s)

Maximum Disk Drives

264

Maximum Storage Capacity

8,110 TB

No. of host interfaces

4-16 ports [FC16Gbit/s)], 4/8 ports [FC(32Gbit/s), iSCSI(10Gbit/s,1Gbit/s)]

Max. no. of hosts

1,024

Supported RAID levels

0, 1, 1+0, 5, 5+0, 6

Drive interface

Serial Attached SCSI (12 Gbit/s)

Thin Provisioning

Yes

Automated Storage Tiering

Yes

Remote Copy functionality

Synchronous and asynchronous

Support Pack Options

Available in major metropolitan areas: 9x5, Next Business Day Onsite Response Time 9x5, 4h Onsite Response Time (depending on country) 24x7, 4h Onsite Response Time (depending on country)

Recommended Service

24x7, Onsite Response Time: 4h

Support Pack Options

Available in major metropolitan areas: 9x5, Next Business Day Onsite Response Time 9x5, 4h Onsite Response Time (depending on country) 24x7, 4h Onsite Response Time (depending on country)

Recommended Service

24x7, Onsite Response Time: 4h

Resources

Data Sheets

ETERNUS AF250 S3

ETERNUS AF150 S3

Brochures & Flyers

Brochure: ETERNUS AF - All-Flash Storage System

Flyer: Top Reasons to invest in ETERNUS AF

Infographic: ETERNUS All-Flash Storage

Brochure: ETERNUS Primary Storage Family

Fujitsu Storage Portfolio

White Papers

ETERNUS AF and ETERNUS DX Feature Set

ETERNUS AF and ETERNUS DX Optimization Features: Automated Storage Tiering and Automated Quality of Service

ETERNUS AF and ETERNUS DX Storage Cluster

Software

FUJITSU ETERNUS SF V16.9 Storage Management Software

ETERNUS SF storage management software supports overall daily operations within the entire ETERNUS AF and ETERNUS DX storage infrastructure by offering an easy-to-use graphical user interface for all management tasks, like health monitoring, capacity management, provisioning, local and remote replication and disaster recovery as well as the management of unified storage. At the same time it reduces significantly administrator’s training efforts with regards to cost and time.

Fujitsu Storage ETERNUS Multipath Driver (only available for APAC region)

ETERNUS Multipath Driver software achieves high-reliability and performance systems due to multipath connection between storages and servers. In case of path failure ETERNUS Mutpath Driver switches the access path to improves system reliability. In addition, further improved system performance is ensured by the load balancing function between multiple paths.