Skip to main content
DW089LG
12V MAX* 3 x 360 Green Line Laser
DW089LG

# 12V MAX* 3 x 360 Green Line Laser

DW089LG

# 12V MAX* 3 x 360 Green Line Laser

- 12V MAX* lithium-ion rechargeable power tool battery platform
- Green beam laser technology
- Integrated magnetic bracket with 1/4" and 5/8" thread

View more features

## Product Overview

The 12V MAX* Green 3x360 Laser features 12V MAX* Lithium-ion battery and green beam laser technology. This laser is debris and water resistant with an IP65 rating and with an over-molded housing, it can withstand harsh conditions found on the worksite.

## Additional Features

- Full-time pulse mode allows use with detector, maintains full brightness for visibility, and extends range
- Overmolded housing and IP65 debris/water resistance
- Locking pendulum helps prevent damage to internal components

## Applications

- Framing
- Drywall
- Extended Ceiling Bracket
- Kitchen Installation
- Interior Finishing
- Layout
- Plumbing Walls
- Squaring Corners
- LEVELING Walls to Foundation
- Laying Steel track
- Railing install
- Laying Boards
- Digging Footings
- Retaining Wall
- Patio
- Tile Backsplash
- Fireplace
- Bathroom tile
- Digging Consistent Depths
- Laying Tile/Linoleum
- Cuts outs
- Level Countertops
- Cabinet Install
- Backsplash
- Drywall Cutouts
- Interior Can Lights
- Use as baseline
- Trim
- Crown Molding

## Includes

- (1) Durable Carrying Case
- (1) Extended Ceiling Bracket
- (1) Battery
- (1) Charger
- (1) 12V MAX* Green 3 x 360 Line Laser
- (1) Target Card

## Specifications

Laser Accuracy | +/-3mm@10m
Battery Chemistry | Rechargeable Lithium Ion
IP Rating | IP65
Laser Beam Color | Green Beam
Voltage | 12 V

## Support

### 3 Year Limited Warranty, 1 Year Free Service, 90 Days Satisfaction Guaranteed

We’re confident of the quality of our products, and we’ll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.

Learn More

### Service

We take extensive measures to ensure all our products are made to the very highest standards and meet all relevant industry regulations.

Learn More

### Support Manual

## Disclaimer(s)

- * Maximum initial battery voltage (measured without a workload) is 12 volts. Nominal voltage is 10.8.

DEWALT® Support

####

Hi there 👋Welcome to DeWalt! Stanley Black & Decker and its vendors use your communications here to provide technical support services and improve customer support. This chat uses an automated bot to respond. By continuing, you consent to the collection, use and sharing of the communications in this chat for the purposes mentioned above and as provided in our Privacy Policy.

I agree to the terms above and want to proceed

### Notice

You are now leaving our website and will be directed to an external website. Would you like to continue?

Continue Go Back