Straight Power 11 750W

Compliance with ATX 12V V2.52 & EPS 12 V2.92 standards
Conformal Coating Application
Global Safety Approved
High efficiency ≧ 92%
Powerful +12V single rail design
Quiet and durable cooling
Japanese electrolytic capacitors
Intelligent fan speed control circuit design
Full protections OCP,OVP, SCP,OPP,OTP, UVP
High Wattages with 80PLUS® Platinum Certification
Unique product ID with changeable side stickers for DIY enthusiasts and gamers

Conformal Coating Application
Off-Wet, Off-Dust and Off-Stain
The conformal coating which protects the power supply and its internal components from dust, humidity, stains. The Straight Power 11 series are covered with conformal coating to guarantee reliable performance in a harsh environment and tested to work perfectly even in 95% relative humidity.

LLC Full-Bridge Topology with DC-DC Module Design
Straight Power 11 Pro series features extremely tight voltage regulation to make the output voltage regulation under +/- 1% above 10% load change a