Skip to content

| Catalogs | Support

Search for:

Catalog

Support

CATALOGS | SUPPORT |

SmartLine Controllers Marcie 2023-08-07T08:16:38-05:00

# SmartLine Controllers

## SL1600, SL1620, SL4800

Smart Controller with Automatic ET Adjustments, Upgrade to Web-Based Remote Access, Pre-Installed Line Cord (Plug-N-Play), SmartLink Network Ready

Models & Product Specifications
Downloads
Training Videos

# SmartLine Controllers

## SL1600, SL1620, SL4800

Smart Controller with Automatic ET Adjustments, Upgrade to Web-Based Remote Access, Pre-Installed Line Cord (Plug-N-Play), SmartLink Network Ready

Compare SmartLink Models
Manuals & Installation
Models & Product Specifications

### BASIC FEATURES

- 4 independent programs – each stacks or can operate simultaneously
- 8 start times per program
- Indoor/outdoor rated
- Zone run times settable from 1 min. to 9 hrs. 55 min.
- Rain/freeze sensing on/off button with tri-color LED indicator
- Rain delay of 1 – 7 days
- SLW5/SLW1 Weather Station rain delay programmable from 0 – 99 hours
- Seasonal % adjust by program, by month
- Omit time of day window, day(s) of week, and up to 7 calendar dates
- Programmable zone-to-zone delay 1 min. – 3 hrs.
- Watering days: custom days of the week, odd/even, or interval days
- Run/Soak cycles by program
- Large backlit LCD display
- Non-volatile memory – with no battery required
- Internal transformer with pre-installed 6’ line cord (SL1600, SL1620 only)
- 2 simultaneous watering modes: basic mode and smart mode. Each zone can run in either mode independent of other zones, even in the same program.
- Basic mode: user controlled conventional operation
- Smart mode: daily automatic programming adjustments
- 5 user-selectable languages
- Simultaneous solenoid operation: 3 solenoids (SL800/SL1600), 5 solenoids (SL4800)

### SMART WATERING FEATURES

- ZIP Code input or latitude input
- Sprinkler type input
- Plant type input
- Soil type input
- More/less ET tuning
- Watering run times
- Review menu displays accumulated ET deficits by zone
- Display maximum run time and minimum soak time
- Displays temperature readings (daily high/low) for previous 5 days
- Accumulates total run times by zone from the last reset date
- Clear deficits for all zones
- Extended rain delay programmable from 0 – 99 hours

### Downloads

#### Sales Sheets & Brochures

#### Manuals & Installation Instructions

#### Design Specifications

### ADDITIONAL FEATURES

- Zone-to-zone delay
- Master valve timing sequence with zone valve programmable
- Master valve/pump start operation assignable On/Off by zone
- Clear program function
- Clear all function
- Grow-in program
- Two independently programmed master valves
- Normally open or normally closed master valve operation
- Real time milliamp display
- Flow sensor data review (requires SmartLink® Aircard)
- Real time flow display (requires SmartLink® Aircard)

### MANUAL OPERATION

- Manual test runs each zone with zone run times from 10 sec. – 10 min.
- Manual zone operation of a single zone (1 min. to 9 hrs. 55 min.)
- Push button manual start of a program from control pane

### ON-SITE DIAGNOSTIC/TROUBLESHOOTING FEATURES

- Fault review displays all faults, including open and shorted zones
- Test function using on-board multi-meter
- Built-in valve locator
- Backtrack Stored Program™

Save Water. Give Life.

1,000 gallons given per controller

### MODELS & PRODUCT SPECIFICATIONS

## SL1600

Dimensions
9 1⁄8” W x 10 1⁄2” H x 4” D
(23.2 cm x 25.7 cm x 10.2 cm)

Electrical
Input: 120 VAC/60Hz
Output: 24 VAC/1.6 Amps
Fuse: 1.0A slow blow

Base # of Zones
4

Maximum # of Zones
16

Compatible Expansion Modules
SLM4
SLM12-1600

## SL1620

Dimensions
9 1⁄8” W x 10 1⁄2” H x 4” D
(23.2 cm x 25.7 cm x 10.2 cm)

Electrical
Input: 120 VAC/60Hz
Output: 24 VAC/1.6 Amps
Fuse: 1.0A slow blow

Base # of Zones
20

Maximum # of Zones
20

Compatible Expansion Modules
N/A

## SL4800

Dimensions
15” W x 16 ½” H x 5 7⁄16” D
(38.1 cm x 41.9 cm x 13.8 cm)

Electrical
Input: 120 VAC/60Hz
Output: 24 VAC/2 Amps
Fuse: 1.5A slow blow

Base # of Zones
12

Maximum # of Zones
48

Compatible Expansion Modules
SLM12-4800

### TRAINING VIDEOS

«
Prev
1
/
1
Next
»
SmartLine Controller Basic Programming
SmartLine Controller Smart Programming
«
Prev
1
/
1
Next
»
RETURN TO CONTROLLERS
Page load link
Go to Top