The SS5L5 Single Stage Air Compressor offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.

A 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.

Our SS5L5 Single Stage Air Compressor feature:
A highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.
A spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.
A 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).
A streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.
An ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig