/ 4 Download

Archer C7 V5

- Archer C7 V4
- Archer C7 V5

# AC1750 Wireless Dual Band Gigabit Router

- Supports 802.11ac standard - Faster than wireless N speeds*
- Simultaneous 2.4GHz 450 Mbps and 5GHz 1300 Mbps connections for 1.75Gbps of total available bandwidth*
- USB Port - easily shares files & media with networked devices or remotely via FTP server
- Guest Network Access - provides secure Wi-Fi access for guests sharing your home or office network
- Easy setup and management with Tether App

BUY NOW

- AC1750 Wireless Dual Band Gigabit Router - Archer C7

- Why 802.11ac

## Overview

The New York Times

## “The Best Router
for Most People”

AC1750 Wireless Dual Band Gigabit Router

Archer C7

*A review of dozens of wireless routers by the New York Times in collaboration with The Wirecutter concluded that the Archer C7 is the best option for most consumers.

## The New WiFi Standard for an Advanced Online Experience

The Archer C7 is a fast 802.11ac router with incredible range. It's better than many routers that are twice as expensive. This advanced WiFi is designed for high-traffic online activities and can help to run applications at triple the speed of the previous 802.11n standard.*

- 1300Mbps
- 450Mbps

## Concurrent Dual Band Connections for Lag-Free Work and Entertainment

The Archer C7 operates both the 2.4GHz and 5GHz bands, ensuring amazing wireless performance. Simple tasks like sending e-mails or web browsing can be handled by the 2.4GHz band while bandwidth intensive tasks like online gaming or HD video streaming can be processed by the 5GHz band – all at the same time.

## External Antennas with Dual Band WiFi Greatly Expand Wireless Coverage

Three external antennas with advanced connection technology allow you to maintain impressive speeds. With antennas serving both the 2.4GHz and 5GHz band, you can enjoy incredible wireless coverage and reliability in any part of your large home or office.

- 5GHz
    The crystal clean 5GHz band is ideal for HD streaming and gaming, creating a blazing-fast network.
- 2.4GHz
    The 2.4GHz band provide stable and strong WiFi signal for everyday tasks, like browsing and surfing.

## Versatile USB Connectivity

A USB 2.0 port makes the Archer C7 a truly resourceful gateway. Share a hard drive full of media through your home network, or via an ftp server whenever you’re away.

- FTP Server
- Media Server
- Storage Sharing

## Full Gigabit Wired Connections for Ultrafast Data Transfer Speeds

With one Gigabit WAN port and four Gigabit LAN ports, speeds can be up to 10× faster than standard Ethernet connections.
The Archer C7 is a powerful hub to support a robust and extremely fast wired network.

- Power
- Power On/Off
- Reset
- Gigabit WAN Port
- 4 Gigabit LAN Ports
- WPS/WiFi

## TP-Link OneMesh™ :
Flexibly Create a Whole-Home WiFi

OneMesh™ is a simple way to form a Mesh network with a single WiFi name for seamless whole-home coverage. Just connect a OneMeshTM range extender to a OneMesh™ router. No more searching around for a stable connection.**

Learn More about OneMesh™ >>

- ### WiFi Dead-Zone Killer

  Eliminate weak signal areas with WiFi coverage for the whole house

- ### Smart Roaming

  Uninterrupted streaming when moving around your home

- ### One WiFi Name

  No more switching WiFi network names

- ### Unified Management

  Manage the whole-home WiFi by managing the central node via Tether app/Web UI

- ### Traditional Router with Extender

- ### OneMesh™ Router + Range Extender

## Enjoy a Mesh Network with Your Existing Router

Want a Mesh network? Hesitate on whether to replace your existing router and buy a Mesh set?
TP-Link OneMesh™ resolves your dilemma.

Check whether your existing router supports OneMesh >>

- Parental Controls
    Manage when and how connected devices can access the internet
- IPv6 Supported
    Supports IPv6, the next generation of Internet protocol, helping you to future-proof your network.
- Quality of Service
    Prioritizes devices or applications to give faster performance where you need it.

## Specifications

WIRELESS
Standards | Wi-Fi 5IEEE 802.11ac/n/a 5 GHzIEEE 802.11n/b/g 2.4 GHz
WiFi Speeds | AC17505 GHz: 1300 Mbps (802.11ac)2.4 GHz: 450 Mbps (802.11n)
WiFi Range | 3 Bedroom Houses 3× Fixed High-Performance AntennasMultiple antennas form a signal-boosting array to cover more directions and large areas
WiFi Capacity | Medium Dual-BandAllocate devices to different bands for optimal performance
Working Modes | Router ModeAccess Point Mode

SECURITY
Network Security | SPI FirewallAccess ControlIP & MAC BindingApplication Layer Gateway
Guest Network | 1× 5 GHz Guest Network1× 2.4 GHz Guest Network
VPN Server | OpenVPNPPTP
WiFi Encryption | WPAWPA2WPA/WPA2-Enterprise (802.1x)

HARDWARE
Processor | Qualcomm CPU
Ethernet Ports | 1× Gigabit WAN Port4× Gigabit LAN Ports
USB Support | 1× USB 2.0 PortSupported Partition Formats:NTFS, FAT32Supported Functions:FTP ServerMedia ServerSamba Server
Buttons | Wi-Fi On/Off ButtonPower On/Off ButtonWPS/Reset Button
Power | 12 V ⎓ 1.5 A

SOFTWARE
Protocols | IPv4IPv6
OneMesh™ | OneMesh™ SupportedWithout replacing your existing devices or buying a whole new WiFi ecosystem, OneMesh™ helps you create a more flexible network that covers your entire home with TP-Link OneMesh™ products. Learn More>All OneMesh Products>
Parental Controls | URL FilteringTime Controls
WAN Types | Dynamic IPStatic IPPPPoEPPTPL2TP
Quality of Service | QoS by Device
Cloud Service | OTA Firmware UpgradeTP-Link IDDDNS
NAT Forwarding | Port ForwardingPort TriggeringDMZUPnP
IPTV | IGMP ProxyIGMP SnoopingBridgeTag VLAN
DHCP | Address ReservationDHCP Client ListServer
DDNS | TP-LinkNO-IPDynDNS
Management | Tether AppWebpageCheck Web Emulator>

OTHER
System Requirements | Internet Explorer 11+, Firefox 12.0+, Chrome 20.0+, Safari 4.0+, or other JavaScript-enabled browserCable or DSL Modem (if needed)Subscription with an internet service provider (for internet access)
Certifications | FCC, CE, RoHS
Environment | Operating Temperature: 0℃~40℃ (32℉ ~104℉)Storage Temperature: -40℃~70℃ (-40℉ ~158℉)Operating Humidity: 10%~90% non-condensingStorage Humidity: 5%~90% non-condensing

TEST DATA
WiFi Transmission Power | CE:<20dBm(2.4GHz)<23dBm(5GHz)FCC:<30dBm
WiFi Reception Sensitivity | 5GHz:11a 6Mbps-96dBm11a 54Mbps: -79dBm11ac HT20: -71dBm11ac HT40: -66dBm11ac HT80: -63dBm2.4GHz:11g 54M: -77dBm11n HT20: -74dBm11n HT40: -72dBm

PHYSICAL
Dimensions (W×D×H) | 9.6 × 6.4 × 1.3 in(243 × 160.6 × 32.5 mm)
Package Contents | Wi-Fi Router Archer C7Power AdapterRJ45 Ethernet CableQuick Installation Guide

For additional version information, please go to the support page.

## Support

*Maximum wireless transmission rates are the physical rates derived from IEEE Standard 802.11 specifications. Range and coverage specifications along with the number of connected devices were defined according to test results under normal usage conditions. Actual wireless transmission rate, wireless coverage, and number of connected devices are not guaranteed, and will vary as a result of 1) environmental factors, including building materials, physical objects and obstacles, 2) network conditions, including local interference, volume and density of traffic, product location, network complexity, and network overhead and 3) client limitations, including rated performance, location, connection quality, and client condition.

**Seamless roaming/No-Drop Wi-Fi refers to the Wi-Fi roaming that supports IEEE 802.11 k/v/r protocol, helping connected devices search and shift from one AP to another within 0.3 second. Clients need to support 802.11 k/v/r and may require additional setup. Performance may vary depending on the client device.

Actual network speed may be limited by the rate of the product's Ethernet WAN or LAN port, the rate supported by the network cable, Internet service provider factors and other environmental conditions.

We have updated our Policies. Read Privacy Policy and Terms of Use here.
This website uses cookies to improve website navigation, analyze online activities and have the best possible user experience on our website. You can object to the use of cookies at any time. You can find more information in our privacy policy .

We have updated our Policies. Read Privacy Policy and Terms of Use here.
This website uses cookies to improve website navigation, analyze online activities and have the best possible user experience on our website. You can object to the use of cookies at any time. You can find more information in our privacy policy .

Basic Cookies

These cookies are necessary for the website to function and cannot be deactivated in your systems.

TP-Link

accepted_local_switcher, tp_privacy_base, tp_privacy_marketing, tp_smb-select-product_scence, tp_smb-select-product_scenceSimple, tp_smb-select-product_userChoice, tp_smb-select-product_userChoiceSimple, tp_smb-select-product_userInfo, tp_smb-select-product_userInfoSimple, tp_top-banner, tp_popup-bottom, tp_popup-center, tp_popup-right-middle, tp_popup-right-bottom, tp_productCategoryType

Livechat

__livechat, __lc2_cid, __lc2_cst, __lc_cid, __lc_cst, CASID

Youtube

id, VISITOR_INFO1_LIVE, LOGIN_INFO, SIDCC, SAPISID, APISID, SSID, SID, YSC, __Secure-1PSID, __Secure-1PAPISID, __Secure-1PSIDCC, __Secure-3PSID, __Secure-3PAPISID, __Secure-3PSIDCC, 1P_JAR, AEC, NID, OTZ

Analysis and Marketing Cookies

Analysis cookies enable us to analyze your activities on our website in order to improve and adapt the functionality of our website.

The marketing cookies can be set through our website by our advertising partners in order to create a profile of your interests and to show you relevant advertisements on other websites.

Google Analytics & Google Tag Manager

_gid, _ga_<container-id>, _ga, _gat_gtag_<container-id>

Google Ads & DoubleClick

test_cookie, _gcl_au

Facebook

_fbp

Crazy Egg

cebsp_, _ce.s, _ce.clock_data, _ce.clock_event, cebs

Hotjar

OptanonConsent, _sctr, _cs_s, _hjFirstSeen, _hjAbsoluteSessionInProgress, _hjSessionUser_14, _fbp, ajs_anonymous_id, _hjSessionUser_<hotjar-id>, _uetsid, _schn, _uetvid, NEXT_LOCALE, _hjSession_14, _hjid, _cs_c, _scid, _hjAbsoluteSessionInProgress, _cs_id, _gcl_au, _ga, _gid, _hjIncludedInPageviewSample, _hjSession_<hotjar-id>, _hjIncludedInSessionSample_<hotjar-id>

Linkedin

lidc, AnalyticsSyncHistory, UserMatchHistory, bcookie, li_sugr, ln_or