 
 
 
Laser Measuring Tool | Fluke 417D Laser Distance Meter | 131 ft. | Fluke
 
 
Skip to main content
 
 
English
 
 
 
 
 
 
 
 
 
 
 
 
 
Fluke
 
 
Other Fluke companies 
 
See more Fluke brands
 
Accelix
 
Amprobe
 
Beha-Amprobe
 
Comark
 
Emaint CMMS
 
Irisys
 
Landauer
 
Pacific Laser Systems
 
Pomona
 
Pruftechnik
 
RaySafe
 
 
Products
 
Featured
 
Award winning
 
New Fluke products
 
Test Tools Catalog
 
Fluke software
 
Accessories
 
Cases and holsters
 
Test leads, probes and clips
 
Building infrastructure
 
HVAC tools
 
Indoor air quality testing
 
Laser distance meters
 
Laser levels
 
Electrical tools
 
Digital multimeters
 
Basic electrical testers
 
Clamp meters
 
Power quality
 
Earth ground
 
Installation testers
 
Insulated tools
 
Intrinsically safe
 
Battery analyzers
 
Insulation testers
 
Portable oscilloscopes
 
Portable appliance testers
 
Solar industry tools
 
eMobility
 
Acoustic and thermal imaging
 
Thermal imaging cameras
 
Acoustic imaging and borescopes
 
IR windows
 
Temperature measurement
 
Contact thermometers
 
IR thermometers
 
Network cable testers
 
Industrial Ethernet testers
 
Alignment tools
 
Laser alignment
 
Vibration analysis
 
Calibration tools
 
mA loop calibrators
 
Multifunction calibrators
 
Pressure calibrators
 
Temperature calibrators
 
Condition monitoring
 
eMaint CMMS
 
Fluke Connect
 
Connect2Assets
 
Fluke Mobile
 
Connected reliability
 
Power monitoring
 
Vibration
 
Learn
 
Fluke Resource Center
 
Fundamentals
 
Calibration
 
Energy management
 
Maintenance and monitoring
 
Safety
 
Troubleshooting
 
All topics
 
Fluke education partnership program
 
Online courses
 
Digital multimeter basics
 
Electrical measurement safety
 
Insulation Resistance
 
Motor and drive troubleshooting
 
Seminars and training
 
Tradeshows
 
Tools and calculators
 
Air leakage calculator
 
FOV calculator
 
LeakQ report generator
 
PDQ Mode Reporting Tool
 
Webinars
 
Support
 
Customer service
 
Contact us
 
Technical support
 
Calibration services
 
Repair
 
Service center locations
 
Return materials authorization
 
Product resources
 
Fluke Manuals
 
Product registration
 
Recycle program
 
Safety notices
 
Service quote request
 
Download software updates
 
Warranties
 
Talk to a Fluke sales expert
We’ll help you select the right product for your needs.
Quick support
Repairs 
Technical support 
 
What is your favorite color? 
 
 
First Name 
*
 
 
Last Name 
*
 
 
Email Address 
*
 
 
Company 
*
 
 
Phone 
*
 
 
Country 
*
 
- Select -
United States (Estados Unidos)
Canada
Afghanistan
Albania
Algeria
American Samoa
Andorra
Angola
Anguilla
Antartica
Antigua and Barbuda
Argentina
Armenia
Aruba
Australia
Azerbaijan
Bahamas
Bahrain
Bangladesh
Barbados
Беларусь (Belarus)
Belgien/Belgique (Belgium)
Belize
Benin
Bermuda
Bhutan
Bolivia
Bonaire
Bosnia and Herzegovina
Bouvet Island
Botswana
Brasil (Brazil)
British Indian Ocean Territory
Brunei Darussalam
Bulgaria
Burkina Faso
Burundi
Cambodia
Cameroon
Cape Verde
Cayman Islands
Central African Republic
Česká republika (Czech Republic)
Chad
Chile
中国 (China)
Christmas Island
Città Di Vatican
Cocos (Keeling) Islands
Cook Islands
Colombia
Comoros
Congo
The Democratic Republic of Congo
Costa Rica
Croatia
Cyprus
Côte D'Ivoire
Danmark (Denmark)
Deutschland (Germany)
Djibouti
Dominica
Ecuador
Egypt
El Salvador
Equatorial Guinea
Eritrea
España (Spain)
Estonia
Ethiopia
Faroese Føroyar
Fiji
France
French Southern Territories
French Guiana
Gabon
Gambia
Georgia
Ghana
Gilbralter
Greece
Greenland
Grenada
Guatemala
Guadeloupe
Guam (USA)
Guinea
Guinea-Bissau
Guyana
Haiti
Heard Island and McDonald Islands
Honduras
Hong Kong
Hungary
Iceland
India
Indonesia
Iraq
Ireland
Israel
Islas Malvinas
Italia (Italy)
Jamaica
日本 (Japan)
Jordan
Kazakhstan
Kenya
Kiribati
대한민국 (Korea Republic of)
Kuwait
Kyrgyzstan
Laos
Latvia
Lebanon
Lesotho
Liberia
Libya
Liechtenstein
Lithuania
Luxembourg
Macao
Macedonia
Madagascar
Malawi
Malaysia
Maldives
Mali
Malta
Marshall Islands
Martinique
Mauritania
Mauritius
Mayotte
México (Mexico)
Micronesia
Moldova
Monaco
Mongolia
Montenegro
Monserrat
Morocco
Mozambique
Myanmar
Namibia
Nauru
Nederland (Netherlands)
Netherlands Antilles
Nepal
New Caledonia
New Zealand
Nicaragua
Niger
Nigeria
Niue
Norge (Norway)
Norfolk Island
Northern Mariana Islands
Oman
Österreich (Austria)
Pakistan
Palau
Palestine
Panama
Papua New Guinea
Paraguay
Perú (Peru)
Philippines
Pitcairn Island
Puerto Rico
Россия (Russia)
Polska (Poland)
Polynesia (French)
Portugal
Qatar
República Dominicana (Dominican Republic)
Réunion
România (Romania)
Rwanda
Saint Helena
Saint Pierre and Miquelon
Saint Kitts and Nevis
Saint Lucia
Saint Vincent and The Grenadines
San Marino
Sao Tome and Principe
Saudi Arabia
Schweiz (Switzerland)
Senegal
Serbia
Seychelles
Sierra Leone
Singapore
Slovakia
Slovenia
Solomon Islands
Somalia
South Africa
South Georgia and The South Sandwich Islands
South Sudan
Sri Lanka
Sudan
Suomi (Finland)
Suriname
Svalbard and Jan Mayen
Sverige (Sweden)
Swaziland
Taiwan, China
Tajikistan
Tanzania
Thailand
Timor-Leste
Tokelau
Togo
Tonga
Trinidad and Tobago
Tunisia
Türkiye (Turkey)
Turkmenistan
Turks and Caicos Islands
Tuvalu
Uganda
Ukraine
United Arab Emirates
United Kingdom
United States Minor Outlying Islands
Uruguay
Uzbekistan
Vanuatu
Virgin Islands (British)
Virgin Islands (USA)
Venezuela
Vietnam
Wallis and Futuna
Western Sahara
Western Samoa
Yemen
Zambia
Zimbabwe
 
Postal Code 
*
 
 
Products of Interest 
*
 
- Select -
Air leak / Partial Discharge detection tools
Calibration tools
Power quality
Thermal imaging
Other
 
iGLastMSCRMCampaignID 
 
 
 
Check this box if you would like to receive information by email (or through social media platforms you visit, by us using your email address, subject always to your settings) about Fluke’s latest products, services, offers and events. You are free to withdraw this consent at any time and a link to unsubscribe will be included in each email sent. For more information about how Fluke handles personal data, see Fluke’s Privacy Policy. Fluke includes Fluke Corporation and its corporate subsidiaries and affiliated companies. 
 
consentLanguage 
 
Privacy policy
 
 
 
 
 
Talk to Sales
 
 
 
 
 
Distributors
Where to buy
Grey market
Fluke Platinum Technical Distributors
 
Promotions
 
 
 
 
My Account
Register
Sign in
 
 
 
Toggle navigation
 
 
 
 
 
 
 
 
 
 
 
 
Home
 
 
Products
 
 
Building infrastructure
 
 
Laser distance meters
 
Fluke 417D Laser Distance Meter
bvseo_sdk, p_sdk, 3.2.1
CLOUD, getAggregateRating, 23.22ms
REVIEWS, PRODUCT
bvseo-msg: HTTP status code of 404 was returned; HTTP status code of 404 was returned;
 
 
 
 
Key features
The Fluke 417D laser meter is accurate, durable, and easy to use—just point and shoot
Instantly measure up to 40 m (131 ft.) with 1-button point-and-click
Continuous measurement capable: adjusting as you move closer and farther from your target
Quickly calculate area (sq feet/meters)
1-meter drop tested and IP54 rated: built to withstand rainy or dusty conditions
Great for interior and exterior applications
 
 
 Manuals + resources 
 
 
 
 
 
Buy now
 
 
Product overview
 
Specifications
 
Models
 
Reviews + Q&A
 
Manuals + resources
 
Product overview: Fluke 417D Laser Distance Meter
The Fluke 417D is accurate, durable, and easy to use—just point and shoot. The simple design and easy, one-button measurement operation allows you to minimize time spent measuring and maximize the reliability of measurements.
Additional Product Features:
Large, 2-line illuminated LCD screen.
Three different measurement tasks can be completed quickly and easily with one hand.
The bright laser is clearly visible, so you can always see your target point even from a hard-to-reach spot or long distance.
Designed for both indoor and outdoor applications.
Operates with the Fluke durability and quality you expect.
Protected by a 3-year warranty.
 
Specifications: Fluke 417D Laser Distance Meter
417D
Typical range [1]
0.2-40 m/0.6-131 ft
Typical measuring tolerance* [1]
2.0 mm ± 1.5 mm/± 0.06 in ***
Maximum measuring tolerance [2]
± 3.0 mm/0.12 in ***
Accuracy up to 10m (+/-)
± 2 mm
Display
2 line/1 mm/1/32 in
Display illumination
Yes
Laser point at distance
6/30/60 mm (10/40/100 m)
Area
Yes
Units setting (smallest units displayed)
0,000m, 0' 00'' 1/32, 0 in 1/32
Auto laser switch off
90 sec
Auto power switch off
180 sec
General
Laser class
II
Laser type
635 nm, <1 mW
Protection class
IP54
Battery life (2 x AAA) 1.5 V NEDA 24A/IEC LR03
Up to 3,000 measurements
Size (Hx W x D)
11.9 x 3.8 x 2.6 cm
Drop test
1 meter
Weight (with batteries)
95g (3.35 oz)
Temperature range: Storage
-25 °C to 70 °C (-13 °F to 158 °F)
Temperature range: Operation
-10 °C to 50 °C (14 °F to 122 °F)
Calibration cycle
Not applicable
Maximum relative humidity
85 % @ 20°F to 120 °F
(-7 °C to 50 °C)
Safety
CAN/CSA-C22.2 No. 61010-1-04, UL Std. No. 61010-1 (2nd Edition), ISA-82.02.01, IEC Standard No. 61010-1:2001, EN60825-1:2007 (Class II)
EMC
61326-1:2006
[1] Applies for 100 % target reflectivity (white painted wall), low background illumination, 25 °C (13 °F).
[2] Applies for 10 % to 500 % target reflectivity, high background illumination, -10 °C to +50 °C (14 °F to +122 °F).
[3] Tolerances apply from 0.05 m to 10 m (0.001 ft to 32.8 ft) with a confidence level of 95 %. The maximum tolerance may deteriorate to 0.1 mm/m (0.003 in/ft) between 10 m to 30 m (32.8 ft to 98.4 ft) and to 0.15 mm/m (0.005 in/ft) for distances above 30 m (98.4 ft).
[4] Applies for 100 % target reflectivity, background illumination between 10,000 lux and 30,000 lux.
[5] After user calibration. Additional angle related deviation of ± 0.01° per degree up to ± 45° in each quadrant. Applies at room temperature. For the whole operating temperature range the maximum deviation increases by ± 0.1°.
 
Models: Fluke 417D Laser Distance Meter
Fluke 417D
Fluke 417D Laser Distance Measurer (Meter)
Buy it
Includes:
Two AAA batteries
Users manual (17 languages)
Quick reference guide
Lanyard
Three-year warranty
 
bvseo_sdk, p_sdk, 3.2.1
CLOUD, getContent, 22.05ms
QUESTIONS, PRODUCT
bvseo-msg: HTTP status code of 404 was returned;
bvseo_sdk, p_sdk, 3.2.1
CLOUD, getReviews, 21.97ms
REVIEWS, PRODUCT
bvseo-msg: HTTP status code of 404 was returned;
 
Manuals + resources: Fluke 417D Laser Distance Meter
 
 Manuals (3) 
 
417D/424D | Users manual
 
417D/424D | Quick reference guide
 
417D/424D | Safety sheet
 
 Data sheet (1) 
 
Fluke 417D Laser Distance Measurer Technical Data
 
 Price (1) 
 
Price list
 
 Register products 
 
Register product
 
Related products
62 MAX Mini Infrared Thermometer
Designed with your on-the-job needs in mind, the Fluke 62 MAX, 62 MAX+ Mini Infrared Thermometers are everything you'd expect from the experts in measurement tools. Small in size, extremely accurate and very easy to use.
 
62 MAX Mini Infrared Thermometer
 is rated 
3.5
 out of 
5
 by 
26
.
bvseo_sdk, p_sdk, 3.2.1
CLOUD, getAggregateRating, 22.74ms
REVIEWS, PRODUCT
Fluke 323 True RMS Clamp Meter
Fluke 320 Series Clamp Meters for electrical troubleshooting
 
Fluke 323 True RMS Clamp Meter
 is rated 
4.3
 out of 
5
 by 
34
.
bvseo_sdk, p_sdk, 3.2.1
CLOUD, getAggregateRating, 23.18ms
REVIEWS, PRODUCT
 
 
 
 
Tech support
 
Tech support
service.uk@fluke.com
800-44-FLUKE (800-873-5853)
 
Repairs
service.uk@fluke.com
How to repair and replace Fluke products
 
Distributor questions
+44 (0)20 7942 0708
 
 
 
About Fluke
 
About us
 
Careers
 
Press
 
Supplier handbook
 
Modern slavery
 
Contact us
 
Contact us
 
Repair
 
Technical support
 
Manuals + resources
 
Promotions
 
Manuals
 
Product registration
 
Safety notices
 
Test tools catalog
 
Where to buy
 
 
Fluke Newsletters Signup
 
 
 
 
Facebook
 
 
 
 
 
YouTube
 
 
 
 
 
Twitter
 
 
 
 
 
LinkedIn
 
 
 
 
 
Instagram
 
 
 
 
 
Fluke
. 
 
 Keeping your world up and running.® 
 
Privacy policy
 
Fluke terms of use
 
Fluke terms and conditions of sale
 
Fluke terms and conditions of service
 
Site map
 
©1995 - 2023 Fluke Corporation 
 
 
 
 
Products
 
Featured
 
Award winning
 
New Fluke products
 
Test Tools Catalog
 
Fluke software
 
Accessories
 
Cases and holsters
 
Test leads, probes and clips
 
Building infrastructure
 
HVAC tools
 
Indoor air quality testing
 
Laser distance meters
 
Laser levels
 
Electrical tools
 
Digital multimeters
 
Basic electrical testers
 
Clamp meters
 
Power quality
 
Earth ground
 
Installation testers
 
Insulated tools
 
Intrinsically safe
 
Battery analyzers
 
Insulation testers
 
Portable oscilloscopes
 
Portable appliance testers
 
Solar industry tools
 
eMobility
 
Acoustic and thermal imaging
 
Thermal imaging cameras
 
Acoustic imaging and borescopes
 
IR windows
 
Temperature measurement
 
Contact thermometers
 
IR thermometers
 
Network cable testers
 
Industrial Ethernet testers
 
Alignment tools
 
Laser alignment
 
Vibration analysis
 
Calibration tools
 
mA loop calibrators
 
Multifunction calibrators
 
Pressure calibrators
 
Temperature calibrators
 
Condition monitoring
 
eMaint CMMS
 
Fluke Connect
 
Connect2Assets
 
Fluke Mobile
 
Connected reliability
 
Power monitoring
 
Vibration
 
Learn
 
Fluke Resource Center
 
Fundamentals
 
Calibration
 
Energy management
 
Maintenance and monitoring
 
Safety
 
Troubleshooting
 
All topics
 
Fluke education partnership program
 
Online courses
 
Digital multimeter basics
 
Electrical measurement safety
 
Insulation Resistance
 
Motor and drive troubleshooting
 
Seminars and training
 
Tradeshows
 
Tools and calculators
 
Air leakage calculator
 
FOV calculator
 
LeakQ report generator
 
PDQ Mode Reporting Tool
 
Webinars
 
Support
 
Customer service
 
Contact us
 
Technical support
 
Calibration services
 
Repair
 
Service center locations
 
Return materials authorization
 
Product resources
 
Fluke Manuals
 
Product registration
 
Recycle program
 
Safety notices
 
Service quote request
 
Download software updates
 
Warranties