Iron–carbon alloy phases
Ferrite Allotropes of ferrite include: α-iron (Alpha ferrite) δ-iron (Delta ferrite) β-iron (Beta ferrite) ε-iron (Hexaferrum) γ-iron (Gamma ferrite) Austenite (γ-iron + carbon in solid solution) Cementite (iron carbide, Fe3C) Graphite (allotrope of carbon) Martensite (metastable phase) ε-carbon (transitional carbide, Fe24C)
Microstructures
Spheroidite (ferrite with cementite inclusions) Pearlite (ferrite-cementite eutectoid, 0.8% carbon) Bainite (transitional microstructure) Ledeburite (austenite-cementite eutectic, 4.3% carbon) Tempered martensite (martensite + ferrite + ε-carbon or cementite, or both) Widmanstatten structures (cementite needles, forms during improper tempering)
Steel classes
Crucible steel (specialty steels) Carbon steel (≤ 2.1% carbon; low alloy) Spring steel (low or no alloy) Alloy steel (contains non-carbon elements) Maraging steel (contains nickel) Stainless steel (contains ≥ 10.5% chromium) Weathering steel (controlled corrosion rate) Tool steel (alloy steel for tools)
Other iron-based materials
Cast iron (> 2.1% carbon) Gray iron (hypereutectic cast-iron, contains graphite) White iron (eutectic or hypoeutectic cast-iron, contains ledeburite) Ductile iron (black-tempered cast-iron, less brittle) Malleable iron (white-tempered cast-iron, workable) Wrought iron (ferrite, contains slag)

In metallurgy, stainless steel, also known as inox steel or inox from French "inoxydable", is defined as a steel alloy with a minimum of 10.5%[1] to 11% chromium content by mass.[2]

Stainless steel does not readily corrode, rust or stain with water as ordinary steel does, but despite the name it is not fully stain-proof, most notably under low oxygen, high salinity, or poor circulation environments.[3] It is also called corrosion-resistant steel or CRES when the alloy type and grade are not detailed, particularly in the aviation industry. There are different grades and surface finishes of stainless steel to suit the environment the alloy must endure. Stainless steel is used where both the properties of steel and resistance to corrosion are required.

Stainless steel differs from carbon steel by the amount of chromium present. Unprotected carbon steel rusts readily when exposed to air and moisture. This iron oxide film (the rust) is active and accelerates corrosion by forming more iron oxide, and due to the dissimilar size of the iron and iron oxide molecules (iron oxide is larger) these tend to flake and fall away. Stainless steels contain sufficient chromium to form a passive film of chromium oxide, which prevents further surface corrosion and blocks corrosion from spreading into the metal's internal structure, and due to the similar size of the steel and oxide molecules they bond very strongly and remain attached to the surface.[4]

Passivation only occurs if the proportion of chromium is high enough and oxygen is present.

## History[edit]

An announcement, as it appeared in the 1915 New York Times, of the development of stainless steel[5]

A few corrosion-resistant iron artifacts survive from antiquity. A famous example is the Iron Pillar of Delhi, erected by order of Kumara Gupta I around AD 400. Unlike stainless steel, however, these artifacts owe their durability not to chromium but to their high phosphorus content, which, together with favorable local weather conditions, promotes the formation of a solid protective passivation layer of iron oxides and phosphates, rather than the non-protective cracked rust layer that develops on most ironwork.

The corrosion resistance of iron-chromium alloys was first recognized in 1821 by French metallurgist Pierre Berthier, who noted their resistance against attack by some acids and suggested their use in cutlery. Metallurgists of the 19th century were unable to produce the combination of low carbon and high chromium found in most modern stainless steels, and the high-chromium alloys they could produce were too brittle to be practical.

In the late 1890s Hans Goldschmidt of Germany developed an aluminothermic (thermite) process for producing carbon-free chromium. Between 1904 and 1911 several researchers, particularly Leon Guillet of France, prepared alloys that would today be considered stainless steel.

Friedrich Krupp Germaniawerft built the 366-ton sailing yacht Germania featuring a chrome-nickel steel hull in Germany in 1908.[6] In 1911, Philip Monnartz reported on the relationship between chromium content and corrosion resistance. On October 17, 1912, Krupp engineers Benno Strauss and Eduard Maurer patented austenitic stainless steel as ThyssenKrupp Nirosta.[7]

Similar developments were taking place contemporaneously in the United States, where Christian Dantsizen and Frederick Becket were industrializing ferritic stainless steel. In 1912, Elwood Haynes applied for a US patent on a martensitic stainless steel alloy, which was not granted until 1919.[8]

Also in 1912, Harry Brearley of the Brown-Firth research laboratory in Sheffield, England, while seeking a corrosion-resistant alloy for gun barrels, discovered and subsequently industrialized a martensitic stainless steel alloy. The discovery was announced two years later in a January 1915 newspaper article in The New York Times.[5] The metal was later marketed under the 'Staybrite' brand by Firth Vickers in England and was used for the new entrance canopy for the Savoy Hotel in London in 1929.[9]

Brearley applied for a US patent during 1915 only to find that Haynes had already registered a patent. Brearley and Haynes pooled their funding and with a group of investors formed the American Stainless Steel Corporation, with headquarters in Pittsburgh, Pennsylvania.[10] In the beginning stainless steel was sold in the US under different brand names like 'Allegheny metal' and 'Nirosta steel'. In 1929 before the Great Depression hit, over 25,000 tons of stainless steel were manufactured and sold in the US.[11]

## Properties[edit]

High oxidation-resistance in air at ambient temperature is normally achieved with additions of a minimum of 13% (by weight) chromium, and up to 26% is used for harsh environments.[12] The chromium forms a passivation layer of chromium(III) oxide (Cr2O3) when exposed to oxygen. The layer is too thin to be visible, and the metal remains lustrous. The layer is impervious to water and air, protecting the metal beneath. Also, this layer quickly reforms when the surface is scratched. This phenomenon is called passivation and is seen in other metals, such as aluminium and titanium. Corrosion-resistance can be adversely affected if the component is used in a non-oxygenated environment, a typical example being underwater keel bolts buried in timber.

When stainless steel parts such as nuts and bolts are forced together, the oxide layer can be scraped off, causing the parts to weld together. When disassembled, the welded material may be torn and pitted, an effect known as galling. This destructive galling can be best avoided by the use of dissimilar materials for the parts forced together, for example bronze and stainless steel, or even different types of stainless steels (martensitic against austenitic), when metal-to-metal wear is a concern. Nitronic alloys reduce the tendency to gall through selective alloying with manganese and nitrogen. Additionally, threaded joints may be lubricated to prevent galling.

Similarly to steel, stainless steel is not a very good conductor of electricity, with about a few percent of the electrical conductivity of copper.[13] Ferritic and martensitic stainless steels are magnetic. Austenitic stainless steels are non-magnetic.

## Applications[edit]

The 630-foot-high (190 m), stainless-clad (type 304) Gateway Arch defines St. Louis's skyline The pinnacle of New York's Chrysler Building is clad with Nirosta stainless steel, a form of Type 302[14][15] An art deco sculpture on the Niagara-Mohawk Power building in Syracuse, New York

Stainless steel?s resistance to corrosion and staining, low maintenance and familiar lustre make it an ideal material for many applications. There are over 150 grades of stainless steel, of which fifteen are most commonly used. The alloy is milled into coils, sheets, plates, bars, wire, and tubing to be used in cookware, cutlery, household hardware, surgical instruments, major appliances, industrial equipment (for example, in sugar refineries) and as an automotive and aerospace structural alloy and construction material in large buildings. Storage tanks and tankers used to transport orange juice and other food are often made of stainless steel, because of its corrosion resistance and antibacterial properties. This also influences its use in commercial kitchens and food processing plants, as it can be steam-cleaned and sterilized and does not need paint or other surface finishes.

Stainless steel is used for jewelry and watches with 316L being the type commonly used for such applications. It can be re-finished by any jeweler and will not oxidize or turn black.

Some firearms incorporate stainless steel components as an alternative to blued or parkerized steel. Some handgun models, such as the Smith Wesson Model 60 and the Colt M1911 pistol, can be made entirely from stainless steel. This gives a high-luster finish similar in appearance to nickel plating. Unlike plating, the finish is not subject to flaking, peeling, wear-off from rubbing (as when repeatedly removed from a holster), or rust when scratched.

Some automotive manufacturers use stainless steel as decorative highlights in their vehicles.

### Architecture[edit]

Main article: Architectural steel

Stainless steel is used for buildings for both practical and aesthetic reasons. Stainless steel was in vogue during the art deco period. The most famous example of this is the upper portion of the Chrysler Building (pictured). Some diners and fast-food restaurants use large ornamental panels and stainless fixtures and furniture. Because of the durability of the material, many of these buildings retain their original appearance.

Type 316 stainless is used on the exterior of both the Petronas Twin Towers and the Jin Mao Building, two of the world's tallest skyscrapers.[15]

The Parliament House of Australia in Canberra has a stainless steel flagpole weighing over 220 tonnes (240 short tons).

The aeration building in the Edmonton Composting Facility, the size of 14 hockey rinks, is the largest stainless steel building in North America.

### Bridges[edit]

- Cala Galdana Bridge in Minorca (Spain) is the first stainless steel road bridge.
- Sant Fruitos Pedestrian Bridge (Catalonia, Spain), arch pedestrian bridge.
- Padre Arrupe Bridge (Bilbao, Spain) links the Guggenheim museum to the University of Deusto.[16]

### Monuments and sculptures[edit]

- The Unisphere, constructed as the theme symbol of the 1964-5 World's Fair in New York City, is constructed of Type 304L stainless steel as a sphere with a diameter of 120 feet, or 36.57 meters.
- The Gateway Arch (pictured) is clad entirely in stainless steel: 886 tons (804 metric tonnes) of 0.25 in (6.4 mm) plate, #3 finish, type 304 stainless steel.[17]
- The United States Air Force Memorial has an austenitic stainless steel structural skin.
- The Atomium in Brussels, Belgium was renovated with stainless-steel cladding in a renovation completed in 2006; previously the spheres and tubes of the structure were clad in aluminium.
- The Cloud Gate sculpture by Anish Kapoor, in Chicago US.
- The Sibelius monument in Helsinki, Finland, is made entirely of stainless steel tubes.

### Other[edit]

Automotive bodies

The Allegheny Ludlum Corporation worked with Ford on various concept cars with stainless steel bodies from the 1930s through the 1970s, as demonstrations of the material's potential. In 1981 and 1982, the DeLorean DMC-12 production automobile used stainless steel body panels over a glass-reinforced plastic monocoque.

Passenger rail cars

Rail cars have commonly been manufactured using corrugated stainless steel panels (for additional structural strength). This was particularly popular during the 1960s and 1970s, but has since declined. One notable example was the early Pioneer Zephyr. Notable former manufacturers of stainless steel rolling stock included the Budd Company (USA), which has been licensed to Japan's Tokyu Car Corporation, and the Portuguese company Sorefame.

Aircraft

Budd also built an airplane, the Budd BB-1 Pioneer, of stainless steel tube and sheet, which is on display at the Franklin Institute.

## Recycling and reuse[edit]

Stainless steel is 100% recyclable. An average stainless steel object is composed of about 60% recycled material of which approximately 40% originates from end-of-life products and about 60% comes from manufacturing processes.[18] According to the International Resource Panel's Metal Stocks in Society report, the per capita stock of stainless steel in use in society is 80?180?kg in more developed countries and 15?kg in less-developed countries.

There is a secondary market that recycles usable scrap for many stainless steel markets. The product is mostly coil, sheet and blanks. This material is purchased at a less-than-prime price and sold to commercial quality stampers and sheet metal houses. The material may have scratches, pits and dents but is made to the current specifications.

## Types of stainless steel[edit]

Pipes and fittings made of stainless steel

There are different types of stainless steels: when nickel is added, for instance, the austenite structure of iron is stabilized. This crystal structure makes such steels virtually non-magnetic and less brittle at low temperatures. For greater hardness and strength, more carbon is added. With proper heat treatment, these steels are used for such products as razor blades, cutlery, and tools.

Significant quantities of manganese have been used in many stainless steel compositions. Manganese preserves an austenitic structure in the steel, similar to nickel, but at a lower cost.

Stainless steels are also classified by their crystalline structure:

- Austenitic, or 300 series, stainless steels have an austenitic crystalline structure, which is a face-centered cubic crystal structure. Austenite steels make up over 70% of total stainless steel production. They contain a maximum of 0.15% carbon, a minimum of 16% chromium and sufficient nickel and/or manganese to retain an austenitic structure at all temperatures from the cryogenic region to the melting point of the alloy. The most widely used austenite steel is the 304 grade or A2 stainless steel (not to be confused with A2 grade steel, also named Tool steel, a steel). The second most common austenite steel is the 316 grade, also called marine grade stainless, used primarily for its increased resistance to corrosion. A typical composition of 18% chromium and 10% nickel, commonly known as 18/10 stainless, is often used in cutlery and high quality cookware. 18/0 and 18/8 are also available.

  Superaustenitic stainless steels, such as alloy AL-6XN and 254SMO, exhibit great resistance to chloride pitting and crevice corrosion because of high molybdenum content (>6%) and nitrogen additions, and the higher nickel content ensures better resistance to stress-corrosion cracking versus the 300 series. The higher alloy content of superaustenitic steels makes them more expensive. Other steels can offer similar performance at lower cost and are preferred in certain applications, for example ASTM A387 is used in pressure vessels but is a low alloy carbon steel with a chromium content of 0.5% to 9%.[19] Low-carbon versions, for example 316L or 304L, are used to avoid corrosion problems caused by welding. Grade 316LVM is preferred where biocompatibility is required (such as body implants and piercings).[20] The "L" means that the carbon content of the alloy is below 0.03%, which reduces the sensitization effect (precipitation of chromium carbides at grain boundaries) caused by the high temperatures involved in welding.

- Ferritic stainless steels generally have better engineering properties than austenitic grades, but have reduced corrosion resistance, because of the lower chromium and nickel content. They are also usually less expensive. They contain between 10.5% and 27% chromium and very little nickel, if any, but some types can contain lead. Most compositions include molybdenum; some, aluminium or titanium. Common ferritic grades include 18Cr-2Mo, 26Cr-1Mo, 29Cr-4Mo, and 29Cr-4Mo-2Ni. These alloys can be degraded by the presence of chromium, an intermetallic phase which can precipitate upon welding.

- Martensitic stainless steels are not as corrosion-resistant as the other two classes but are extremely strong and tough, as well as highly machinable, and can be hardened by heat treatment. Martensitic stainless steel contains chromium (12?14%), molybdenum (0.2?1%), nickel (less than 2%), and carbon (about 0.1?1%) (giving it more hardness but making the material a bit more brittle). It is quenched and magnetic.

- Precipitation-hardening martensitic stainless steels have corrosion resistance comparable to austenitic varieties, but can be precipitation hardened to even higher strengths than the other martensitic grades. The most common, 17-4PH, uses about 17% chromium and 4% nickel.

- Duplex stainless steels have a mixed microstructure of austenite and ferrite, the aim usually being to produce a 50/50 mix, although in commercial alloys the ratio may be 40/60. Duplex stainless steels have roughly twice the strength compared to austenitic stainless steels and also improved resistance to localized corrosion, particularly pitting, crevice corrosion and stress corrosion cracking. They are characterized by high chromium (19?32%) and molybdenum (up to 5%) and lower nickel contents than austenitic stainless steels.

  The properties of duplex stainless steels are achieved with an overall lower alloy content than similar-performing super-austenitic grades, making their use cost-effective for many applications. Duplex grades are characterized into groups based on their alloy content and corrosion resistance.
  - Lean duplex refers to grades such as UNS S32101 (LDX 2101), S32304, and S32003.
  - Standard duplex is 22% chromium with UNS S31803/S32205 known as 2205 being the most widely used.
  - Super duplex is by definition a duplex stainless steel with a pitting corrosion equivalent (PRE) > 40, where PRE = %Cr 3.3x(%Mo 0.5x%W) 16x%N. Usually super duplex grades have 25% chromium or more and some common examples are S32760 (Zeron 100), S32750 (2507) and S32550 (Ferralium),.
  - Hyper duplex refers to duplex grades with a PRE > 48 and at the moment only UNS S32707 and S33207 are available on the market.

### Comparison of standardized steels[edit]

EN-standard Steel no. k.h.s DIN | EN-standard Steel name | SAE grade | UNS
--- | --- | --- | ---
|  | 440A | S44002
1.4112 | X90CrMoV18 | 440B | S44003
1.4125 | X105CrMo17 | 440C | S44004
|  | 440F | S44020
1.4016 | X6Cr17 | 430 | S43000
1.4408 | G-X 6 CrNiMo 18-10 | 316 |
1.4512 | X6CrTi12 | 409 | S40900
|  | 410 | S41000
1.4310 | X10CrNi18-8 | 301 | S30100
1.4318 | X2CrNiN18-7 | 301LN |
1.4307 | X2CrNi18-9 | 304L | S30403
1.4306 | X2CrNi19-11 | 304L | S30403
1.4311 | X2CrNiN18-10 | 304LN | S30453
1.4301 | X5CrNi18-10 | 304 | S30400
1.4948 | X6CrNi18-11 | 304H | S30409
1.4303 | X5CrNi18-12 | 305 | S30500
| X5CrNi30-9 | 312 |
1.4541 | X6CrNiTi18-10 | 321 | S32100
1.4878 | X12CrNiTi18-9 | 321H | S32109
1.4404 | X2CrNiMo17-12-2 | 316L | S31603
1.4401 | X5CrNiMo17-12-2 | 316 | S31600
1.4406 | X2CrNiMoN17-12-2 | 316LN | S31653
1.4432 | X2CrNiMo17-12-3 | 316L | S31603
1.4435 | X2CrNiMo18-14-3 | 316L | S31603
1.4436 | X3CrNiMo17-13-3 | 316 | S31600
1.4571 | X6CrNiMoTi17-12-2 | 316Ti | S31635
1.4429 | X2CrNiMoN17-13-3 | 316LN | S31653
1.4438 | X2CrNiMo18-15-4 | 317L | S31703
1.4362 | X2CrNi23-4 | 2304 | S32304
1.4462 | X2CrNiMoN22-5-3 | 2205 | S31803/S32205
1.4539 | X1NiCrMoCu25-20-5 | 904L | N08904
1.4529 | X1NiCrMoCuN25-20-7 |  | N08926
1.4547 | X1CrNiMoCuN20-18-7 | 254SMO | S31254

### Stainless steel grades[edit]

There are a number of different systems for grading stainless and other steels. The article on US SAE steel grades details a large number of grades with their properties.

### Stainless steel in 3D printing[edit]

Some 3D printing providers have developed proprietary stainless steel sintering[21] blends for use in rapid prototyping. Currently available grades do not vary significantly in their properties.[22]

## Stainless steel finishes[edit]

Main article: Brushed metal
316L stainless steel, with an unpolished, mill finish

Standard mill finishes can be applied to flat rolled stainless steel directly by the rollers and by mechanical abrasives. Steel is first rolled to size and thickness and then annealed to change the properties of the final material. Any oxidation that forms on the surface (mill scale) is removed by pickling, and a passivation layer is created on the surface. A final finish can then be applied to achieve the desired aesthetic appearance.

- No. 0: Hot rolled, annealed, thicker plates
- No. 1: Hot rolled, annealed and passivated
- No. 2D: Cold rolled, annealed, pickled and passivated
- No. 2B: Same as above with additional pass-through highly polished rollers
- No. 2BA: Bright annealed (BA or 2R) same as above then bright annealed under oxygen-free atmospheric condition
- No. 3: Coarse abrasive finish applied mechanically
- No. 4: Brushed finish
- No. 5: Satin finish
- No. 6: Matte finish (brushed but smoother than #4)
- No. 7: Reflective finish
- No. 8: Mirror finish
- No. 9: Bead blast finish
- No. 10: Heat colored finish-wide range of electropolished and heat colored surfaces

## See also[edit]

Argon oxygen decarburization List of blade materials Panel edge staining Stainless steel fiber | Marine grade stainless Rouging Stainless steel soap

## References[edit]

1. ^ "The Stainless Steel Family". Retrieved 2009-11-12.
2. ^ "Steel Glossary". American Iron and Steel Institute (AISI). Retrieved October 21, 2008.
3. ^ "Why is Stainless Steel Stainless?". Retrieved 2008-12-20.
4. ^ Stainless Steels and Alloys: Why They Resist Corrosion and How They Fail". Corrosionclinic.com. Retrieved on 2012-06-29.
5. ^ a b "A non-rusting steel". New York Times. 31 January 1915.
6. ^ "A Proposal to Establish the Shipwreck Half Moon as a State Underwater Archaeological Preserve". Bureau of Archaeological Research, Division of Historical Resources, Florida Department of State. May 2000.
7. ^ "ThyssenKrupp Nirosta: History". Retrieved 2007-08-13.
8. ^ Rodney P. Carlisle, Scientific American Inventions and Discoveries, p. 380, John Wiley and Sons, 2004, ISBN 0-471-24410-4
9. ^ Geoffrey Howse, A Photographic History of Sheffield Steel, History Press, 2011, ISBN 0752459856
10. ^ Cobb, Harold M. (2010). The History of Stainless Steel. ASM Internationa. p. 360. ISBN 1-61503-010-7.
11. ^ Bonnier Corporation (1930). Popular Science. Bonnier Corporation. pp. 31?. ISSN 0161-7370.
12. ^ Ashby, Michael F.; David R. H. Jones (1992) [1986]. "Chapter 12". Engineering Materials 2 (with corrections ed.). Oxford: Pergamon Press. p. 119. ISBN 0-08-032532-7.
13. ^ Electrical resistivity and conductivity
14. ^ http://www.thyssenkrupp-nirosta.de/index.php?id=576
15. ^ a b What is Stainless Steel? nickelinstitute.org
16. ^ "Stainless steel bridge" "Stainless Steel Bridge in Bilbao". Outokumpu.
17. ^ Gateway Arch Fact Sheet. Nps.gov. Retrieved on 2012-06-29.
18. ^ "The Recycling of Stainless Steel ("Recycled Content" and "Input Composition" slides)" (Flash). International Stainless Steel Forum. 2006. Retrieved 2006-11-19.
19. ^ ASTM A 387/ A387M ? 06a Standard Specification for Pressure Vessel Plates, Alloy Steel, Chromium-Molybdenum
20. ^ Material Properties Data: Marine Grade Stainless Steel. Makeitfrom.com. Retrieved on 2012-06-29.
21. ^ Stainless Steel. Shapeways. Retrieved on 2012-06-29.
22. ^ Material Properties Data: 3D Printing Steel. Makeitfrom.com. Retrieved on 2012-06-29.

## External links[edit]

| This article's use of external links may not follow Wikipedia's policies or guidelines. Please improve this article by removing excessive or inappropriate external links, and converting useful links where appropriate into footnote references. (March 2012)

| Wikimedia Commons has media related to API.

| Look up api in Wiktionary, the free dictionary.

- Animated presentation outlining the manufacture process by industry leaders Outokumpu
- Glossary of Stainless Steel Related Terms by Specialty Steel Supply
- Stainless Steel Properties and Corrosion Resistance
- Comprehensive Information About Stainless Steel by The Stainless Steel Information Center
- Technical Library on Stainless Steel by BSSA
- Comprehensive Information About Metallurgy of Stainless Steel by Cambridge University
- Converter for Stainless Steel Standards
- Stainless Steel Composition
- Super Duplex Imperial Properties
- Super Duplex Metric Properties
- Comparison of foreign standards in stainless steel specifications
- Online Information Centre for Stainless Steel in Construction by the SCI.org of the UK
- Practical Guidelines for the Fabrication of Duplex Stainless Steels by IMOA
- Tables of Technical Properties by Euro Inox
- Guide to Stainless Steel Finishes by Euro Inox
- FAQ: Cleaning Stainless Steel in the Home by Euro Inox
- The Ferritic Solution. Properties, Advantages, Applications by ISSF
- How do you remove and prevent flash rust on stainless steel?

Metalworking
Casting
Processes | Centrifugal Continuous Die Evaporative-pattern Full mold Lost foam Investment (Lost wax) Permanent mold Plaster mold Sand Semi-solid metal Shaw process Shell molding Spin
Components | Chill Cope and drag Core Flask Molding sand Pattern Riser Sprue
Terminology | Casting defects Draft Dross Ingot Semi-finished casting products Slag
Forming, fabrication, and finishing
General | Fabrication Piece work Sheet metal
Forming processes | Coining Drawing Electrohydraulic forming Electromagnetic forming Explosive forming Forging Hydroforming Progressive stamping Punching Rolling Sinking Spinning Swaging Tube bending
Joining processes | Brazing Crimping Riveting Soldering Welding
Finishing processes | Anodizing Galvanizing Heat treating Mass finishing Patination Peening Plating Polishing
Machining and computing
Computer-aided engineering | 2.5D CAD CAM G-code Numerical control (NC and CNC) Stewart platform
Drilling and threading | Die head Drill Drill bit Drill bit shank Drill bit sizes Drilling List of drill and tap sizes Tap and die Tap wrench Threading
Grinding and lapping | Abrasive Angle grinder Bench grinder Coated abrasives Cylindrical grinder Diamond plate Flick grinder Grinding Grinding dresser Grinding machine Grinding wheel Jig grinder Lapping Sanding Sharpening stone Spark testing Surface grinder Tool and cutter grinder
Machining | Boring Broaching Electrical discharge machining Electrochemical machining Electron beam machining Endmill Engraving Facing Hobbing Jig borer Machine tool Machining Metal lathe Milling cutter Milling machine Pantograph Photochemical machining Planer Reamer Shaper Turning Ultrasonic machining
Machine tooling | Angle plate Chuck Collet Fixture Indexing head Jig Lathe center Machine taper Magnetic base Mandrel Rotary table Wiggler
Terminology | Cutting fluid Machining vibrations Speeds and feeds Swarf Tolerance Tool and die making Tramp oil
Tools
Cutting machines | Bandsaw Cold saw Laser Miter saw Plasma Water jet cutter
Cutting tools | Broach Burr Chisel Counterbore Countersink End mill File Hand scraper Milling cutter Nibbler Reamer Shears Tipped tool Tool bit
Forming tools | Brake Die English wheel Hydraulic press Machine press Punch press Screw press Stamping press
Hand tools | Clamp Combination square Drift pin Hacksaw Hammer Hand scraper Machinist square Needlegun scaler Piercing saw Pliers Punch Scriber Tap and die Tongs Vise Workbench Wrench
Machine tooling | Angle plate Chuck Collet Fixture Indexing head Jig Lathe center Machine taper Magnetic base Mandrel Rotary table Wiggler
Measuring instruments | Bore gauge Caliper Center gauge Dial indicator Engineer's blue Engineer's spirit level Feeler gauge Gauge Gauge block Go/no go gauge Height gauge Machinist square Marking blue Marking gauge Marking out Micrometer Optical comparator Radius gauge Ruler Sine bar Straightedge Surface plate Tape measure Thread pitch gauge Vernier scale
Smithing tools | Anvil Forge Fuller Hardy tools Pritchel Steam hammer Swage block Trip hammer
Welding
Arc welding | Atomic hydrogen (Athydo/AHW) Electrogas (EGW) Flash Flux-cored (FCAW) Gas metal (Microwire/MIG/GMAW) Gas tungsten (Heliarc/TIG/GTAW) Plasma (PAW) Shielded metal (Stick/MMA/SMAW) Submerged (SAW)
Other processes | Electric resistance (ERW) Electron beam (EBW) Electroslag (ESW) Exothermic Forge Friction Friction stir (FSW) Friction stud Laser beam (LBW) Laser-hybrid Magnetic pulse Oxyacetylene (OAW) Spot (RSW) Ultrasonic Upset
Equipment | Electrode Filler metal Helmet Power supply Robot Shielding gas
Related terms | Heat-affected zone Photokeratitis Residual stress Weldability
Casting Fabrication Forming Jewellery Machining Metallurgy Smithing Tools and terminology Welding

Jewellery
Forms | Anklet Belt buckle Belly chain Bindi Bracelet Brooch Chatelaine Collar pin Crown Cufflink Earring Lapel pin Necklace Pendant Ring Tiara Tie clip Tie pin Toe ring Watch pocket
Making |
People | Bench jeweler Clockmaker Goldsmith Silversmith Jewelry designer Lapidary Watchmaker
Processes | Casting centrifugal lost-wax vacuum Enameling Engraving Filigree Metal clay Plating Polishing Repoussé and chasing Soldering Stonesetting Wire sculpture Wire wrapped jewelry
Tools | Draw plate File Hammer Mandrel Pliers
Materials |
Precious metals | Gold Palladium Platinum Rhodium Silver
Precious metal alloys | Britannia silver Colored gold Crown gold Electrum Shakudō Shibuichi Sterling silver Tumbaga
Base metals | Brass Bronze Copper Mokume-gane Pewter Stainless steel Titanium Tungsten
Mineral gemstones | Aventurine Agate Amethyst Beryl Carnelian Chrysoberyl Diamond Diopside Emerald Garnet Jade Jasper Lapis lazuli Larimar Malachite Marcasite Moonstone Obsidian Onyx Opal Peridot Quartz Ruby Sapphire Sodalite Sunstone Tanzanite Tiger's eye Topaz Tourmaline Turquoise Yogo sapphire
Organic gemstones | Abalone Amber Ammolite Copal Coral Ivory Jet Pearl Nacre
Other natural objects | Shell jewelry
Terms | Carat (mass) Carat (purity) Finding Millesimal fineness
Related topics: Body piercing Fashion Gemology Metalworking Wearable art