[' Based on the search results, here are some recommended air compressors:\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are a top choice for a variety of jobsite applications. They are designed for enhanced usability and serviceability, and the 400HH model offers air pressures up to 200 psi. The compressors are compact and easy to maneuver, with multiple engine options available.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is another high-quality option. It features durable cast-iron cylinders, heads, and frame for continuous operation and extended pump life. The oversized belt wheel provides reliable design and cooler operation, and the high-efficiency stainless steel finger valves are simple, efficient, and easy to maintain.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is a great choice for those looking for a high-pressure air compressor. It has a max tank storage pressure of 225 PSI, providing 80% more usable air than the industry leader. The compressor also has a vertical stand feature and collapsible handle for easy transportation and storage.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and reliable. They feature advanced rotary screw air compressor technology and are designed for 100% duty cycle. The compressors also have a standard quiet enclosure and low oil carryover.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is a great option for those looking for a maintenance-free air compressor. It has a high-pressure design that optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The compressor is also lightweight and easy to transport.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders are a great choice for industrial metal transformation applications. They offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in the line-up. It has a motor-pump that delivers a whopping 6.5 CFM @ 90 PSI. The compressor also has heavy-duty flat-free tires and a fold-down handle for easy storage and low profile.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is equipped with Makita’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and increased compressor efficiency. It has a cast iron cylinder with greater bore and stroke for maximum performance and roll cage construction for extra protection to pump and motor assembly.', ' Based on the search results, here are some recommended air compressors:\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is a top-of-the-line option, offering 80% more usable air than the industry leader. It has a 5.0 SCFM @ 90 PSI for quick recovery, a vertical stand feature and collapsible handle for easy storage, and an efficient high pressure motor that can run with an extension cord. It also has a high flow coupler for maximum nailer performance and a metal console panel for protection.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is another excellent choice, with a high-pressure design that optimizes air tool performance and delivers 2.6 SCFM at 90 psi for quick recovery time. It has a durable oil-free pump for long life and no maintenance, and a shroud, handle, and console cover to protect vital components. It also has two regulated, factory-installed air couplers to support two users.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are a great option for those who need a powerful and portable compressor. They offer air pressures up to 200 psi and a compact design for easy towing and maneuverability. They also have multiple engine options and extended runtime.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up, with a motor-pump that delivers a whopping 6.5 CFM @ 90 PSI. It has a foot-actuated folding handle and heavy-duty flat-free tires for easy mobility, and a cast-iron cylinder and stainless-steel reed valves for longer life.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is a durable and reliable option, with cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. It has an oversized belt wheel for reliable design and cooler operation, and a synthetic lubricant that provides 2,000-hour oil change intervals.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders are a great option for those who need a low total cost of operation. They offer a highly durable spiral bevel gear that reduces vibration and stress of torque transmission, and a regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are a highly efficient option, with advanced rotary screw air compressor technology and a low cost of ownership. They have a standard quiet enclosure, 8,000 hr. premium synthetic fluid, and a long life V-belt drive.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is a powerful and efficient option, with a cast iron cylinder with greater bore and stroke for maximum performance. It has a roll cage construction for extra protection to pump and motor assembly, and an oil drain and oil sight glass conveniently located for easy access and maintenance.\n\nIn conclusion, these are some of the best air compressors available, each with its own unique features and benefits. It is important to consider your specific needs and budget when choosing the right air compressor for you.', ' Based on the search results, here are some recommended air compressors:\n\nThe Rolair VT25BIG is a highly recommended air compressor for its high air output. It delivers a whopping 6.5 CFM @ 90 PSI, making it the highest air output of any direct drive air compressor in the Rolair line-up. The motor-pump is designed with ball bearings, a cast-iron cylinder, and stainless-steel reed valves for longer life. The 2.5 HP motor has overload protection with manual reset and runs at 3400 RPM. The compressor comes with heavy-duty wheels for greater jobsite mobility, a start/stop pressure switch with on/off lever, and a user-friendly control panel.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and reliable sources of compressed air for a wide range of industrial applications. They feature advanced rotary screw air compressor technology, enabling easy maintenance and low cost of ownership. The compressors are designed for 100% duty cycle and have a standard quiet enclosure, 8,000 hr. premium synthetic fluid, and low oil carryover. They also come with a True Blue 5-Year Warranty with start up.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is a high-performance compressor with a max tank storage pressure of 225 PSI, providing 80% more usable air than the industry leader. It has a 5.0 SCFM @ 90 PSI for quick recovery after its initial tank charge is exhausted. The compressor has a vertical stand feature and collapsible handle for easy transportation and storage. It also has a 78 dBA operational noise level for a quieter work environment.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is a powerful compressor that delivers 6.5 CFM @ 90PSI, making it powerful enough to run two framing nailers. It has a cast iron cylinder with greater bore and stroke for maximum performance and a roll cage construction for extra protection to the pump and motor assembly. The compressor has an oil drain and oil sight glass conveniently located for easy access and maintenance.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications. They have a highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are compact and designed for enhanced usability and serviceability. They have multiple units, including the award-winning 400HH featuring air pressures up to 200 psi. The compressors have multiple engine options, including Caterpillar C4.4 (T4F) and Perkins 1204F (T4F). They also have an easy pressure change and extended runtime.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is designed for the professional and is ideal for most anyone, from the do-it-yourselfer to the professional. It has durable cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. The oversized belt wheel provides reliable design and cooler operation. The compressor has high-efficiency stainless steel finger valves that are simple, efficient, and easy to maintain.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is a high-pressure design optimized for air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. It has a durable oil-free pump for long life and no maintenance. The compressor has a low amp 120V motor that starts easily in cold weather or with an extension cord. It also has a shroud, handle, and console cover that protects vital components and makes the unit easier to carry.', ' Based on the search results, here are some recommended air compressors:\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are designed for enhanced usability and serviceability, with a compact design that makes it easier to tow and maneuver. It features multiple engine options, including a reliable Caterpillar or Perkins engine, and delivers air pressures up to 200 psi.\n\nThe Porter-Cable 6 Gallon Oil-Free Pancake Compressor is a high-pressure design that optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. It has a durable oil-free pump for long life and no maintenance, and is easy to transport with its integrated cord wrap.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up, delivering a whopping 6.5 CFM @ 90 PSI. It features a foot-actuated folding handle and heavy-duty flat-free tires for easy mobility around the job site.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is designed for continuous operation and extended pump life, with durable cast-iron cylinders, heads, and frame. It features a highly efficient stainless steel finger valves that are simple, efficient, and easy to maintain.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors feature the most advanced rotary screw air compressor technology, serving as a reliable source of compressed air for a wide range of industrial applications. It has a standard quiet enclosure, 8,000 hr. premium synthetic fluid, and low oil carryover.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is equipped with Makita’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and increased compressor efficiency. It has a cast iron cylinder with greater bore and stroke for maximum performance.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor has a 225 PSI max tank storage pressure that provides a user with 80% more usable air than the industry leader. It has a 5.0 SCFM @ 90 PSI that allows the compressor to recover quickly after its initial tank charge is exhausted.', ' Based on the search results, here are some recommended air compressors:\n\nThe Makita 3.0 HP* Big Bore Air Compressor is recommended as the best overall air compressor. It delivers powerful performance, with 6.5 CFM @ 90PSI, enough to run two framing nailers. The cast iron cylinder with greater bore and stroke ensures maximum performance, while the roll cage construction provides extra protection to the pump and motor assembly. The Big Bore™ piston and cylinder are larger than those in standard compressors, resulting in increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is another excellent option. It offers 225 PSI max tank storage pressure, providing 80% more usable air than the industry leader. The 5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted. The oil-free, maintenance-free pump ensures convenient use, while the high flow coupler allows for maximum nailer performance.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up, with a motor-pump delivering a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move around the job site. The cast-iron cylinder, stainless-steel reed valves, and splash lubrication ensure longer life, while the 2.5 HP motor with overload protection and manual reset provides reliable performance.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is a more budget-friendly option. It is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance, while the integrated cord wrap makes transporting easy.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and reliable, serving as a reliable source of compressed air for a wide range of industrial applications. The QGS features advanced rotary screw air compressor technology, enabling easy maintenance and low cost of ownership. The standard quiet enclosure, 8,000 hr. premium synthetic fluid, and low oil carryover ensure high efficiency and long life.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are designed for enhanced usability and serviceability, with multiple units including the award-winning 400HH featuring air pressures up to 200 psi. The compact design allows for easier towing to and from the job site, while the improved maneuverability fits more easily in smaller spaces. The multiple engine options, including Caterpillar C4.4 (T4F) and Perkins 1204F (T4F), provide reliable performance.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders offer a low total cost of operation, with a highly durable spiral bevel gear that reduces vibration and stress of torque transmission. The 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders are designed for 7” and 9” wheels and pads. The spindle lock feature allows for quick and easy abrasive replacement, while the 360° adjustable air exhaust with integrated muffler improves operator’s comfort.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is designed for the professional, with durable cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. The oversized belt wheel provides reliable design and cooler operation, while the Ingersoll Rand synthetic lubricant provides 2,000-hour oil change intervals, four times longer than mineral-based lubricants. The high-efficiency stainless steel finger valves are simple, efficient, and easy to maintain.', ' Based on the search results, here are some recommended air compressors:\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are a top choice for a variety of jobsite applications. They are crafted for enhanced usability and serviceability, with multiple units including the award-winning 400HH featuring air pressures up to 200 psi. The compact design allows for easier towing to and from the job site and improved maneuverability. The compressors are available with your choice of a reliable Caterpillar or Perkins engine.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is another excellent option. It delivers a powerful performance with 6.5 CFM @ 90PSI, enough to run two framing nailers. The cast iron cylinder with greater bore and stroke ensures maximum performance. The compressor is also built for durability with roll cage construction for extra protection to pump and motor assembly.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and reliable, featuring advanced rotary screw air compressor technology. They are designed for 100% duty cycle and have a low cost of ownership. The compressors are equipped with a high efficiency intake filter and a True Blue 5-Year Warranty with start up.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor offers a 225 PSI max tank storage pressure, providing 80% more usable air than the industry leader. It has a 5.0 SCFM @ 90 PSI, allowing the compressor to recover quickly after its initial tank charge is exhausted. The compressor is also oil free and maintenance free, with an efficient high pressure motor that allows it to be run with an extension cord.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up, delivering a whopping 6.5 CFM @ 90 PSI. It features a motor-pump with ball bearings, cast-iron cylinder, and stainless-steel reed valves for longer life. The compressor also has a foot-actuated folding handle and heavy-duty flat-free tires for easy mobility around the job site.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is constructed with a pancake style tank for stability and has a high-pressure design that optimizes air tool performance. It delivers 2.6 SCFM at 90 psi for quick recovery time and has an oil-free pump for maintenance-free performance. The compressor is also lightweight and portable, weighing only 30 lbs.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is designed for continuous operation and extended pump life with durable cast-iron cylinders, heads, and frame. It has an oversized belt wheel for reliable design and cooler operation, and an Ingersoll Rand synthetic lubricant that provides 2,000-hour oil change intervals.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders offer a low total cost of operation with a 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications. They feature a highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.', ' Based on the search results, here are some recommended air compressors:\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is a highly recommended option. It offers a max tank storage pressure of 225 PSI, providing 80% more usable air than the industry leader. With 5.0 SCFM at 90 PSI, it allows for quick recovery after the initial tank charge is exhausted. The compressor is also designed for quiet operation with a 78 dBA operational noise level. It features an oil-free, maintenance-free pump for convenient use and a high flow coupler for maximum nailer performance.\n\nThe Makita 3.0 HP* Big Bore Air Compressor is another top choice. It delivers 6.5 CFM at 90 PSI, making it powerful enough to run two framing nailers. The cast iron cylinder with a greater bore and stroke ensures maximum performance. The roll cage construction provides extra protection to the pump and motor assembly, enhancing durability. The oil drain and oil sight glass are conveniently located for easy access and maintenance.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is a durable option with cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. It features an oversized belt wheel for reliable design and cooler operation. The Ingersoll Rand synthetic lubricant provides 2,000-hour oil change intervals, four times longer than mineral-based lubricants.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are compact and designed for enhanced usability and serviceability. They offer multiple units, including the award-winning 400HH with air pressures up to 200 psi. These compressors are available with your choice of a reliable Caterpillar or Perkins engine.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and serve as a reliable source of compressed air for a wide range of industrial applications. They feature advanced rotary screw air compressor technology and a low cost of ownership. The QGS compressors are designed for 100% duty cycle and come with a True Blue 5-Year Warranty with start up.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is a lightweight and portable option. It is constructed with a pancake style tank for stability and features a high-pressure design that delivers 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications. They feature a highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up. The motor-pump delivers a whopping 6.5 CFM at 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the VT25BIG around the job site.', ' Based on the search results, here are some recommended air compressors:\n\nThe Makita 3.0 HP* Big Bore Air Compressor is a top-of-the-line option. It delivers 6.5 CFM at 90 PSI, making it powerful enough to run two framing nailers. The cast iron cylinder with greater bore and stroke ensures maximum performance, and the roll cage construction provides extra protection to the pump and motor assembly. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke, resulting in increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nThe Rolair VT25BIG is another excellent choice. It boasts the highest air output of any direct drive air compressor in the line-up, with a motor-pump delivering a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move around the job site. The pump features ball bearings, a cast-iron cylinder, and stainless-steel reed valves and splash lubrication for longer life. The motor is heavy-duty/industrial grade with ball bearings for greater durability.\n\nThe Porter-Cable 6 Gallon Oil Free Pancake Compressor is a more budget-friendly option. It features a high-pressure design that optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance, and the integrated cord wrap makes it easy to transport. The compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is another good option. It has a 225 PSI max tank storage pressure, providing 80% more usable air than the industry leader. The 5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted. The vertical stand feature and collapsible handle allow for easy transportation and storage. The compressor is oil free and maintenance free, and the efficient high pressure motor allows it to be run with an extension cord.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are a highly efficient option for industrial applications. They feature advanced rotary screw air compressor technology and a low cost of ownership. The compressors are designed for 100% duty cycle and have a standard quiet enclosure. They come with an 8,000 hr. premium synthetic fluid and have low oil carryover.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are designed for enhanced usability and serviceability. They have multiple units, including the award-winning 400HH featuring air pressures up to 200 psi. The compressors are compact and have easy pressure change and extended runtime. They are available with your choice of a reliable Caterpillar or Perkins engine.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is a durable option with cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. The oversized belt wheel provides reliable design and cooler operation. The compressor uses Ingersoll Rand synthetic lubricant, which provides 2,000-hour oil change intervals.\n\nThe Chicago Pneumatic cp3850 series - industrial angle grinders & sanders are not air compressors, but rather grinders and sanders. They offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications. They feature a highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.', ' Based on the search results, here are some recommended air compressors:\n\nThe Makita 3.0 HP* Big Bore Air Compressor is a powerful and efficient option, delivering 6.5 CFM at 90 PSI. It is equipped with a cast iron cylinder for maximum performance and a roll cage construction for extra protection. It also includes oil and 1/4” universal quick couplers.\n\nThe Rolair VT25BIG is another high-performance air compressor, boasting the highest air output of any direct drive air compressor in its line-up. It delivers a whopping 6.5 CFM at 90 PSI and features a foot-actuated folding handle and heavy-duty flat-free tires for easy mobility.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is a compact and portable option with a maximum tank storage pressure of 225 PSI. It has a 5.0 SCFM at 90 PSI and a vertical stand feature and collapsible handle for easy storage and transportation.\n\nThe Porter-Cable 6 Gallon Oil-Free Pancake Compressor is a stable and durable option with a pancake style tank and tough rubber feet. It has a high-pressure design that delivers 2.6 SCFM at 90 PSI for quick recovery time and an oil-free pump for maintenance-free performance.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are compact and easy to maneuver, with multiple units available including the award-winning 400HH with air pressures up to 200 psi. They are available with a reliable Caterpillar or Perkins engine.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and reliable, with advanced rotary screw air compressor technology. They are designed for 100% duty cycle and have a long life V-belt drive.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is a durable and reliable option with cast-iron cylinders, heads, and frame designed for continuous operation and extended pump life. It has an oversized belt wheel for reliable design and cooler operation.\n\nThe Chicago Pneumatic CP3850 series grinders and sanders are not air compressors, but rather industrial governed angle grinders and sanders. They offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.', ' Based on the search results, here are some recommended air compressors:\n\nThe Makita 3.0 HP* Big Bore Air Compressor is recommended as the best overall air compressor. It delivers powerful performance with 6.5 CFM at 90PSI, enough to run two framing nailers. The cast iron cylinder with greater bore and stroke ensures maximum performance, while the roll cage construction provides extra protection to the pump and motor assembly. It also features an oil drain and oil sight glass for easy access and maintenance.\n\nThe Sullair 375 Series T4F Portable Diesel Compressors are recommended for their enhanced usability and serviceability. They offer multiple units with air pressures up to 200 psi, and are available with your choice of a reliable Caterpillar or Perkins engine. The compact design allows for easier towing to and from the job site, improved maneuverability, and more convenient storage.\n\nThe Rolair VT25BIG boasts the highest air output of any direct drive air compressor in its line-up, with a motor-pump delivering a whopping 6.5 CFM at 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move around the job site. The pump features a cast-iron cylinder, stainless-steel reed valves, and splash lubrication for longer life.\n\nThe Ingersoll Rand SS5L5 Single Stage Air Compressor is designed for the professional, with durable cast-iron cylinders, heads, and frame for continuous operation and extended pump life. The oversized belt wheel provides reliable design and cooler operation, while the Ingersoll Rand synthetic lubricant provides 2,000-hour oil change intervals.\n\nThe DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor offers 80% more usable air than the industry leader, with a 5.0 SCFM at 90 PSI for quick recovery after its initial tank charge is exhausted. The vertical stand feature and collapsible handle allow for easy transportation and storage, while the efficient high pressure motor allows the compressor to be run with an extension cord.\n\nThe Porter-Cable 6 Gallon Oil-Free Pancake Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance, while the low amp 120V motor starts easily in cold weather or with extension cord.\n\nThe Chicago Pneumatic cp3850 series of industrial angle grinders and sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications. They feature a highly durable spiral bevel gear that reduces vibration and stress of torque transmission, a spindle lock feature for quick and easy abrasive replacement, and a 360° adjustable air exhaust with integrated muffler.\n\nThe Quincy Compressors QGS 5-100 hp Belt Drive Compressors are highly efficient and feature advanced rotary screw air compressor technology. They serve as a reliable source of compressed air for a wide range of industrial applications, with a standard quiet enclosure, 8,000 hr. premium synthetic fluid, low oil carryover, and designed for 100% duty cycle.']