[['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'CRAFTSMAN® CMHT65043 Plumber Wrench Faucet Tool is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. The CMHT65043 is a set to be marveled. Limited Lifetime Warranty.', 'Torque screwdrivers by Craftsman allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Craftsman are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Craftsman are just the right tool, also for your requirements!\n\nThe tools\n\nCMHT65043 adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nCMHT65043 ESD adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nCMHT65043 ESD adjustable torque screwdrivers (0.1-1.0 Nm)\n\nCMHT65043 ESD Torque screwdrivers, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nCMHT65043 pistol handle, adjustable torque screwdrivers (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nCMHT65043 VDE', "The CMHT65043 (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Craftsman brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the CMHT65043 can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Craftsman’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Craftsman 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe Craftsman CMHT65043 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nCMHT65043 battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Craftsman CMHT65043 Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nCraftsman CMHT65043 Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The CRAFTSMAN CMHT65043 shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'RIDGID® EZ Change Plumber Wrench Faucet Tool is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece EZ Change Faucet Tool are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. Limited Lifetime Warranty.', 'Torque screwdrivers by Ridgid allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Ridgid are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Ridgid are just the right tool, also for your requirements!\n\nThe tools\n\nEZ Change Faucet Tool adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nEZ Change Faucet Tool ESD adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nEZ Change Faucet Tool ESD adjustable torque screwdrivers (0.1-1.0 Nm)\n\nEZ Change Faucet Tool, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nEZ Change Faucet Tool pistol handle, adjustable torque screwdrivers (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nEZ Change Faucet Tool VDE', "The EZ Change Faucet Tool (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Ridgid brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the EZ Change Faucet Tool can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Ridgid’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Ridgid 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe RCF680N1 EZ Change Faucet Tool 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nRidgid battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Ridgid Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nRidgid Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The RIDGID EZ Change Faucet Tool shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)\n\nThis product is part of the STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips.', 'STANLEY® STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. Limited Lifetime Warranty.', 'Torque screwdrivers by Stanley allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Stanley are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Stanley are just the right tool, also for your requirements!\n\nThe tools\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips ESD (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips ESD (0.1-1.0 Nm)\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips ESD, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips pistol handle, adjustable (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nSTANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips VDE', "The STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Stanley brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Stanley’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Stanley 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe SCF680N1 STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nSTANLEY FATMAX battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Stanley Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nStanley Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The STANLEY STANLEY FATMAX Simulated Diamond Tip 6 Pc Screwdriver Set with Standard & Phillips shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'Wera series 7400 kraftform torque screwdrivers is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. The series 7400 kraftform torque screwdrivers are backed by a Limited Lifetime Warranty.', 'Torque screwdrivers by Wera allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Wera are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Wera are just the right tool, also for your requirements!\n\nThe tools\n\nSeries 7400 Kraftform adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nSeries 7400 ESD Kraftform adjustable torque screwdrivers (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nSeries 7400 ESD Kraftform adjustable torque screwdrivers (0.1-1.0 Nm)\n\n7400 ESD series Kraftform Torque screwdrivers, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nSeries 7400 Kraftform pistol handle, adjustable torque screwdrivers (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nSeries 7400 VDE', "The series 7400 kraftform torque screwdrivers (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Wera brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the series 7400 kraftform torque screwdrivers can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Wera’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Wera 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe Wera DCF680N1 series 7400 kraftform torque screwdrivers 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nseries 7400 kraftform torque screwdrivers battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Wera Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nWera Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The Wera series 7400 kraftform torque screwdriver shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'MAKITA® 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. Limited Lifetime Warranty.', 'Torque screwdrivers by Makita allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Makita are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Makita are just the right tool, also for your requirements!\n\nThe tools\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only ESD (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only ESD (0.1-1.0 Nm)\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only ESD series, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only pistol handle, adjustable (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\n18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only VDE', "The 18V LXT® Lithium-Ion Cordless Drywall Screwdriver (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Makita brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the 18V Drywall Screwdriver can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Makita’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Makita 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe Makita 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\n18V LXT Lithium_Ion battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Makita 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nMakita 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The MAKITA 18V LXT Lithium_Ion Brushless Cordless 4,000 RPM Drywall Screwdriver, Tool Only shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'DeWalt® 8V MAX Gyroscopic Screwdriver is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. The 8V MAX Gyroscopic Screwdriver is a set to be marveled. Limited Lifetime Warranty.', 'Torque screwdrivers by DeWalt allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by DeWalt are available with adjustable as well as pre-set torque.\nTorque screwdrivers by DeWalt are just the right tool, also for your requirements!\n\nThe tools\n\n8V MAX Gyroscopic Screwdriver (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\n8V MAX Gyroscopic Screwdriver ESD (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\n8V MAX Gyroscopic Screwdriver ESD (0.1-1.0 Nm)\n\n8V MAX Gyroscopic Screwdriver ESD, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\n8V MAX Gyroscopic Screwdriver pistol handle, adjustable (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\n8V MAX Gyroscopic Screwdriver VDE', "The 8V MAX Gyroscopic Screwdriver (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a DeWalt brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the 8V MAX Gyroscopic Screwdriver can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of DeWalt’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. DeWalt 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe DCF680N1 8V MAX* Gyroscopic Screwdriver 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\n8V MAX battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'DeWalt 8V MAX Gyroscopic Screwdriver Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nDeWalt 8V MAX Gyroscopic Screwdriver Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The DeWalt 8V MAX Gyroscopic Screwdriver shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'BOSCH® Go 3.6V Smart Screwdriver is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. The Go 3.6V Smart Screwdriver is a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. Limited Lifetime Warranty.', 'Torque screwdrivers by Bosch allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Bosch are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Bosch are just the right tool, also for your requirements!\n\nThe tools\n\nGo 3.6V Smart Screwdriver (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nGo 3.6V Smart Screwdriver ESD (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nGo 3.6V Smart Screwdriver ESD (0.1-1.0 Nm)\n\nGo 3.6V Smart Screwdriver ESD, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nGo 3.6V Smart Screwdriver pistol handle, adjustable (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nGo 3.6V Smart Screwdriver VDE', "The Go 3.6V Smart Screwdriver (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Bosch brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the Go 3.6V Smart Screwdriver can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Bosch’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Bosch 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe Bosch DCF680N1 Go 3.6V Smart Screwdriver 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nGo 3.6V battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Bosch GO Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nBosch GO Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The BOSCH Go 3.6V Smart Screwdriver shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.'], ['6 pc. Jewelers screwdriver set features heat-treated, alloy steel blades for increased durability. A comfort optimized handle is ideal for high and low torque applications. Blades and shafts are coated with a satin-nickel finish to resist corrosion.\n\nSTRENGTH AND DURABILITY: Made of heat-treated alloy steel \n COMFORT OPTIMIZED HANDLE: For high and low torque application \n Satin-nickel finish\n\nBattery Included: No\nCordless or Corded: Cordless\nIndividual or Set: SET\nProduct Material: Steel\nMeasurement Standard: SAE\nNumber of Batteries included: 0\nNumber of Pieces: 6\nPower Source: NON-ENERGY USING\nProduct Height: 1.0 IN\nProduct Length: 7.3 IN\nProduct Weight: 0.3 LB\nProduct Width: 5.8 IN\nWarranty: Full Lifetime Warranty\nIncludes: (3) Sl 1/16-In. X 1.75-In. (1), Sl 5/64-In. X 2-In. (1), Sl 3/32 X 2.25-In. (1). (3) Ph #0000 X 1.75-In. (1), Ph #000 X 2-In. (1), Ph #00 X 2.25-In. (1)', 'MEGAPRO® Automotive Ratcheting 13-in-1 Screwdriver is the one tool for common faucet installations and sink strainers. Quickly and easily install new fixtures with certainty. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces. Unique cubed insert provides a variety of common nut sizes. Ideal for most common 2, 3, 4, and 6 tab mounting nuts. Wrench for tight shut-off valves. Retainer for 3 or 4 slot strainer baskets. 5/8" deep welled socket for many single hole mountings. Short body for clearance in tight spaces.', 'The 6-piece simulated Diamond Screwdrivers are a set to be marveled. With Industrial Grade simulated diamond technology on the tip they help with a longer tip life. The black phosphate bars provide corrosion resistance. For on the job easy identification you can rely on our color coded handles. Color coded for easy tip identification. Includes (3) Standard Edges 1PT X 3" 2PT X 4" 3PT X 6" and (3) Phillips Head 3/16" X 4" 1/4" X 4" 5/16" X 6". Tip Type: Phillips. Limited Lifetime Warranty.', 'Torque screwdrivers by Megapro allow variable torque settings with the very highest degree of precision.  Measuring accuracy: ± 6 % as per the EN ISO 6789 standard. Distinct acoustic and noticeable excess-load signal when the pre-set torque is reached. Unlimited torque for loosening seized screws. Torque screwdrivers by Megapro are available with adjustable as well as pre-set torque.\nTorque screwdrivers by Megapro are just the right tool, also for your requirements!\n\nThe tools\n\nAutomotive Ratcheting 13-in-1 Screwdriver (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nAutomotive Ratcheting 13-in-1 Screwdriver ESD (0.1-3.0 Nm) with Rapidaptor quick-release chuck\n\nAutomotive Ratcheting 13-in-1 Screwdriver ESD (0.1-1.0 Nm)\n\nAutomotive Ratcheting 13-in-1 Screwdriver ESD series, with factory pre-set value (0.1-1.0 Nm) and quick-release chuck\n\nAutomotive Ratcheting 13-in-1 Screwdriver pistol handle, adjustable (3.0-8.8 Nm) with Rapidaptor quick-release chuck\n\nAutomotive Ratcheting 13-in-1 Screwdriver VDE', "The Automotive Ratcheting 13-in-1 Screwdriver (model XSF03Z, tool only, batteries and charger sold separately) breaks new ground for drywall contractors. It's powered by a Megapro brushless motor for longer run time, increased power and speed, and longer tool life. With the exclusive Push Drive™ Technology, the Automotive Ratcheting 13-in-1 Screwdriver can be set on lock-on mode so the motor starts only when the fastener is engaged. This gives contractors a quieter work environment, and also saves on battery power. It’s built for added durability with Extreme Protection Technology (XPT™), which is engineered for improved dust and water resistance for operation in harsh job site conditions. It is ideal for hanging sheetrock, metal framing, installing subfloors, backer board, and decking applications.\nIt’s part of Megapro’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Megapro 18V Lithium-Ion batteries have the fastest cha", 'Motion activation variable speed and reversing control for precise fastening control\nMotion activated variable speed 0-430 rpm for fastening into wood, plastic, and light-gauge metal\nAdjustable two-position handle allows for operation in either in-line or pistol-grip\nThe MCF680N1 Automotive Ratcheting 13-in-1 Screwdriver 1 Battery Kit is ideal for achieving precision, speed, and control. Adjustable two-position handle allows for operation in either in-line or pistol-grip to suit the professional\'s needs.\nAllows control when completing light fastening applications\nLED provides illumination in confined areas without shadowing\nBattery charge status on tool notifies when to charge packs\n1/4" hex allows for quick screwdriver bit change and holds 1" bit tips\nAutomotive Ratcheting 13-in-1 Screwdriver battery pack allows for longer run-time and charges in one hour\n#8x1 5/8" Drywall Screw into 2" x 4" SPF\n#8 & #6 Machine screw insertion and removal\n#6 & #8 Cabinet hardware screws\nElectrical switch and outlet wall plate screws\nIdeal tool fo', 'Megapro Professional\n\nCordless Screwdriver\n\nMinimum Effort, Maximum Efficiency\n\nEasy to control – tool stops immediately after deactivation via electronic brake\n\nDual-activation mode – simply push tool or press button to begin\n\nMechanical clutch with 5 torque settings and maximum performance mode\n\nSee technical details\n\nFunctions & key features\n\nYour Selection\n\nin carrying case\n\nShow variant\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nCheck availability on location\n\nFind a local dealer\n\nYour Selected Variant\n\nYour Selected Variant\n\nin carrying case\n\n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nMegapro Professional\n\nYour Selection\n\nin carrying case\n\nOrder number: \n0 601 9H2 100\n\n23.00 OMR\n\nRecommended retail price excluding VAT\n\nFind a local dealer\n\nIncluded in this variant\n\nMicro USB cable\n\nOrder number: 1 607 000 CG9\n\n1 x screwdriver bit PH2\n\nOrder number: 2 608 521 M11\n\nCardboard box\n\nCarrying case\n\n1 x screwdriver bit PH1\n\nOrder nu', 'The MEGAPRO 13-in-1 automotive ratcheting screwdriver shaft is made from Stainless Steel 303 and includes 6 sizes of star screwdriver bits. This magnetic screwdriver drive fasteners easier and faster with its precision 28-tooth ratchet design and rubberized cushion grip handle.\n\nLoaded with 12-one inch insert bits made from S2 industrial grade steel, this assortment of bit types and sizes provides the most suitable tips for driving automotive screws. The shaft opening serves as a 1/4″ hex driver. This is simply the right tool for difficult spaces and angles.']]