[['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. Random Orbit Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n 382 5 Random Orbit Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", '382 5 Random Orbit Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The 5” Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The Random Orbit Sander powered by battery technology delivers up to 35 minutes of run-time on a 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) 382 5 Random Orbit Sander\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The Porter-Cable MOUSE 20V MAX cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX lithium ion battery.\n\nStart strong, finish strong. With the Porter-Cable MOUSE 20V MAX cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'PORTER-CABLE introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the PORTER-CABLE 3-Year Manufacturer\'s Warranty, the 382 5 Random Orbit Sander includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The 382 5 Random Orbit Sander has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the Porter-Cable dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the Porter-Cable dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use Porter-Cable Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) 382 5 Random Orbit Sander\n(1) Dust Bag\n(1) Carrying Bag', '382 5 Random Orbit Sander\n\nSanders\n\n382 5 Random Orbit Sander\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nPorter-Cable’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. SR211601 Random Orbit Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) SKIL SR211601 Random Orbit Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n Random Orbital Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", 'SR211601 Random Orbit Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The SR211601 5” Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The SR211601 Random Orbit Sander powered by REDLITHIUM™ battery technology delivers up to 35 minutes of run-time on a SKIL 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) SR211601 Random Orbit Sander\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the SKIL System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The SKIL MOUSE 20V MAX cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX lithium ion battery.\n\nStart strong, finish strong. With the SKIL MOUSE 20V MAX cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'SKIL introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the SKIL 3-Year Manufacturer\'s Warranty, the SR211601 Random Orbit Sander includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The SR211601 Random Orbit Sander Kit with hook & loop pad has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the SKILV010 or SKILV012 dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the SKILV010 or SKILV012 dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use SKILV9000 Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) SR211601 Sander\n(1) Dust Bag\n(1) Carrying Bag', 'SR211601 Professional\n\nSanders\n\nSR211601 Professional\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nSKIL’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. FSX 200 Intec. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) FSX 200 Intec\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n FSX 200 Intec, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", 'FSX 200 Intec (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The FSX 200 Intec delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The FSX 200 Intec powered by REDLITHIUM™ battery technology delivers up to 35 minutes of run-time on a Metabo 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) FSX 200 Intec\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the Metabo System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The Metabo MOUSE 20V MAX cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX lithium ion battery.\n\nStart strong, finish strong. With the Metabo MOUSE 20V MAX cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'METABO introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the METABO 3-Year Manufacturer\'s Warranty, the FSX 200 Intec includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The FSX 200 Intec has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the MV010 or MV012 dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the MV010 or MV012 dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use MV9000 Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) FSX 200 Intec Sander\n(1) Dust Bag\n(1) Carrying Bag', 'FSX 200 Intec\n\nSanders\n\nFSX 200 Intec\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nMetabo’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. 2648-20 M18 5 Random Orbit Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) 2648-20 M18 5 Random Orbit Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n 2648-20 M18 5 Random Orbit Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", '2648-20 M18 5 Random Orbit Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The M18™ 5” Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The M18™ Random Orbit Sander powered by REDLITHIUM™ battery technology delivers up to 35 minutes of run-time on a M18™ 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) M18™ Random Orbit Sander (2648-20)\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the M18 System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The Milwaukee MOUSE 20V MAX* cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX* lithium ion battery.\n\nStart strong, finish strong. With the Milwaukee MOUSE 20V MAX* cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'MILWAUKEE introduces the all new 18V 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new 2648-20 M18 5 Random Orbit Sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the MILWAUKEE 3-Year Manufacturer\'s Warranty, the 2648-20 M18 5 Random Orbit Sander includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The 2648-20 M18 5 Random Orbit Sander has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the Milwaukee dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the Milwaukee dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use Milwaukee Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) 2648-20 M18 5 Random Orbit Sander\n(1) Dust Bag\n(1) Carrying Bag', '2648-20 M18 5 Random Orbit Sander\n\nSanders\n\n2648-20 M18 5 Random Orbit Sander\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nMilwaukee’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance BDCMS20C 20V MAX Lithium Ion Mouse Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) BDCMS20C 20V MAX Lithium Ion Mouse Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n BDCMS20C 20V MAX Lithium Ion Mouse Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", 'BDCMS20C 20V MAX Lithium Ion Mouse Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The 5” Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The Random Orbit Sander powered by Lithium Ion battery technology delivers up to 35 minutes of run-time on a 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) BDCMS20C 20V MAX Lithium Ion Mouse Sander\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the BLACKDECKER System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The BLACK+DECKER® MOUSE® 20V MAX* cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX* lithium ion battery.\n\nStart strong, finish strong. With the BLACK+DECKER® MOUSE™ 20V MAX* cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', "BLACKDECKER introduces the all new 20V MAX BDCMS20C Lithium Ion Mouse Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new BDCMS20C sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the BLACKDECKER 3-Year Manufacturer's Warranty, the 20V MAX BDCMS20C Lithium Ion Mouse Sander includes an assortment of sandpaper and an operator's manual. Battery and charger sold separately.", 'The BDCMS20C 20V MAX Lithium Ion Mouse Sander has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the BLACKDECKER dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the BLACKDECKER dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use BLACKDECKER Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) BDCMS20C Sander\n(1) Dust Bag\n(1) Carrying Bag', 'BDCMS20C 20V MAX Lithium Ion Mouse Sander\n\nSanders\n\nBDCMS20C 20V MAX Lithium Ion Mouse Sander\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nBLACKDECKER’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. P411 ONE 18V Random Orbit Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) Ryobi P411 ONE 18V Random Orbit Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n P411 ONE 18V Random Orbit Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", 'P411 ONE 18V Random Orbit Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The ONE 18V 5” Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The ONE 18V Random Orbit Sander powered by Ryobi battery technology delivers up to 35 minutes of run-time on a Ryobi 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) P411 ONE 18V Random Orbit Sander\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the Ryobi System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The Ryobi MOUSE 18V cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 18V lithium ion battery.\n\nStart strong, finish strong. With the Ryobi MOUSE 18V cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'RYOBI introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the RYOBI 3-Year Manufacturer\'s Warranty, the 18V ONE+ 5" Random Orbit Sander includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold\xa0separately.', 'The Ryobi P411 ONE 18V Random Orbit Sander has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the Ryobi dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the Ryobi dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use Ryobi Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) Ryobi P411 ONE 18V Random Orbit Sander\n(1) Dust Bag\n(1) Carrying Bag', 'P411 ONE 18V Random Orbit Sander\n\nSanders\n\nP411 ONE 18V Random Orbit Sander\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nRyobi’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", '5 in. Variable Speed Random Orbit Sander Kit - H&L Pad (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad powered by REDLITHIUM™ battery technology delivers up to 35 minutes of run-time on a DeWalt 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the DeWalt System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The DeWalt MOUSE 20V MAX cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX lithium ion battery.\n\nStart strong, finish strong. With the DeWalt MOUSE cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'DeWalt introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the DeWalt 3-Year Manufacturer\'s Warranty, the 5 in. Variable Speed Random Orbit Sander Kit - H&L Pad includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The DWE6423 5 in. Variable Speed Random Orbit Sander Kit with hook & loop pad has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the DWV010 or DWV012 dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the DWV010 or DWV012 dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use DWV9000 Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) DWE6423 Sander\n(1) Dust Bag\n(1) Carrying Bag', '5 in. Variable Speed Random Orbit Sander Kit - H&L Pad\n\nSanders\n\n5 in. Variable Speed Random Orbit Sander Kit - H&L Pad\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nDeWalt’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round'], ['HIGH-OUTPUT FOR PRO-GRADE RESULTS: Provides maximum sanding speed for smooth finishes\nEASY OPERATION AND MINIMAL SCRAPING: Controlled Finishing System maintains controllable pad speed and minimizes gouging during start-up\nREDUCES USER FATIGUE with dual-plane, counter-balanced fan\nView more features\n\nProduct Overview\nTake on demanding jobs with this high-performance 5 in. ROS20VSC PROFESSIONAL Random Orbit Sander. Get smooth, expert-level finishes with this sander’s controlled finishing system that delivers easy operability and less gouging during start-up. Cut user fatigue with its dual-plane fan and tackle routine tasks with the confidence and protection provided by a dust-sealed switch that defends against dust ingestion for longer life.\n\nAdditional Features\nPROTECTS AGAINST DUST INGESTION: Dust-sealed switch keeps harmful particles out for long tool life\nHIGH-ENDURANCE CONSTRUCTION: Sealed 100% ball-bearing\nSPECIALIZED COMPATIBILITY: Accepts 5 in., 8-hole hook-and-loop paper\n\nIncludes\n(1) ROS20VSC PROFESSIONAL Random Orbit Sander\n(1) Oper', "Fine Finish without Mess.\n\nThis nimble, variable-speed sander has the power and sophistication to deliver fine, swirl-free finishes all while collecting the dust to cut down on mess. It’s ideal for sanding applications on wood, metal and plastic. More About This Product: - 7000-13, 000 OPM- Variable Speed Dial- X-Flow Dust Collection- Vibration Control- Easy to change attachments and sanding sheets.\n\nWhat's Included:\n ROS20VSC PROFESSIONAL Random Orbit Sander, 1pc Dust Box, 3pcs Sanding Sheet\n\nFeatures \n\nPowerful – With a 2.8 amp motor and 13,000 orbits per minute, it’s able to deliver a smooth performance over a variety of sanding applications.\n\nEasy to clean dust container – The x-flow dust collector uses cyclone force to collect dust in it’s easy-to-empty transparent container.\n\nSpeed Control – Variable speed control provides the right amount of power and control across different materials.\n\nLow vibration – Through its ergonomic design and a soft rubber grip, your hand stays comfortable while counterwe", 'ROS20VSC PROFESSIONAL Random Orbit Sander (609225190) Random orbital sander \n\n(220-240 V / 50 Hz); Cardboard box\n\nOrder no.: 609225190\n\nEAN: 4007430161864 \n\nDiameter of backing pad:\n\n125 mm / 5 " \n\nRated input power:\n\n240 W\n\nNo-load speed:\n\n11000 rpm\n\nOrbit diameter:\n\n2.7 mm / 1/8 " \n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\n\nAccessories Detail\n\nLight and handy machine for convenient one-hand operation\nVery good weight/performance ratio for low-fatigue working\nGrip area with non-slip soft-grip surface\nDust-proof ball bearings for long service life of the machine\nDust collector cartridge with filter for working without connecting to a vacuum cleaner\nExtraction possibility by means of connecting to an all-purpose vacuum cleaner via an adapter (accessory)\n\nThe machine shown may differ in equipm', 'The ROS20VSC PROFESSIONAL Random Orbit Sander delivers corded power with 12,000 Max OPM output. The 7,000-12,000 variable speed dial allows the user more control over the output of the tool to match the orbit speed for the application. The tool’s powerful motor allows the user to remove more material per battery charge. The ROS20VSC PROFESSIONAL Random Orbit Sander powered by battery technology delivers up to 35 minutes of run-time on a 3.0Ah Battery Pack (Battery Sold Separately).\n\nIncludes\n\n(1) ROS20VSC PROFESSIONAL Random Orbit Sander\n(1) Dust Canister\n(1) Universal Hose Adapter\n(1) Extension Adapter\n(2) 80 Grit Sandpaper\n\nKey Features\n- 12,000 OPM Max\n- More Material Removed Per Charge\n- Variable Speed Control\n- 5" Sanding Pad\n- 7,000-12,000 OPM Variable Speed\n- 3/32" Orbit Diameter\n- Universal Hose Adapter Included\n- Dust Canister with Filter\n- Part of the Bosch System of 150+ Tools\n\nProduct Specifications\n- Power Source: Cordless\n- Length: 10.50\n- Weight: 2lbs\n- Height: 5.74\n- Width: 4.92\n- Battery Sys', 'The Bosch MOUSE 20V MAX cordless sheet sander removes material at 12,000 OPM (orbits per minute) and has a finger attachment to sand hard-to-reach surfaces. It has a 2-position grip and a hook-and-loop system to change the sandpaper quickly. The on-board dust bag can be detached and emptied. The sander is powered by a rechargeable 20V MAX lithium ion battery.\n\nStart strong, finish strong. With the Bosch MOUSE cordless sheet sander, you’ll give every passion project and home DIY task the beautiful, refined finish they deserve. This power sander removes material at 12,000 opm, while a detail finger attachment even lets you sand hard-to-reach surfaces. Compact and ergonomic, it’s designed with a 2-position grip that enhances your control and stability, and reduces muscle fatigue. A handy hook-and-loop system allows you to change the sandpaper quickly, and the on-board dust bag can be detached and emptied in seconds, making cleanup a breeze. For cordless conven', 'BOSCH introduces the all new 18V ONE+ 5" Random Orbit Sander.  With a fast 10,000 orbits per minute (OPM) this sander will provide a swirl-free finish to each new project. This all new ONE+ sander delivers optimized control and comfort while sanding with 40% reduced vibration vs the previous model.  Quickly and easily change sandpaper with the easy hook and loop sanding pad base.  Backed by the BOSCH 3-Year Manufacturer\'s Warranty, the ROS20VSC PROFESSIONAL Random Orbit Sander includes an assortment of sandpaper and an operator\'s manual. Battery and charger sold separately.', 'The Bosch ROS20VSC PROFESSIONAL Random Orbit Sander has a 3 amp motor that delivers between 8,000 to 12,000 OPM. The separate counterweight reduces vibration and along with the rubber overmold grip provides comfortable sanding. A shorter design allows users to get closer to the work surface and the one-handed locking dust bag attaches securely to the sander to aid in dust collection or the user can attach the sander directly to the Bosch dust collectors.\n\nRubber over-mold in all of the critical areas of the sander\nImproved dust-sealed switch to protect against dust ingestion for longer switch life\nImproved dust collection and one-handed locking dust bag\nDust port is designed to fit directly to the Bosch dust collectors\nTo attach dust port to other vacuum systems with 1-1/4 in. hoses, use Bosch Universal Quick Connector\n\nApplications\n\nSanding Wood\nSanding Metal\nSanding Plastics\n\nIncludes\n\n(1) Bosch ROS20VSC PROFESSIONAL Random Orbit Sander\n(1) Dust Bag\n(1) Carrying Bag', 'ROS20VSC Professional\n\nSanders\n\nROS20VSC Professional\n\nSanders\n\n5 In. Palm Random Orbit Sander/Polisher\n\nIntegral pad dampening brake system helps prevent swirl marks\n\nBosch’s hook-and-loop disc attachment delivers secure fit\n\nMicrocellular backing pad for smooth, fine finishes\n\nVariable-speed control to match speed to workpiece and task\n\nAdjustable from between 7,500 and 12,000 OPM\n\nOptimal on-board system for filtering fine dust\n\nSoft-grip top and body\n\nLow-vibration operation\n\nSanding disc, vacuum hose adapter and carrying bag\n\nHook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks\n\nTechnical data\n\nThe most important data\n\nAmperage\n\n2.5 \n\nCase Type\n\nBag \n\nDisc Size\n\n5" \n\nDust Collection\n\nYes \n\nEccentric Offset\n\n3/64” (1.2 mm) \n\nHeight in\n\n6 "\n\nLength in\n\n9 "\n\nNo Load OPM\n\n7,500-12,000 \n\nOrbit Diameter\n\n3/32" (2.5 mm) \n\nOrbit Radius\n\n3/64" (1.25 mm) \n\nPad Size\n\n5" \n\nPaper Size / Type\n\n5" Round ']]