['225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for ', "Our 150 psi 6-Gallon Oil-Free Pancake Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", '400HH\nDESIGNED TO GET THE JOB DONE\n\nSullair 375 Series portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the 375 compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Sullair sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n375 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres', 'QGS 5-100 hp Belt Drive Compressors\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Quincy QGS can meet your needs. Featuring the most advanced rotary screw air compressor technology, the QGS serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of QGS ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the QGS Air Compressor\n\nOur QGS compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'The VT25BIG boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the VT25BIG around the job site. \n\nABOUT THE PUMP\nROLAIR Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'SS5L5 Single Stage Air Compressor \n\nPart Number:\nSS5L5\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nSS5L5\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nIngersoll Rand synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', 'MAC5200\n\n3.0 HP* Big Bore™ Air Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nMakita’s 3.0 HP Air Compressor is equipped with Makita’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i']