[["Our 150 psi 6-Gallon Oil-Free Pancake Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The 6 Gallon Oil Free Pancake Compressor boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the 6 Gallon Oil Free Pancake Compressor around the job site. \n\nABOUT THE PUMP\nPORTER-CABLE Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'MAC5200\n\n6 Gallon Oil Free Pancake Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nPorter-Cable’s 6 Gallon Oil Free Pancake Compressor is equipped with Porter-Cable’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the 6 Gallon Oil Free Pancake Compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the 6 Gallon Oil Free Pancake Compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the 6 Gallon Oil Free Pancake Compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The 6 Gallon Oil Free Pancake Compressor offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed 6 Gallon Oil Free Pancake Compressor designed for 7” and 9” wheels and pads.\n\nOur 6 Gallon Oil Free Pancake Compressor feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', '6 Gallon Oil Free Pancake Compressor\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Porter-Cable 6 Gallon Oil Free Pancake Compressor can meet your needs. Featuring the most advanced rotary screw air compressor technology, the 6 Gallon Oil Free Pancake Compressor serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of 6 Gallon Oil Free Pancake Compressor ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the 6 Gallon Oil Free Pancake Compressor Air Compressor\n\nOur 6 Gallon Oil Free Pancake Compressor compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', '6 Gallon Oil Free Pancake Compressor \n\nPart Number:\n6 Gallon Oil Free Pancake\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \n6 Gallon Oil Free Pancake\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nPorter-Cable synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nPorter-Cable 6 Gallon Oil Free Pancake Compressor are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the 6 Gallon Oil Free Pancake Compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Porter-Cable sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n6 Gallon Oil Free Pancake Compressor – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi VT25BIG is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our Rolair products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The VT25BIG boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the VT25BIG around the job site. \n\nABOUT THE PUMP\nROLAIR Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'VT25BIG\n\n3.0 HP* Big Bore™ Air Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nRolair’s VT25BIG is equipped with Rolair’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the VT25BIG to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The VT25BIG grinders and sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur VT25BIG angle grinders and sanders feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'VT25BIG\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Rolair VT25BIG can meet your needs. Featuring the most advanced rotary screw air compressor technology, the VT25BIG serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of VT25BIG ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the VT25BIG Air Compressor\n\nOur VT25BIG compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'VT25BIG \n\nPart Number:\nVT25BIG\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nVT25BIG\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nRolair synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nRolair VT25BIG portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the VT25BIG compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Rolair sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\nVT25BIG – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi Makita 3.0 HP* Big Bore Air Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The Makita 3.0 HP* Big Bore Air Compressor boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the Makita 3.0 HP* Big Bore Air Compressor around the job site. \n\nABOUT THE PUMP\nMAKITA Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'MAC5200\n\n3.0 HP* Big Bore™ Air Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nMakita’s 3.0 HP Air Compressor is equipped with Makita’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the Makita 3.0 HP* Big Bore Air Compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the Makita 3.0 HP* Big Bore Air Compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the Makita 3.0 HP* Big Bore Air Compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The Makita 3.0 HP* Big Bore Air Compressor offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur Makita 3.0 HP* Big Bore Air Compressor feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'Makita 3.0 HP* Big Bore Air Compressor\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Makita can meet your needs. Featuring the most advanced rotary screw air compressor technology, the Makita 3.0 HP* Big Bore Air Compressor serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of Makita ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the Makita 3.0 HP* Big Bore Air Compressor\n\nOur Makita 3.0 HP* Big Bore Air Compressor feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'Makita 3.0 HP* Big Bore Air Compressor \n\nPart Number:\nMakita 3.0 HP* Big Bore\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nMakita 3.0 HP* Big Bore\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nMakita synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nMakita 3.0 HP* Big Bore Air Compressor portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the Makita 3.0 HP* Big Bore Air Compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Makita sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\nMakita 3.0 HP* Big Bore Air Compressor – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 225 psi DeWalt 1.6 HP Continuous, 4.5 Gallon Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our DeWalt products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor around the job site. \n\nABOUT THE PUMP\nDeWalt Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'MAC5200\n\n1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nDeWalt’s 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor is equipped with DeWalt’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for ', 'The DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor\n\nIf you’re looking for a highly efficient compressor, the DeWalt can meet your needs. Featuring the most advanced rotary screw air compressor technology, the DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of DeWalt ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor Air Compressor\n\nOur DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor\n\nPart Number:\nDeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nDeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nDeWalt synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nDeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your DeWalt sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n375 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi cp3850 series - industrial angle grinders & sanders is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our Chicago Pneumatic products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The cp3850 series - industrial angle grinders & sanders boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the cp3850 series - industrial angle grinders & sanders around the job site. \n\nABOUT THE PUMP\nCHICAGO PNEUMATIC Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'CP5200\n\ncp3850 series - industrial angle grinders & sanders\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nChicago Pneumatic’s cp3850 series - industrial angle grinders & sanders is equipped with Chicago Pneumatic’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the cp3850 series - industrial angle grinders & sanders in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the cp3850 series - industrial angle grinders & sanders to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The CP3850 series grinders and sanders offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur CP3850 angle grinders and sanders feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'cp3850 series - industrial angle grinders & sanders\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Chicago Pneumatic cp3850 series can meet your needs. Featuring the most advanced rotary screw air compressor technology, the cp3850 series serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of cp3850 series ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the cp3850 series - industrial angle grinders & sanders Air Compressor\n\nOur cp3850 series - industrial angle grinders & sanders feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'cp3850 series - industrial angle grinders & sanders \n\nPart Number:\ncp3850\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \ncp3850\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nChicago Pneumatic synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, cp3850 series - industrial angle grinders & sanders are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nChicago Pneumatic cp3850 series - industrial angle grinders & sanders are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the cp3850 series - industrial angle grinders & sanders family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Chicago Pneumatic sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n375 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi QGS 5-100 hp Belt Drive Compressors is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our Quincy Compressors products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The QGS 5-100 hp Belt Drive Compressors boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the QGS 5-100 hp Belt Drive Compressors around the job site. \n\nABOUT THE PUMP\nQuincy Compressors Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'QGS5200\n\nQGS 5-100 hp Belt Drive Compressors\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nQuincy Compressors’ QGS 5-100 hp Belt Drive Compressors is equipped with Quincy Compressors’ Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the QGS 5-100 hp Belt Drive Compressors to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the QGS 5-100 hp Belt Drive Compressors in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the QGS 5-100 hp Belt Drive Compressors to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The QGS 5-100 hp Belt Drive Compressors offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur QGS 5-100 hp Belt Drive Compressors feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'QGS 5-100 hp Belt Drive Compressors\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Quincy QGS can meet your needs. Featuring the most advanced rotary screw air compressor technology, the QGS serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of QGS ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the QGS Air Compressor\n\nOur QGS compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'QGS 5-100 hp Belt Drive Compressors \n\nPart Number:\nQGS 5-100\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nQGS 5-100\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nQuincy Compressors synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nQuincy Compressors QGS 5-100 hp Belt Drive Compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the QGS compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Quincy Compressors sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n375 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi SS5L5 Single Stage Air Compressor is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our Ingersoll Rand products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The SS5L5 Single Stage Air Compressor boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the SS5L5 Single Stage Air Compressor around the job site. \n\nABOUT THE PUMP\nINGERSOLL RAND Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'SS5L5\n\n3.0 HP* Big Bore™ Air Compressor\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nIngersoll Rand’s SS5L5 Single Stage Air Compressor is equipped with Ingersoll Rand’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '225 PSI max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the SS5L5 Single Stage Air Compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the SS5L5 Single Stage Air Compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the SS5L5 Single Stage Air Compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The SS5L5 Single Stage Air Compressor offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed angle grinders and sanders designed for 7” and 9” wheels and pads.\n\nOur SS5L5 Single Stage Air Compressor feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', 'SS5L5 Single Stage Air Compressor\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Ingersoll Rand SS5L5 can meet your needs. Featuring the most advanced rotary screw air compressor technology, the SS5L5 serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of SS5L5 ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the SS5L5 Air Compressor\n\nOur SS5L5 compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', 'SS5L5 Single Stage Air Compressor \n\nPart Number:\nSS5L5\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \nSS5L5\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nIngersoll Rand synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nIngersoll Rand SS5L5 Single Stage Air Compressor are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the SS5L5 compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Ingersoll Rand sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\nSS5L5 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres'], ["Our 150 psi 375 Series T4F Portable Diesel Compressors is constructed with a pancake style tank for stability, with a water drain valve and tough rubber feet. The high-pressure design optimizes air tool performance, delivering 2.6 SCFM at 90 psi for quick recovery time. The oil-free pump provides maintenance-free performance. Transporting is easy with the integrated cord wrap.\n\nAdditional Features\nLow Amp 120V motor starts easily in cold weather or with extension cord\nDurable oil-free pump for long life and no maintenance\nShroud, handle and console cover protects vital components, makes unit easier to carry and includes cord wrap\nTwo regulated, factory installed air couplers to easily support two users\nOnly 30 lbs for easy portability\n\nWe're confident of the quality of our Sullair products and we'll repair, without charge, any defects due to faulty materials or workmanship within the specified warranty.", 'The 375 Series T4F Portable Diesel Compressors boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the 375 Series T4F Portable Diesel Compressors around the job site. \n\nABOUT THE PUMP\nSULLAIR Quality\nSingle Stage\nBall Bearings\nCast-Iron Cylinder\nStainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life\n\nABOUT THE MOTOR\n2.5 HP\n3400 RPM\nOverload Protection with Manual Reset\n115 Volt\n60 Hz\nHeavy-Duty/Industrial Grade with Ball Bearings for Greater Durability\n\nSTANDARD EQUIPMENT\nHeavy Duty Wheels for Greater Jobsite Mobility\nStart/Stop Pressure Switch with On/Off Lever\nFold-Down Handle for Easy Storage/Low Profile\nUser-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,\nSafety Relief Valve\nIntake Filter with Silencer\n13.8 Amp Motor\nInitial 10 oz. Oil Fill Included\n\nSpecifications\nHorse Power: 2.5 HP\nCFM Displaced: 9.3 CFM\nCFM Delivered: 6.5 CFM @ 90 PSI\nPump/Motor RPM: 3', 'Sullair5200\n\n375 Series T4F Portable Diesel Compressors\n\nPOWER : 6.5 CFM @ 90PSI; Powerful enough to run two framing nailers\n\nPERFORMANCE : Cast iron cylinder with greater bore and stroke for maximum performance\n\nDURABILITY : Roll cage construction for extra protection to pump and motor assembly\n\nCONVENIENCE : Oil drain and oil sight glass conveniently located for easy access and maintenance\n\nINCLUDES : Oil and 1/4” universal quick couplers (2)\n\nBig Bore™ Compressors equipped with a Big Bore™ piston, cast iron pump and heavy duty crankshaft deliver faster recovery time and higher CFMs for more efficient nailing and fastening. The Big Bore™ piston and cylinder are larger than those in standard compressors, so they compress more air on each stroke. The result is increased compressor efficiency, faster recovery, and lower RPM for reduced noise.\n\nSullair’s 375 Series T4F Portable Diesel Compressors are equipped with Sullair’s Big Bore™ engineered pump cylinder and piston for higher output for two nailers, with less noise and i', '375 Series T4F Portable Diesel Compressors max tank storage pressure provides a user with 80% more usable air than the industry leader\n5.0 SCFM @ 90 PSI allows the compressor to recover quickly after its initial tank charge is exhausted\nVertical stand feature and collapsible handle allows a user to save space by transporting or storing the compressor in a vertical position\n78 dBA* operational noise level for a quieter work environment (* tested per ISO3477)\n10 in. non-flat pneumatic tires allow for easy transportation around the jobsite\nEHP® Efficient high pressure technology allows for longer pump and motor life\nOil free, maintenance free pump for convenient use\nEfficient high pressure motor allows the compressor to be run with an extension cord (12 Ga. or heavier, 50 ft. or less) due to consistent amp draw requirement of the compressor\nHigh flow coupler allows for maximum nailer performance\nMetal console panel provides a display area as well as protects the gauges, couplers, and regulator\nHigh flow coupler allows for', 'The 375 Series T4F Portable Diesel Compressors offer a low total cost of operation thanks to their 2000 hours bevel gear durability and regulated motor designed for aggressive usage found in industrial metal transformation applications.\n\nA 11-model range of 2.8 hp / 2100 W industrial governed 375 Series T4F Portable Diesel Compressors designed for 7” and 9” wheels and pads.\n\nOur 375 Series T4F Portable Diesel Compressors feature:\nA highly durable spiral bevel gear that reduces vibration and stress of torque transmission resulting in a maintenance interval of 2,000 hours.\nA spindle lock feature that allows for quick and easy abrasive replacement to reduce tool downtime.\nA 360° adjustable air exhaust with integrated muffler. It improves operator’s comfort keeping the noise level as low as 84 dB(A).\nA streamlined and ergonomic two-position safety trigger that can be adapted to an operator’s grip above or below the housing.\nAn ergonomic handle to promote a good operating position by maintaining the operator’s wrist straig', '375 Series T4F Portable Diesel Compressors\n\nIf you’re looking for a highly efficient 5-100 hp compressor, the Sullair 375 Series T4F Portable Diesel can meet your needs. Featuring the most advanced rotary screw air compressor technology, the 375 Series T4F Portable Diesel serves as a reliable source of compressed air for a wide range of industrial applications. And with the low cost of 375 Series T4F Portable Diesel ownership, this peak-performing screw compressor will have a positive impact on your company’s bottom line.\n\nAt a Glance\n\nStandard quiet enclosure\n\n8,000 hr. premium synthetic fluid\n\nLow oil carryover\n\nDesigned for 100% duty cycle\n\nIntegrated dryer option\n\nTank mount option\n\nUp Close\n\nHigh efficiency intake filter\n\nTrue Blue 5-Year Warranty with start up\n\nLong life V-belt drive\n\nTEFC motor, IP 55 (wash down)\n\nKey Features\n\nApplications\n\nPerformance\n\nModel Specs\n\nMaintenance\n\nWarranties\n\nVideos\n\nKey Features of the 375 Series T4F Portable Diesel Air Compressor\n\nOur 375 Series T4F Portable Diesel compressors feature advanced rotary screw compressor technology, enabling easy maintenance and low cost of ownership with', '375 Series T4F Portable Diesel Compressors \n\nPart Number:\n375 Series T4F\n\nPrice\n\nPrice:\n$1,489.99\n\nChoose Options\n\nKits\n\nNone \n\nStart-up Kit (+$159.92)\n\nDelivery Options\n\nFree Freight \n\nLift Gate Service (+$75.00)\n\nQuantity\n\n Add to Cart\n\nDescription\n\nCustomer Reviews\n\nAvailability\n\nShipping Info\n\nProduct Specifications\n \n \n \n \n \n\xa0\n \n \nPart Number:\n \n375 Series T4F\n \n \nStart up kit included\n \n \n \n \nTechnical Details\n \n \n \nDurable cast-iron cylinders, heads, and frame are designed for continuous operation and extended pump life \n \nOversized belt wheel provides reliable design and cooler operation \n \nSullair synthetic lubricant provides 2,000-hour oil change intervals(four times longer than mineral-based lubricants \n \nHigh-efficiency stainless steel finger valves are simple, efficient, and easy to maintain \n \nManual thermal overload protection of the motor \n \nProduct Description\n \nDesigned for the professional, single-stage air compressors are ideal for most anyone, from the do-it-yourselfer to the professi', '400HH\nDESIGNED TO GET THE JOB DONE\n\nSullair 375 Series portable air compressors are ready to hit the ground running for a variety of jobsite applications. Crafted for enhanced usability and serviceability, the 375 compressor family has multiple units—including the award-winning 400HH featuring air pressures up to 200 psi.\n\nCompact design\n\nEasy pressure change\n\nExtended runtime\n\nAvailable with your choice of a reliable Caterpillar or Perkins engine!\n\nModels vary by region. Please contact your Sullair sales representative for more details.\n\nJump To:\n\nSpecs\n\nContact Us\n\nFlow\n375 – 425 cfm\n10.6 – 12 m³/min\n\nPressure\n150 – 200 psi\n10.3 – 13.8 bar\n\nPower\n122 – 157 hp\n91 – 117 kW\n\nFeatures & Benefits\n\nOptions\n\nModels & Specs\n\nFeatures & Benefits\n\nMultiple Engine Options\nCaterpillar C4.4 (T4F)\nPerkins 1204F (T4F)\n\nCompact Design\nEasier towing to and from the job site\nImproved maneuverability — fits more easily in smaller space\nMore convenient storage — on the job site or at the yard\n\nEasy Pres']]