Nikon D700
Overview
Type | Single-lens reflex
Lens
Lens | Interchangeable, Nikon F mount
Sensor/medium
Sensor | 36 mm × 23.9 mm CMOS
Image sensor maker | Nikon
Maximum resolution | 4,256 × 2,832 (12.1 million)
ASA/ISO range | 200–6400, extended mode to 100–12800, HI2 mode 25600
Storage | CompactFlash (Type I only)
Focusing
Focus modes | Single-servo (AF-S); Continuous-servo (AF-C); Manual (M)
Focus areas | 51 AF points (15 cross-type)
Exposure/metering
Exposure metering | TTL 3D Color Matrix Metering II with a 1005 pixel RGB sensor
Metering modes | Matrix metering, center-weighted metering, spot metering
Flash
Flash | Manual pop-up with button release Guide number 12/39 (ISO 100, m/ft)
Flash bracketing | -3 to +1 EV in increments of 1/3 or 1/2 EV
Shutter
Shutter | Electronically controlled focal-plane
Shutter speed range | 1/8000 to 30 sec, bulb, X-sync at 1/250 sec.
Continuous shooting | Approx. 5.0 frame/s, 8.0 frame/s w/battery grip
Viewfinder
Viewfinder | Optical pentaprism, 95% coverage
General
Rear LCD monitor | 3.0-inch (76 mm), VGA resolution, 307,200 pixels (921,600 dots)
Battery | Nikon EN-EL3e rechargeable Lithium-Ion battery
Dimensions | 147×123×77 mm (5.8×4.8×3.0 in)
Weight | 995 g (35.1 oz), body only
Made in | Japan