2.2 & 2.5 engine
Manufacturer | Chrysler
Production | 1981-1995
Configuration | inline-four
Displacement | 2213 cc (135.0 cu in) 2501 cc (152.6 cu in)
Cylinder bore | 87.5 mm (3.44 in)
Piston stroke | 92 mm (3.62 in) 104 mm (4.09 in)
Block material | Cast Iron
Head material | Aluminum
Valvetrain | Double overhead camshafts Single overhead camshaft
Compression ratio | 8.1:1 8.5:1 8.9:1 9.0: 1 9.5:1
Fuel system | Carburetor Single-point fuel injection Multi-point fuel injection
Fuel type | Gasoline Methanol
Oil system | Wet sump
Cooling system | Water-cooled
Successor | AMC straight-4 engine Chrysler 1.8, 2.0 & 2.4 engine