Pau–Canfranc railway
Status | Open: Pau - Bedous Closed: Bedous - Canfranc
Termini | Pau Bedous (Operational)
Planned opening | 1883
Opened | 1928
Closed | 1985
Reopened | 2016
Owner | Chemins de fer du Midi (1874-1937) SNCF (1938-1997) RFF (1997-2014) SNCF (2014-present)
Operator(s) | TER Aquitaine
Electrification | 1928 (1500 V DC overhead)
Partial Closure | 20 March 1970
Closed to passengers | 30 May 1980
Line length | 93 km (58 mi)
Track gauge | 1,435 mm (4 ft 8 1⁄2 in) standard gauge