The DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor boasts the highest air output of any direct drive air compressor in our line-up. The motor-pump delivers a whopping 6.5 CFM @ 90 PSI. The foot-actuated folding handle and heavy-duty flat-free tires make it easy to move the DeWalt 1.6 HP Continuous, 225 PSI, 4.5 Gallon Compressor around the job site. 

ABOUT THE PUMP
DeWalt Quality
Single Stage
Ball Bearings
Cast-Iron Cylinder
Stainless-Steel Reed Valves and Splash Lubrication Ensure Longer Life

ABOUT THE MOTOR
2.5 HP
3400 RPM
Overload Protection with Manual Reset
115 Volt
60 Hz
Heavy-Duty/Industrial Grade with Ball Bearings for Greater Durability

STANDARD EQUIPMENT
Heavy Duty Wheels for Greater Jobsite Mobility
Start/Stop Pressure Switch with On/Off Lever
Fold-Down Handle for Easy Storage/Low Profile
User-Friendly Control Panel Including Gauges and 2 Quick-Disconnects,
Safety Relief Valve
Intake Filter with Silencer
13.8 Amp Motor
Initial 10 oz. Oil Fill Included

Specifications
Horse Power: 2.5 HP
CFM Displaced: 9.3 CFM
CFM Delivered: 6.5 CFM @ 90 PSI
Pump/Motor RPM: 3