Search Site:
HOME | ABOUT US | PRODUCTS | MANUALS | SUPPORT | PRESS ROOM | WHERE TO BUY | REGISTER PRODUCT

# Finex FX3000

The FX3000 is a full size HVLP spray gun for larger jobs and the gun of choice when HVLP is required.

Innovations of the Finex gun include 29% fewer parts, precision lids, repair kits, optional 3M™ PPS™ adapter, optional interchangeable aluminum cups and lowest trigger pull among all guns in its class.

- Features
- Technical Specs
- Applications
- Downloads

- Large pattern size, up to 12.5 inches
- HVLP gun with multiple nozzles ranging from 1.0 to 1.8 spray primer, base, and clear
- Includes FX3000 gun, 600cc aluminum cup, wrench and cleaning brush
- One year warranty

Back to top

- Fluid Tips: 1.0 mm, 1.3 mm, 1.4 mm, 1.5 mm, 1.8 mm
- Air Consumption (cfm): 9.5 SCFM
- Max Inlet HVLP psi: 29 psi (2.0 bar, 200 kPa)
- Weight With Cup: 1.11 lb
- Air Inlet npsm: 1/4 in
- Finish: Black Nickel
- Cup Size: 600 cc
- Pattern Size: 12.5 in
- Warranty: 1 year

Tip Size (mm) | Gun Part Number | Needle, Nozzle, Air Cap Kit Part Number
1.0 | 288878 | 289296
1.3 | 288879 | 289297
1.4 | 288880 | 289298
1.5 | 288881 | 289299
1.8 | 288882 | 289300

Back to top

- 1.0 mm: Light industrial, hobby, spot repair, base coat, clear coat
- 1.3 mm: Base coat, high solid, single stages, clear coat
- 1.4 mm: Base coat, clear coat single stages, sealers, low solid clear, clear coat
- 1.5 mm: Base coat, sealers, enamels, medium to high viscosity, clear coat
- 1.8 mm: Primer, high viscosity

Back to top

- Find Literature
- Find Manual

Back to top

## Accessories

Ultra Mini Aluminum Cup
125cc
PN: 289517
Mini Aluminum Cup
250cc
PN: 289321
3M™ PPS™ Adapter
PN: 289520
Needle Packing Kit
PN: 288891
Air Adjusting Valve
PN: 2210