- LinkedIn
- Facebook
  - STIHL International
  - STIHL TIMBERSPORTS®
- Twitter
- Youtube
  - STIHL International
  - STIHL TIMBERSPORTS®
- Instagram

- Press
- List

Search
Direct product selection: High-pressure cleaners

# RE 90

## Entry-level compact high-pressure cleaner

### General

Lightweight and compact high-pressure cleaner with extensive features. Aluminium pump head, integrated wheel kit, cleaning agent spray set, rotary nozzle, adjustable fan jet nozzle with pressure regulation, anti-drill, quick-release coupling on the trigger, park position for switching off the sprayer when taking breaks, 6 m high-pressure hose, transport handle.

#### Versions

- RE 90
  Note and compare

Deviations from the product range and information provided here are possible, depending on the country. STIHL reserves the right to make changes to technical specifications and equipment.

### Technical specifications

Technical specifications | Value
--- | ---
Working pressure | 100 bar
Weight 1) | 9,8 kg
Max. pressure 2) | 120 bar
Power cable length | 5 m
Min. water flow | 348 l/h
High-pressure hose length | 6 m
Max. water flow | 520 l/h
Max. water supply temperature | 40 °C
Sound power level 3) | 88 dB(A)
Vibration level left 4) | 2,5 m/s²
Vibration level right 4) | 2,5 m/s²
Rated voltage | 220-240 V

1) Complete, ready for use
2) Maximum pressure system
3) K factor according to DIR2006/42/EC = 1.5(dB(A))
4) (K) factor according to Dir. 2006/42/EC = 2m/s²

Deviations from the product range and information provided here are possible, depending on the country. STIHL reserves the right to make changes to technical specifications and equipment.

### Features

### Standard equipment

- ##### ROTATING SPRAY LANCE

  FLEXIBLE WORKING. Thanks to the rotating spray lance, you can easily adapt the alignment of the high-pressure jet to the work situation. The high-pressure lance is ergonomically secure in the hand at all times.

- ##### Rotary nozzle

  Powerful rotary nozzle for tackling stubborn dirt on hard-wearing surfaces. The rotary motion combines the cleaning power of a concentrated pencil jet with the capacity to clean large areas.

- ##### Cleaning agent spray set

  The spray set delivered with the tool makes it possible to add cleaning agent to the spray jet in order to tackle stubborn dirt. The spray set is also easy to attach to the spray lance.

- ##### Storing accessories on the tool

  The high-pressure trigger, spray lance, fan jet nozzle, rotary nozzle, high-pressure hose and cleaning agent spray set can be stored securely.

- ##### Fan jet nozzle, adjustable pressure

  Fan jet nozzle with pressure regulation to clean different types of surfaces quickly and effectively.

- ##### Cable hook

  The two cable hooks allow the cable to be wound up and neatly and securely stored on the tool.

- ##### Integrated wheel kit

  The integrated wheel kit allows the high-pressure cleaner to be manoeuvred comfortably.

- ##### Anti-drill and quick-release coupling

  The anti-drill and quick-release coupling makes setting up the high-pressure cleaner easier and prevents the high-pressure hose from tangling while you work, allowing the full length of the hose to be used.

- ##### Park position

  Allows you to switch off the assembled high-pressure lance when taking breaks, and to store the lance on the tool.

Deviations from the product range and information provided here are possible, depending on the country. STIHL reserves the right to make changes to technical specifications and equipment.

### Accessories

- - ##### RA 110 surface cleaner

    Ø 310 mm. For quick, splash-free cleaning of larger surfaces. With pressure adjustment, for RE 90 – RE 170 PLUS.

  #### Versions

  - Surface cleaner RA 110
    Note and compare

- - ##### RA 101 surface cleaner

    For quick and splash-free cleaning of large horizontal and vertical areas. Including spray lance extension, for RE 90 – RE 170 PLUS.

  #### Versions

  - Surface Cleaner RA 101 for RE 88 - RE 143 PLUS
    Note and compare

- - ##### RA 90 surface cleaner

    Ø 255 mm. For quick, splash-free cleaning of medium-sized areas. With pressure adjustment, for RE 90 – RE 130 PLUS.

  #### Versions

  - Surface cleaner RA 90
    Note and compare

- - ##### High-pressure hose extensions

    For more range. With quick-release coupling.

  #### Versions

  - 7 m, textile mesh for RE 90 – RE 130 PLUS
    Note and compare

- - ##### Flat textile hose with holder

    12 m long. Low-pressure hose including holder, can be easily rolled and unrolled, enabling space-saving storage. Can be stored directly on the tool.

  #### Versions

  - Flat textile hose with holder
    Note and compare

- - ##### High-pressure hose extensions

    For more range. With quick-release coupling.

  #### Versions

  - 9 m, steel-reinforced for RE 90 – RE 170 PLUS
    Note and compare

- - ##### Backflow preventer including 3/4" coupling

    Prevents water flowing back out of the high-pressure cleaner into the drinking water supply.

  #### Versions

  - Backflow preventer for RE 232 – RE 282 PLUS
    Note and compare

- - ##### Pipe cleaning set

    15 m long. Also suitable for smaller diameter pipes. With nozzle, for RE 90 – RE 163 PLUS.

  #### Versions

  - Pipe cleaning set
    Note and compare

- - ##### Rotating wash brush

    Ø 155 mm. For effective cleaning of sensitive surfaces, with rotating inner brush and adjustable working angle, for RE 90 – RE 170 PLUS .

  #### Versions

  - Rotating wash brush
    Note and compare

- - ##### Wet sandblasting device

    For wet sandblasting of brickwork and metal parts. Best results with the STIHL blasting granulate SB 90, for RE 90 – RE 163 PLUS.

  #### Versions

  - Wet sandblasting device
    Note and compare

- - ##### Suction set

    3 m long. For low-pressure water supply from rain water tanks and cisterns. It is recommended that a water filter is fitted, for RE 90 – RE 163 PLUS.

  #### Versions

  - Suction set
    Note and compare

- - ##### Foam nozzle

    Powerful cleaning effect due to foam that adheres to the surface for a long time. The alignment of the spray jet and spray angle can be adjusted. With measuring system and large filler opening, for RE 90 – RE 170 PLUS.

  #### Versions

  - Foam nozzle
    Note and compare

- - ##### Spray lance

    1,080 mm long. Sturdy, angled spray lance for cleaning difficult-to-access spots, for RE 90 – RE 170 PLUS.

  #### Versions

  - Spray lance
    Note and compare

- - ##### Spray lance extension

    430 mm long. For RE 90 – RE 170 PLUS.

  #### Versions

  - Spray lance extension
    Note and compare

- - ##### Flat wash brush

    Approx. 285 mm wide. For cleaning delicate surfaces. With integrated rubber lip for removing water residue, for RE 90 – RE 130 PLUS.

  #### Versions

  - Flat wash brush
    Note and compare

- - ##### Water filter for RE 80 - RE 170 PLUS

    Protects the pump against dirt from the water supply. 3/4" connection. For RE 90 – RE 170 PLUS.

  #### Versions

  - Water filter for RE 80 - RE 170 PLUS
    Note and compare

Deviations from the product range and information provided here are possible, depending on the country. STIHL reserves the right to make changes to technical specifications and equipment.

### Documents

### Owners manuals and safety brochures

Languages | Date | Link
--- | --- | ---
International | 22.08.2019 | Download PDF Download PDF