The FX3000 is a full size HVLP spray gun for larger jobs and the gun of choice when HVLP is required.

Innovations of the Finex gun include 29% fewer parts, precision lids, repair kits, optional 3M
™

	PPS
™
 adapter, optional interchangeable aluminum cups and lowest trigger pull among all guns in its class.

Features

Technical Specs

Applications

Downloads

Large pattern size, up to 12.5 inches 

HVLP gun with multiple nozzles ranging from 1.0 to 1.8 spray primer, base, and clear

Includes FX3000 gun, 600cc aluminum cup, wrench and cleaning brush 

One year warranty

Fluid Tips:
 1.0 mm, 1.3 mm, 1.4 mm, 1.5 mm, 1.8 mm

Air Consumption (cfm):
 9.5 SCFM

Max Inlet HVLP psi:
 29 psi (2.0 bar, 200 kPa)

Weight With  Cup:
 1.11 lb 

Air Inlet npsm:
 1/4 in

Finish:
 Black Nickel

Cup Size:
 600 cc

Pattern Size:
 12.5 in

Warranty:
 1 year

Tip Size (mm)

Gun Part Number

Needle, Nozzle, Air Cap Kit Part Number

1.0

288878

289296

1.3

288879

289297

1.4

288880

289298

1.5

288881

289299

1.8

288882

289300

1.0 mm:
 Light industrial, hobby, spot repair, base coat, clear coat

1.3 mm:
 Base coat, high solid, single stages, clear coat

1.4 mm:
 Base coat, clear coat single stages, sealers, low solid clear, clear coat

1.5 mm:
 Base coat, sealers, enamels, medium to high viscosity, clear coat

1.8 mm:
 Primer, high viscosity

Accessories

Ultra Mini Aluminum Cup
125cc
PN: 289517
	

Mini Aluminum Cup
250cc
PN: 289321
	

3M
™
 PPS
™
 Adapter
PN: 289520
	

		Needle Packing Kit
PN: 288891
	

Air Adjusting Valve
PN: 2210