XCV11Z
18V LXT® Lithium‑Ion Brushless Cordless 2 Gallon HEPA Filter Portable Wet/Dry Dust Extractor/Vacuum, Tool Only
XCV11Z

### 18V LXT® Lithium‑Ion Brushless Cordless 2 Gallon HEPA Filter Portable Wet/Dry Dust Extractor/Vacuum, Tool Only

- PERFORMANCE : Powerful Brushless motor delivers 57 CFM using a 18V LXT® Lithium-Ion battery (battery not included)
- PORTABILITY : Compact and portable design; weighs only 10.1 lbs.
- EFFICIENCY : Filter cleaning system is designed to maintain optimum suction efficiency and longer filter life
- DUST MANAGEMENT : Efficient HEPA filter captures 99.97% of particulates .3 microns and larger
- INCLUDES : Flexible hose, wide nozzle, crevice nozzle, HEPA Filter

- VIEW DUST MANAGEMENT OPTIONS

- - Download Image as:
  - - JPG
  - - PNG
  - - TIF

OVERVIEW
APPLICATIONS
FEATURES

- #### LXT® Lithium-Ion

  Tool users who unplug the cord with Makita 18V LXT® experience new levels of convenience, efficiency and productivity. Makita created the 18V Lithium-Ion cordless tool category in 2005, and today it is the world’s largest 18V cordless tool line-up. Makita’s leading technology gives tool users unmatched performance and breadth of line, with innovation in motor and battery technology that is obliterating industry standards – and leaving old thinking behind. With high amp-hour batteries, efficient brushed and brushless motors, and 36V (18V X2) LXT® technology, Makita 18V LXT® tools not only meet corded demands, they can exceed the performance of corded, all while remaining in a single cordless platform powered by the industry's fastest-charging 18V lithium-ion batteries. [Learn More]

- #### Star Protection Computer Controls™

  Makita cordless tools are engineered for industrial applications, and for added protection during the most demanding jobs Makita created STAR Protection Computer Controls™. STAR is communications technology that monitors conditions during use, allowing the tool and battery to exchange data to protect against overloading, overdischarging and overheating. If STAR detects conditions that threaten to overload, overdischarge or overheat the tool or battery, the tool will automatically stop. At that time the user can either restart the tool, change or charge the battery, and put the tool back to work. When you slide a Makita 18V LXT® battery with the STAR symbol onto a Makita tool that has either the STAR symbol or a yellow terminal, you are benefitting from STAR Protection Computer Controls™.

- #### XPT™ Extreme Protection Technology

  When the job takes your Makita tool into harsh conditions, Makita Extreme Protection Technology (XPT™) provides added protection. XPT™ is a series of integrated seals engineered to channel away dust and water for increased durability. Wherever the job takes you, Makita tools equipped with XPT™ are engineered for increased durability and longer tool life.

The 18V LXT® Brushless 2 Gallon HEPA Filter Portable Wet/Dry Dust Extractor/Vacuum, Tool Only (XCV11Z) is a powerful, portable solution in dust management applications. The XCV11Z captures 99.97% of particulates .3 microns and larger with the efficient HEPA filter. It’s compact and cordless design with an shoulder strap (sold separately) allows easy transport of the vacuum throughout the space for efficient use. Get up to 60 minutes of continuous run-time and up to 57 CFM and 27” water lift of suction with just one 5.0Ah battery (sold separately).

It’s part of Makita’s expanding 18V Lithium-Ion system, the world’s largest cordless tool system powered by 18V Lithium-Ion slide-style batteries. Makita 18V Lithium-Ion batteries have the fastest charge times in their categories, so they spend more time working and less time sitting on the charger.

For improved tool performance and extended battery life, Makita created Star Protection Computer Controls™. Star Protection is communication technology that allows the Star Protection-equipped tool and battery to exchange data in real time and monitor conditions during use to protect against overloading, over-discharging and overheating. For increased versatility, the tool can also be powered by Makita 18V LXT® and Compact Lithium-Ion batteries with the star symbol on the battery indicating Star Protection inside.

- Powerful BL™ Brushless motor delivers 57 CFM and 27" water lift of suction using an 18V LXT® Lithium-Ion battery (battery not included)
- Filter cleaning system is designed to maintain optimum suction efficiency and longer filter life
- Efficient HEPA filter captures 99.97% of particulates .3 microns and larger
- Up to 60 minutes of continuous run time using an 18V LXT® Lithium-Ion 5.0Ah battery BL1850B (battery not included)
- L.E.D. battery indicator shows charge level for 18V LXT® Lithium-Ion battery
- The BL™ Brushless Motor eliminates carbon brushes, enabling the BL™ Motor to run cooler and more efficiently for longer life
- Compact and portable design; weighs only 10.1 lbs. with 18V LXT® 5.0Ah battery (battery not included)
- Two tools in one; quickly converts from vacuum to blower for increased versatility
- Two speed push button power selection (high/low) for a variety of applications
- Battery compartment keeps the battery protected from harmful debris on the jobsite
- Integrated tethering hooks for increased portability with optional shoulder strap
- Carrying top handle stores out of the way and provides increased comfort during transport
- On-board hose and nozzle storage allow for easy and convenient transport
- Quick-release latch for easy removal and disposal of debris from canister
- Optional Shoulder Strap available (part no.162523-7) for convenient carrying
- Extreme Protection Technology (XPT™) is engineered for improved dust and water resistance for operation in harsh conditions
- Equipped with Star Protection Computer Controls™ to protect against overloading, over-discharging and over-heating
- Rapid Optimum Charger communicates with the battery's built-in chip throughout the charging process to optimize battery life by actively controlling current, voltage and temperature (battery and charger sold separately)
- Rapid Optimum Charger has a built-in fan to cool the battery for faster, more efficient charging (battery and charger sold separately)
- Makita technology delivers category-leading charge time so the battery spends more time working and less time sitting on the charger (battery and charger sold separately)
- Compatible with Makita 18V Lithium-Ion batteries with a Star symbol
- 3-year limited warranty
- Only use genuine Makita batteries and chargers

- (1) Round Wet/Dry HEPA Filter (162518-0)
- (1) Pre-Filter Set, XCV11Z (199827-4)
- (1) 5" Black Upholstery Nozzle (458891-7)
- (1) 7" Black Crevice Nozzle (458919-1)
- (1) Flexible Anti-Static Hose, 1” x 6.5’ (140G04-3)
- Gross Container Size : 2 gal.
- Air Flow Rate : 57 CFM
- Static Water Lift : 27"
- Continuous Use (max, in minutes) : 60 min.
- Battery : 18V LXT® Lithium-Ion
- Filter Cleaning : Yes
- HEPA filter : Yes
- Equipped Filter Efficiency : 99.97% of .3 microns
- Working Sound Level : 76 dB(A)
- Net Weight (with battery) : 10.1 lbs.
- Power Type : Cordless
- Form Factor (LXT) : 18V LXT®
- Motor Type : Brushless
- Shipping Weight : 10.5 lbs.
- UPC Code : 088381-870474
- XCV11 Instruction Manual
- XCV11 Parts Breakdown
- Makita XCV11Z New Tool Flyers (English)
Page of Start over
162523-7 Shoulder Strap 424379-9 Tool Cuff Adapter, 24mm for 1" hose 195548-6 Cuff Joint Adapter, 38mm to 22mm 199827-4 Pre-Filter Set, XCV11Z 192562-3 Curved Pipe 192563-1 Straight Pipe 191657-9 2" Black Round Brush XCV09Z 36V (18V X2) LXT® Brushless 1/2 Gallon HEPA Filter Backpack Dry Vacuum XCV04Z 36V (18V X2) LXT® 2.1 Gallon HEPA Filter Dry Dust Extractor/Vacuum XCV02Z 18V LXT® 3/4 Gallon Portable Dry Dust Extractor/Blower

You May Also Be Interested In...

Page Of Start over
162518-0 Round Wet/Dry HEPA Filter 199827-4 Pre-Filter Set, XCV11Z 458891-7 5" Black Upholstery Nozzle 458919-1 7" Black Crevice Nozzle 140G04-3 Flexible Anti-Static Hose, 1” x 6.5’ XCV24ZX 36V (18V X2) LXT® Brushless 4 Gallon HEPA Filter Dry Dust Extractor XCV08PT 36V (18V X2) LXT® Brushless 2.1 Gal HEPA Filter Dry Dust Extractor/Vac Kit, AWS® XCV21PTX 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor Kit XCV04PT 36V (18V X2) LXT® 2.1 Gallon HEPA Filter Dry Dust Extractor/Vacuum Kit XCV07PTX 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor Kit XCV25ZUX 36V (18V X2) LXT® Brushless 4 Gallon HEPA Filter Dust Extractor/Vacuum, AWS® XCV04Z 36V (18V X2) LXT® 2.1 Gallon HEPA Filter Dry Dust Extractor/Vacuum DCL501Z 18V LXT® Brushless Cyclonic Canister Vacuum VC4210L 11 Gallon Wet/Dry HEPA Filter Dust Extractor/Vacuum, AWS® Capable XCV20Z 36V (18V X2) LXT® Brushless 2.1 Gallon Wet/Dry Dust Extractor/Vacuum XLC07SY1 18V LXT® Compact Handheld Canister Vacuum Kit XLC07Z 18V LXT® Handheld Canister Vacuum ADCV11T Outdoor Adventure™ 18V LXT® Brushless Wet/Dry Vacuum Kit XCV22PTU 36V (18V X2) LXT® Brushless 2.1 Gal. HEPA Filter Dust Extractor/Vacuum Kit, AWS® XCV21ZX 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dry Dust Extractor ADCV11Z Outdoor Adventure™ 18V LXT® Brushless Wet/Dry Vacuum XCV22ZU 36V (18V X2) LXT® Brushless 2.1 Gallon HEPA Filter Dust Extractor/Vacuum, AWS® XCV02Z 18V LXT® 3/4 Gallon Portable Dry Dust Extractor/Blower XCV23Z 36V (18V X2) LXT® Brushless 4 Gallon Wet/Dry Dust Extractor/Vacuum XCV11T 18V LXT® Brushless 2 Gal. HEPA Filter Portable Wet/Dry Dust Extractor/Vacuum Kit
X
Share your wish list
Don't show again

La página que selecciono por el momento no está disponible en español.

Le gustaría:

¿Proceder con esta página en Inglés?