ROS20VSC Professional

Sanders

ROS20VSC Professional

Sanders

5 In. Palm Random Orbit Sander/Polisher

Integral pad dampening brake system helps prevent swirl marks

Bosch’s hook-and-loop disc attachment delivers secure fit

Microcellular backing pad for smooth, fine finishes

Variable-speed control to match speed to workpiece and task

Adjustable from between 7,500 and 12,000 OPM

Optimal on-board system for filtering fine dust

Soft-grip top and body

Low-vibration operation

Sanding disc, vacuum hose adapter and carrying bag

Hook-Tight™ hook-and-loop disc attachment includes over 35,000 long-life hooks ensure firm grip of disc, up to twice the standard number of hooks

Technical data

The most important data

Amperage

2.5 

Case Type

Bag 

Disc Size

5" 

Dust Collection

Yes 

Eccentric Offset

3/64” (1.2 mm) 

Height in

6 "

Length in

9 "

No Load OPM

7,500-12,000 

Orbit Diameter

3/32" (2.5 mm) 

Orbit Radius

3/64" (1.25 mm) 

Pad Size

5" 

Paper Size / Type

5" Round 