Laser distance measures offer a fast and convenient solution to distance measuring applications that would otherwise require multiple steps to achieve. The Makita Laser Distance Measure, 262' (model LD080P) is engineered to make tape measuring methods obsolete and provide unmatched productivity and sophistication for a full range of measuring applications. 
The LD080P provides a distance operating range of up to 262' for long distance capacity, and has a top-class accuracy of +/- 1/16" for maximum precision. For added versatility, it provides both standard and metric units of measurement, and the following measurement functions: Distance; Area; Volume; Permanent; Min/Max; Add/Subtract; Stake-Out; Pythagoras (2 point); Pythagoras (3 point); Pythagoras (partial height). Convenience features include an auto power-off function that shuts off the device automatically for increased run time performance, and a simplified user interface button and screen.

Features

Measuring distance operating range up to 262' for moderate distance capacity

Provides top-class accuracy of +/- 1/16" for maximum precision

Provides both standard and metric units of measurement

Provides 9 measurement functions for increased versatility of applications: Distance, Area, Volume, Permanent, Min/Max, Add/Subtract, Stake-Out, Pythagoras (2 point), Pythagoras (3 point), Pythagoras (partial height)

Bright 635 nm class II (<1mw) laser for best-in-class visibility in moderate ambient light environment

Battery run time delivers up to 5,000 measurements for continuous work and increased productivity

Records history of 20 measurements for convenience

Auto power-off function automatically shuts the device off for increased run time performance

Rubber over-mold for increased protection and durability

Dust and water resistance with IP 54 rating for increased durability

Simplified user interface buttons and screen for convenience

Flip out end piece is designed to enable accurate readings from a corner or defined edge position

Integrated 1/4" thread enables mounting to a tripod for measurement stability and accuracy

Backlight L.E.D. display for increased screen visibility

Specs

Line accuracy (at 33') : +/- 1/16"

Working range (in.) : 262'

Smallest unit of measure : 1/32"

Laser diode : Class II, 635 nm

Historical memory : 20

Auto shut off : Yes

Net Weight : .3 lbs.

Power supply (AAA battery) : 2

Shipping Weight : .6 lbs.

UPC Code : 088381-635165

Includes

(1) Carrying Pouch

(1) Laser Strap

(2) AAA Batteries