ZT6000e
ZT6000e
Electric Zero-Turn Mower

# ZT6000e
Electric Zero-Turn Mower

- Reduced sound levels and zero emissions provide an enhanced operator comfort experience
- 4.3-inch touch display provides easy adjustment of power, speed, performance and control
- Low maintenance with fewer parts, including no gas or belts
- Up to 4-6+ hours* of mowing performance with an integrated lithium ion battery
- Recharges in 6.3 hours with 240-volt connection or 12.6 hours with 120-volt connection

*Times will vary depending on conditions

Search Inventory

- Contact Dealer
- Find Dealer

## ZT6000e Overview

The ZT6000e brings electric-powered innovation to high-performance commercial mowing. With its impressive runtime of 4-6+ hours* and an AirFX™ cutting deck, Bobcat has amplified electric-powered mowing.

- Bullnose AirFX™ cutting deck with a deep deck design that increases vacuum, lifting grass up to the cutting blade for a superior quality of cut.
- Zero-maintenance battery and fewer parts that require repair or replacement.
- Three electric motors provide high and low blade speeds to make quick work of any mowing condition.

*Times will vary depending on conditions.

## ZT6000e Specs & Compare

Compare
Units
Metric

##### ZT6000e Key Specifications

Battery Type
Lithium Ion
System Voltage
58 V
Gross Battery Capacity
20.4 kW·h
On-Board Charge Time - 120 V
12.6 hrs - (Estimated Run Time: 4-6+ hrs. depending on grass-cutting conditions)
On-Board Charge Time - 240 V
6.3 hrs - (Estimated Run Time: 4-6+ hrs. depending on grass-cutting conditions)
Mower Deck
AirFX Cutting System
Deck Material
10-gauge layer top with 3-gauge and 7-gauge brackets throughout
Baffle System
Replaceable, Air Gap
Leading Edge
Adjustable, Front Lip Standard
Cutting Width
52 in
Blade Tip Speed - High
18,244 ft/min
Blade Tip Speed - Low
16,766 ft/min
Weight
1425 lb
Length
82.3 in
Width (Chute Up)
56 in
Width (Chute Down)
67.9 in
Height (ROPS Up)
75.4 in
Height (ROPS Folded)
49.8 in
Seat
High Back, Full Mechanical Suspension Seat
Seat Adjustment
Seat Slide Lever
Fold Down ROPS
Standard
Operator Touch Screen Display
4.3" touchscreen display
Drive Wheel Size
24 x 10.5-12
Front Caster Wheel Size
15 x 6.5-6
Caster Tire Type
Pneumatic
Forward Speed - High
10.9 mph
Forward Speed - Medium
9 mph
Forward Speed - Low
7 mph
Reverse Speed - High
4.1 mph
Reverse Speed - Medium
3.4 mph
Reverse Speed - Low
3.1 mph

##### Electrical System

Battery Type
Lithium Ion
System Voltage
58 V
Gross Battery Capacity
20.4 kW·h
On-Board Charge Time - 120 V
12.6 hrs - (Estimated Run Time: 4-6+ hrs. depending on grass-cutting conditions)
On-Board Charge Time - 240 V
6.3 hrs - (Estimated Run Time: 4-6+ hrs. depending on grass-cutting conditions)

##### Deck

Mower Deck
AirFX Cutting System
Deck Material
10-gauge layer top with 3-gauge and 7-gauge brackets throughout
Baffle System
Replaceable, Air Gap
Leading Edge
Adjustable, Front Lip Standard
Cutting Width
52 in
Blade Tip Speed - High
18,244 ft/min
Blade Tip Speed - Low
16,766 ft/min
Discharge Chute
Flexible Molded Polymer

##### Engine

##### Dimension

Weight
1425 lb
Length
82.3 in
Width (Chute Up)
56 in
Width (Chute Down)
67.9 in
Height (ROPS Up)
75.4 in
Height (ROPS Folded)
49.8 in
Front and Rear
1.5- x 2.5-inch Steel Tubing; Welded Steel Reinforced Frame

##### Features

Seat
High Back, Full Mechanical Suspension Seat
Seat Adjustment
Seat Slide Lever
Fold Down ROPS
Standard
Operator Touch Screen Display
4.3" touchscreen display

##### Wheels

Drive Wheel Size
24 x 10.5-12
Front Caster Wheel Size
15 x 6.5-6
Caster Tire Type
Pneumatic

##### Power System

Drive Description
HD Planetary Gearbox w/ integrated parking brake
Forward Speed - High
10.9 mph
Forward Speed - Medium
9 mph
Forward Speed - Low
7 mph
Reverse Speed - High
4.1 mph
Reverse Speed - Medium
3.4 mph
Reverse Speed - Low
3.1 mph

###### ZT6000e

###### ZT2042SA

Compare

###### ZT2052SB

Compare

###### ZT2048SA

Compare

###### ZT3048SC

Compare

###### ZT3061SE

Compare

###### ZT3052SD

Compare

###### ZT3548SF

Compare

###### ZT3552SG

Compare

###### ZT3561SH

Compare

###### ZT5061SH

Compare

###### ZT5052SH

Compare

###### ZT6052SL

Compare

###### ZT6061SL

Compare

###### ZT6161SN

Compare

###### ZT7061SP

Compare

###### ZT7072SP

Compare

###### ZT7072SW

Compare

###### ZT7061SW

Compare

###### ZT7061SR

Compare

###### ZT7072SR

Compare

- Search Inventory
- Build & Quote
- Contact Dealer
- Download Brochure
- Request Demo

- Search Inventory
- Build & Quote
- Contact Dealer
- Download Brochure
- Request Demo

- Search Inventory
- Build & Quote

## ZT6000e Features & Benefits

##### Battery Power Benefits

6

##### Low Cost of Ownership

With significantly fewer parts, no gas and its high voltage maintenance-free battery, the ZT6000e costs considerably less to operate than its gas-powered equivalents.

##### Minimal Service and Maintenance

There's no combustion engine parts that will ever need to be repaired or replaced. There's no fluids, no belts and no need for gas refills. Because the ZT6000e is a fully electric powered machine, there are fewer components that can fail and lead to downtime. You'll also spend significantly less time maintaining the all-electric ZT6000e and more time cutting grass. Aside from routine recharges, the lithium-ion battery requires no maintenance for the life of the machine.

##### Integrated 58 V/20.4 kWh Lithium-Ion Battery

One a single charge, the powerful 20.4-kWh lithium battery supports up to 4-6+ hours* of runtime in commercial mower applications. The ZT6000e can be fully recharged in 6.3 hours with a 240-volt connection, or 12.6 hours using a 120-volt connection.

##### Maintenance-Free Battery Integrated 58 V/20.4 kWh Lithium-Ion Battery

Apart from routine recharge cycles, the powerful lithium-ion battery requires no maintenance for the life of the machine.

##### Zero Emissions

Producing no emissions, the ZT6000e enhances the working environment for the operator and bystanders alike. These machines can also generate new business among a growing number of businesses, homeowners and other potential customers who choose to support eco-friendly practices and a more sustainable future. Government agencies and businesses are increasingly adopting environmental, social and governance principles that give priority to sustainable business practices.

##### Improved Operator Experience

The all-electric drivetrain eliminates the noise created by gas-powered engines. Bystanders will appreciate the noticeable noise reduction, especially when the mowing deck is not engaged.

##### Performance

9

##### Integrated 58 V/20.4 kWh Lithium-Ion Battery

At the heart of the ZT6000e is its powerful 20.4-kWh, lithium-ion battery. On a single charge, it supports up to 4-6+ hours* of runtime in commercial mowing applications. The ZT6000e can be fully recharged in 6.3 hours with a 240-volt connection, or 12.6 hours using a 120-volt connection.

##### Three Independent Blade Motors (Electric)

Three powerful electric motors provide high and low blade speeds to make quick work of both heavy and light mowing conditions.

61-Inch deck blade speeds:

- High: 18,500 f/min.
- Low: 16,999 f/min.

52-inch deck blade speeds:

- High: 18,244 f/min.
- Low: 16,766 f/min.

##### On-Board Charger

The ZT6000e features an on-board charger with a standardized connection point that accommodates either 240-volt or 120-volt connections.

##### AirFX Cutting Deck

The AirFX™ cutting deck allows you to deliver a cut above the rest. It's deep profile and bullnose design creates a powerful vacuum that lifts the grass to the blade for a razor-sharp, uniform cut and a professional finish. AirFX cutting technology accelerates airflow under the deck and aggressively shoots clippings out the extra-large discharge chute.

Bullnose Design

The robust bullnose design provides optimal durability while lifting the grass and increasing the vacuum effect.

Adjustable Front Lip

The deck's adjustable front lip optimizes your cutting capability for all kinds of mowing conditions and grass types.

Deep-Deck Design With Patent-Pending Air-Gap Baffles

The deep-deck design and patent-pending Air-Gap baffles create powerful airflow throughout the cutting deck. This allows the cutting system to efficiently move the clippings out from the extra-large discharge chute and evenly disperse them on the ground. You can tackle tough mowing and get a cleaner deck at the end of the workday.

Polymer Discharge Chute

The flexible, molded chute is constructed for even clipping dispersal and improved deck cleanliness.

Learn More

##### Productive Travel Speeds

Ground speeds of 10.9 mph, along with 24-inch drive tires, help you cover big and small lots in less time.

##### On-The-Go Blade Speed Changes

Change the blade speed on the go to meet the mowing conditions, get more mowing done in less time and leave behind a quality cut. The ZT6000e features high and low blade speeds to meet the mowing conditions. Low blade speeds allow you to conserve power during lighter mowing tasks.

61-Inch deck blade speeds:

- High: 18,500 f/min.
- Low: 16,999 f/min.

52-inch deck blade speeds:

- High: 18,244 f/min.
- Low: 16,766 f/min.

##### HD Planetary Gearbox with Integrated Parking Brake

The lithium-ion battery powers two heavy-duty planetary gearboxes which automatically engage and disengage the parking brake depending on the lap bar position.

##### Three Drive Response Modes

With three drive response modes, operators can choose how the ZT6000e responds to the movement of the lap bars. Whether you like a more gradual response; quick, instant feedback; or a response somewhere in between, three drive response modes put you in control.

The three drive response settings are:

- Drive Response 1 provides a smooth responsive reaction to lap bar movement. With a top speed of 7.07 mph (Drive only)
- Drive Response 2 is the default setting and provides a normal responsive reaction to lap bar movement. With a top speed of 9 mph (Drive only)
- Drive Response 3 provides a quick, responsive reaction to lap bar movement. With a top speed of 10.92 mph (Drive only)

##### 24-Inch Drive Tires (24x10.5)

The large, 24-inch, tires are designed specifically for zero turn mowers, providing exceptional maneuverability, traction and a light footprint. They offer great performance on a variety of surfaces, including slopes and rough terrain. These drive tires deliver a smooth ride and all the maneuverability you need to mow around obstacles in your path.

##### Uptime Protection & Durability

8

##### Integrated 58 V/20.4 kWh Lithium- Ion Battery

The ZT6000e features a powerful 20.4-kWh lithium-ion battery that requires no maintenance.

##### AirFX Cutting Deck High-Pressure Die Cast Aluminum Spindles

The AirFX cutting deck, with high-strength die-cast aluminum spindles, provides the rugged durability you need for nonstop mowing productivity.

Learn More

##### AirFX Cutting Deck Heavy-Gauge Steel Construction

The rugged AirFX cutting deck is built from 10-gauge steel with and 3- and 7-gauge reinforcements to keep you on the lawn and out of the repair shop.

Learn More

##### Battery and Operator Uptime Protection

When the battery needs to be recharged, (below 2% state of charge) the ZT6000e automatically cuts power to the deck, giving the operator approximately 30 minutes of drive time to arrange for a recharge.

##### Strong Dampers

Dampers feature helm joints for more durability and less free play.

##### Pneumatic Caster Wheels (15 x 6.5-6)

The front caster wheels are built tough to keep your mower rolling smoothly and uniformly over the ground for consistent, efficient results. Optional no-flat caster wheels are also available.

##### Dual-Tubed Frame

The ZT6000e frame is built with heavy-duty, dual-tubed steel framing that provides maximum durability to keep you on the job and out of the shop.

##### Protective Bumper

Made from heavy-duty steel to protect mower components, the bumper provides simple access to maintenance items.

##### Comfort

11

##### Reduced Noise

The all-electric drivetrain eliminates the noise created by gas-powered engines. Bystanders will appreciate the noticeable noise reduction, especially when the mowing deck is not engaged.

##### Smooth Operation. Less Vibration.

With no engine vibration, you’ll experience smooth mower movement and a more comfortable ride that reduces the fatigue of long workdays.

##### 4.3-Inch Touch Display

The 4.3-inch touch display provides vital information that makes daily mowing more productive and regular maintenance easier. The touchscreen displays the drive response mode, blade speed, calibration and battery management. It offers password protection for display access and can be used while wearing gloves.

Home Screen

The digital display’s home screen provides the following information:

- Drive Response Mode
- Blade Speed Selection or Deck Mode
- Battery Life
- Time of day
- Machine Hours
- Service Code Notifications
- Machine Derate Notification
- Operator Presence Icon
- Lap Bar Open Icon
- Parking Brake Icon

Startup Screen

With passcode entry, operators can view machine hours, the state of battery charge and PTO hours.

Vitals Screen

The display’s Vitals screen provides the following information:

- Battery Life
- Time of Day
- Machine Hours
- Battery State of Charge - High Voltage Battery
- Battery Temperature - High Voltage Battery
- Battery Voltage - Low Voltage Battery
- PTO (cutting hours)
- Machine Hours
- Blade Tip Speed
- Machine Performance Card

Service Screen

The touchscreen displays active service codes to help operators manage any maintenance needs.

Settings Screen

Operators can use the settings screen to:

- Calibrate the lab bar
- View the blade tip-speed
- Change the touchscreen access passcode
- Set the digital clock display
- Set the display brightness

Charging Screen

The charge display, active only when the mower is connected for a recharge, shows the state of charge and if a connection fault occurs.

##### Professional-Level Comfort and Usability

When you mow for a living, you can’t sacrifice comfort. With Bobcat mowers, you won’t. Your Bobcat mower surrounds you in comfort with a deluxe suspension seat, and it puts all the mower’s capability within easy reach.

##### Wider Footplate

The wider footplate gives you extra room to stretch out for long mowing jobs.

##### High-Back Deluxe Suspension Seat

Your Bobcat mower gives you all-day comfort in the operator station. Its extra high back seat provides unbeatable support and comfort while you work. It features weight adjustment with fore and aft mechanical adjustment.

##### Standard Headlight

Get extra visibility for early and late mowing, and make yourself more visible to bystanders.

##### Almond-Shaped Handles

The ergonomic almond-shaped handles provide smooth, responsive control with a natural, comfortable shape that feels great in your hands and keeps fatigue to a minimum.

##### Spring-Assisted Return to Neutral

The control levers have a spring-assisted return to neutral from either forward or reverse.

##### Operator Controls

Ergonomic design and placement of controls, gauges and creature comforts ensure that the operation of your mower is easy, intuitive and enjoyable.

On the Right:

- Display
- PTO
- Hour meter
- Storage cubby

On the Left:

- USB port
- Cup holder
- Cell phone holder
- Storage cubby

Control Lever:

- Almond shaped handles
- Adjustable levers – up/down, fore/aft
- Enhanced Mounting

Deck Lift Controls:

- The hand-controlled, deck lift lever is in easy reach
- Full length provides mechanical advantage
- Adjustable foot pedal
- Tethered HOC pin

##### Rear Bumper with Tie-Downs

The rear bumper offers added protection and is designed with large tie-down openings that allow for simple trailering and transportation.

##### Serviceability

4

##### Minimal Service and Maintenance

There's no combustion engine parts that will ever need to be repaired or replaced. There's no fluids, no belts and no need for gas refills. Because the ZT6000e is a fully electric powered machine, there are fewer components that can fail and lead to downtime. You'll also spend significantly less time maintaining the all-electric ZT6000e and more time cutting grass.

##### AirFX Cutting Deck Bolt-On Baffles

The bolt-on, air-gap baffles can be removed and replaced without cutting or rewelding.

Learn More

##### AirFX Cutting Deck Tool-Free Cleaning Access

Convenient deck covers can be easily removed without tools. You can also utilize the blow-out ports to save even more time.

Learn More

##### Maintenance-Free Battery

Apart from routine recharge cycles, the powerful lithium-ion battery requires no maintenance for the life of the machine.

##### Versatility

3

##### Accessories

With a variety of accessories geared toward mowing professionals, you can customize your machine for the way you work.

- ECO plate
- Mulching kit
- Striping kit
- 3.75- and 5-bushel poly side bag
- No-flat caster wheel options
- Laser edge blades
- Mulching blades
- High lift blades

Learn More

##### AirFX Cutting Deck Adjustable Front Lip

The AirFX cutting deck's adjustable front lip allows you to optimize your cutting capability for all kinds of mowing conditions and grass types.

Learn More

##### AirFX Cutting Deck Available in Two Sizes

The AirFX cutting deck is available in two sizes:

- 52-inches wide
- 61-inches wide

## Related Models

View All Zero-Turn Mowers
ZT3048SC
ZT3000

#### ZT3048SC

Starting at $7,429 USD*

Deck Size
48 in
Horsepower
20 hp
View Model
ZT2052SB
ZT2000

#### ZT2052SB

Starting at $5,799 USD*

Deck Size
52 in
Horsepower
21.5 hp
View Model
ZT2048SA
ZT2000

#### ZT2048SA

Starting at $5,579 USD*

Deck Size
48 in
Horsepower
21.5 hp
View Model
ZT2042SA
ZT2000

#### ZT2042SA

Starting at $5,419 USD*

Deck Size
42 in
Horsepower
21.5 hp
View Model
ZT3548SF
ZT3500

#### ZT3548SF

Starting at $9,319 USD*

Deck Size
48 in
Horsepower
21.5 hp
View Model
ZT3552SG
ZT3500

#### ZT3552SG

Starting at $9,549 USD*

Deck Size
52 in
Horsepower
22 hp
View Model
ZT3052SD
ZT3000

#### ZT3052SD

Starting at $7,659 USD*

Deck Size
52 in
Horsepower
22 hp
View Model
ZT3561SH
ZT3500

#### ZT3561SH

Starting at $9,919 USD*

Deck Size
61 in
Horsepower
24 hp
View Model
ZT3061SE
ZT3000

#### ZT3061SE

Starting at $7,999 USD*

Deck Size
61 in
Horsepower
24 hp
View Model
ZT6052SL
ZT6000

#### ZT6052SL

Starting at $12,399 USD*

Deck Size
52 in
Horsepower
25.5 hp
View Model
ZT6061SL
ZT6000

#### ZT6061SL

Starting at $12,789 USD*

Deck Size
61 in
Horsepower
25.5 hp
View Model
ZT5052SH
New
ZT5000

#### ZT5052SH

Starting at $10,699 USD*

Deck Size
52 in
Horsepower
25.5 hp
View Model
ZT5061SH
New
ZT5000

#### ZT5061SH

Starting at $10,999 USD*

Deck Size
61 in
Horsepower
25.5 hp
View Model
ZT6161SN
ZT6100

#### ZT6161SN

Starting at $14,199 USD*

Deck Size
61 in
Horsepower
29.5 hp
View Model
ZT7072SP
ZT7000

#### ZT7072SP

Starting at $17,142 USD*

Deck Size
72 in
Horsepower
35 hp
View Model
ZT7061SP
ZT7000

#### ZT7061SP

Starting at $15,902 USD*

Deck Size
61 in
Horsepower
35 hp
View Model
ZT7072SW
ZT7000

#### ZT7072SW

Starting at $18,092 USD*

Deck Size
72 in
Horsepower
38.5 hp
View Model
ZT7061SW
ZT7000

#### ZT7061SW

Starting at $16,972 USD*

Deck Size
61 in
Horsepower
38.5 hp
View Model
ZT6000e
New
ZT6000

#### ZT6000e

Deck Size - 52 in

System Voltage (V)
58 V
View Model
View All Zero-Turn Mowers

WARNING: This product can expose you to chemicals including engine exhaust (including diesel engine exhaust when equipped), lead and lead compounds, mineral oils, soots, phthalates, and carbon monoxide which are known to the State of California to cause cancer and birth defects or other reproductive harm. For more information go to www.P65Warnings.ca.gov.

Certain specification(s) are based on engineering calculations and are not actual measurements. Specification(s) are provided for comparison purposes only and are subject to change without notice. Specification(s) for your individual equipment will vary based on normal variations in design, manufacturing, operating conditions, and other factors.