Pull apart to zoom

Fixed-Base Routers

# MRF23EVS Professional

Fixed-Base Routers

### 2.3 HP Electronic Fixed-Base Router

- Trigger-control system – trigger power switch located in handle for enhanced control
- Powerful 15 Amp motor – produces 10,000 to 25,000 RPM and 2.3 horsepower
- Precision-centering design – makes it easy to keep bit on cutline
- Versatile fixed-base depth adjustment – features 1-5/8 In. continuous microfine adjustment range
- Above-table depth adjustment when fixed base is installed in router table
- Constant Response circuitry – maintains constant speed under load
- Always-on LED lighting – for enhanced visibility in bit area
- Soft-start function – reduces start-up torque
- Two-stage quick clamp system – for fast tool-free conversion
- Variable-speed dial – for matching speed to workpiece and task
- Contoured soft grip handles – for enhanced control and comfort
- Fixed base has threaded holes for mounting to router table positioned in common three-hole pattern
- Cord swivel – for added mobility
- Compatible with optional RA1129 Template Guide Adapter Set – for easy change of Bosch quick-release template guides and common threaded template guides

Show variant

Your Selected Variant
Your Selected Variant
MRF23EVS Professional

## MRF23EVS Professional

Your Selection

Order number: 0601624011

Your selection

## Technical data

### The most important data
Amperage | 15
Base Diameter | 6" Fixed
Base Opening | 3-3/4"
Case Type | No Case Included
Collet Capacity | 1/2" and 1/4"
Dust Collection | No
Fixed-Base Depth Range | 1-5/8"
Horsepower Rating | 2.3
Length in | 6 "
No Load RPM | 10,000-25,000
Rating | 120V AC
Subbase Opening | 2"
Variable Speed | Yes
Voltage | 120V
Weight | 9.3 lb
Width in | 10.25 "
Works With | Router Tables, RA1171 Cabinet-Style Router Table, RA1181 Router Table, RA1152 Offset Bit-Change Wrench Set, Router Guide, RA1054, Template Guides, RA1128 Template Guide Set, RA1129 Template Guide Adapter Set, Centering Device for Subbases and Attached Template Guides, RA1151, Dust Collection Attachments, RA1175 Edge-forming Dust Hood, RA1176AT Two-Hood Dust Hood Set, Plunge Base, MRP01
Includes | Fixed Base (MRF01) 1/4" Self-Releasing Collet Chuck - 2 610 906 283 1/2" Self-Releasing Collet Chuck - 2 610 906 284 16mm Shaft Wrench - 2 610 991 388 24mm Collet Nut Wrench - 2 610 992 417 T-Handle Hex Height Adjustment Wrench - 2610923193 Pack of 3 M4 Screws for table mounting - 2610005966

## MRF23EVS Professional: Further information

### Product Highlights

The Bosch MRF23EVS 2.3 HP Electronic Fixed-Base Router delivers optimum user control, with the trigger-controlled power system that features a power switch in the fixed-base handle. This router has the power to get results, with its 15 Amp motor and adjustable speed settings. The variable-speed dial allows the operator to set the optimal speed. The Bosch Constant Response circuitry in the motor maintains a constant speed throughout the cut, resulting in clean, accurate product. The router has microfine bit-depth adjustment, with a continuous depth range of 1-5/8 in., allowing for accurate and fast changes, while its precision-centering design allows the bit to be centered with the sub-base or optional template guides. Users can glide along the intended cutline using dovetail fixtures, templates, jigs and other guidance devices.

## Fits to MRF23EVS Professional

Router Attachments for Medium & Large Routers

Router Dust Attachments

## Downloads

User Manual

User Manual | o202450v2_2610033452_0214_MR23EVS.pdf (PDF 2.1 MB)
Join our email list

Subscribe now for new product updates and more.

Subscribe
Change of view

In order for the page to be displayed optimally, it must be reloaded. Please click the button below to reload the page.

Reload now