Dealer Login Become A Dealer Find A Dealer Website Tutorial

# Veloci Performance Products

Categories

- Products
- Services
- About Veloci
- Dealer Resources

## Need Assistance?

We are here to help.

Call (866) 686-4020

# MTM Hydro PF22 Foam Cannon

View larger image

This item has been replaced by our new stand-up version 14.7022

MTM Hydro's Italian Manufactured PF22 Foam Cannon is the new standard in the foaming industry. Whether you are foaming down your car on the weekend or you are a professional contract cleaner foaming hog barn for hours, this tool will save you time and money. Simply attach the foam cannon to your pressure washer using one of the included fittings, fill with your desired ratio of chemical and you are up and running.

The MTM Hydro PF22 launched in 2017 as the latest and greatest foam cannon to hit the world stage. The PF22 offers both, adjustable fan blades, and a two stage nozzle allowing you to spray vertically and horizontally. By adjusting the fan blades (narrow or jet) MTM Hydro Foam cannons throw thick foam onto your vehicle, pole barn siding, house, fence, sidewalk, roof or other washable items. The chemical injection knob on top of the PF22 also clicks and allows for precise measurement of more or less chemical to be drawn through the internal chamber, increasing or decreasing the foam output. This allows the internal agitator to create a dense foam that is stickier than the Chinese knock-off foam cannons. In doing so, this thick foam has a longer dwell time which allows the chemical to work on the cleaning surface for longer in its effort to emulsify the dirt and grime. some surfaces may still require some elbow grease, however, if the chemical does its job, very little (if any) scrubbing is required.

NOTE A specific 1/4" Male plug may be required in order to attach the QC plug to the end of some residential pressure washer setups. MTM Hydro 1/4" plugs are standard for industrial use but many residential pressure washers such as Generac, Greenworks, Ryobi, AR Blue Clean,etc... have certain models where the coupler will not receive an MTM plug. Not all of these brands are impacted, just certain models. If you look closely, the Chamfer at the end of an MTM plug as well as the neck is, 1.5mm shorter than some couplers may allow. We now offer this new Low Profile QC plug under item #24.5006. Once you install the correct plug in your new MTM Foam Cannon, you sill see that it was worth finding this specialized fitting as our foam cannons are second to none, even when manufactures try to change their fittings!

Contents of the PF22 Foam Cannon Kit:

- Italian Nickel Plated Brass -Single Cast Foam Cannon body
- Italian Calibrated 32 oz Grey Bottle
- 1/4" x 9" tube for drawing chemical
- 3.5 Orifice (1.25mm) installed in the Foamer Body
- 3.0 Orifice (1.1mm) included with kit
- Fitting pack (2-peices) containing a 1/4" M22 adaptor and 1/4" QC Plated Steel Plug
- Manual with care instructions and exploded view

Specs:

- Min. 1,100 psi - Max. 5,000 psi
- Min. 1.4 gpm - Max. 5.3 gpm
- Max. 140°F

Note: The full spectrum of ratings are not supported by the 3.5 or 3.0 orifices included with this kit. Other orifices may be required for higher flow machines that have lower PSI- Example: 2000 PSI with 3.5 GPM requires a 5.0 Orifice. For larger orifices, you will know it does not work because you will experience starting and stopping of the foam cannon as your unloader slips in and out of bypass. You will also get watery foam as the orifice size 3.5 is significantly smaller than the 5.0 needed for your machine. MTM Foam Cannons will not work with flow sensing unloaders as you will experience the same results listed for an under-sized orifice. See below for additional orifice sizes and replacement items available for purchase.

Foam Cannon Replacement Items and Upgrades:

- 5.0 Orifice (1.5mm) - Part #36.0235
- 6.5 Orifice (1.7mm) - Part #36.0236
- Replacement White Bottle - Part #37.0253
- Replacement Grey (PF22) Bottle - Part #37.0451
- Replacement 9" Suction Tube - Part #41.0338
- Replacement Filter - Part #36.0226
- Repair Kit for Original Foam Cannon including O-Rings - Part #41.0400
- Repair Kit for PF22 Foam Cannon including O-Rings - Part #41.5001
- Karcher Brass Bayonet and fitting - Part #s 24.0459 & 24.0127 Purchase both
- Karcher Plastic Bayonet and fitting - Part #s 37.0259 & 24.0127*Purchase both*
- 1/4" x 33' Hose for Foam Jet Kit with Chem Filter - Part #41.0401"

WARNING

This product can expose you to chemicals, including DINP and/or DEHP which is known to the state of California to cause cancer or birth defects or other reproductive harm, go to www.p65Warnings.ca.gov for more information.

The products we sell are not intended for use in potable water systems and are only for industrial non-drinking water applications.

##### Sales of this product must follow Veloci MAPP pricing

- Sales Flyer
- Manual Manual and Exploded View