1/1
Trimmers

# RedMax TRZ230S

1.37 cu.inch

###### Cylinder displacement

0.94 hp

###### Power output

10.14 lbs

###### Weight (excl. cutting equipment)

#### TRZ230S

This RedMax trimmer is a powerful performer for homeowners as well as commercial contractors. The TRZ230S features a 22.5 cc, 0.94 horsepower engine and its light weight makes the trimmer extra portable for landscaping use. A Strato-Charged engine ensures up to 20% better fuel economy than a traditional two-stroke engine while increasing torque and improving emissions. A steel drive shaft with 7-point splined engagement ensures durability and quick acceleration.
Specifications

#### TRZ230S Article Number: 967 19 41‑01
Engine | TRZ230S Article Number: 967 19 41‑01
Cylinder displacement | 1.37 cu.inch
Clutch engagement speed (±120) | 4,000 rpm
Electrode gap | 0.03 in
Fuel consumption | 450 g/kWh
Fuel tank volume | 21.64 fl oz
Idling speed | 3,000 rpm
Maximum rpm output shaft | 8,208 rpm
Power output | 0.94 hp
Spark Plug | NGK BPMR8Y
Torque, max. | 1 Nm
Torque, max. at rpm | 6,500 rpm
Product data |
Drive gear angle | 60 °
Gear ratio | 1.462
Emission |
Exhaust emissions (CO average) | 495.18 g/kWh
Dimensions |
Weight (excl. cutting equipment) | 10.14 lbs

Owner support
Manuals, handbooks, spare parts, guides, and related information for TRZ230S can be found in the product support.
Product support for TRZ230S