Skip to content

BLACK FRIDAY SALE STARTS NOW

Up to 78% Off Certified Refurbished PC Cases

Roll over image to zoom in Click on image to zoom
/

# TeraMax II 1200W 80+ Gold Certified Power Supply ATX 3.0 / PCI-E 5.0 Modular PSU

Save 19%
Zalman Item Code: ZM1200-TMX2 BK

Color: Black
Variant
Price:
Sale price$169.99 Regular price$210.00
/
Quantity:

Minimum Cart Quantity | Discount | Wholesale Price
--- | --- | ---

Minimum Cart Amount | Cart Discount
--- | ---

### TeraMax II 1200W 80+ Gold Certified Power Supply ATX 3.0 / PCI-E 5.0 Modular PSU

$169.99 $300

- Fully modular design for easy installation and maintenance
- Intel ATX Ver 3.0 type and active PFC for stable and efficient power delivery
- Ultra-quiet 120mm FDB fan with FDB bearing for silent and efficient operation
- Includes 105°C Japanese capacitors for reliable and long-lasting performance
- Supports both SLI and AMD Crossfire for high-performance gaming rigs and workstations
- Multiple protection circuit system for ultimate protection (OCP/OTP/OPP/OVP/UVP/SCP)

Model | ZM1200-TMX2
Efficiency | Max 90% @ 115VAC, Typical Load
Dimensions | 140(L) x 150(W) x 86(H)mm
MTBF | 100,000 Hours
Weight | 2.8kg
Operating Temperature | 10~40℃
PFC | Active PFC
Regulatory | CE, CB, RoHS, EAC, cTUVus, TUV
Type | ATX Ver 3.0
Protection | OCP/OTP/OPP/OVP/UVP/SCP
Input Voltage | 100-240VAC
Input Current | 14-7A
Input Frequency | 50-60Hz
Fan Size | 120mm
Fan Bearing | FDB
Cables (Connector) | Mainboard Cable (1) EPS Cable (2) PCI Express Cable (Connector 2ea) (1) PCI Express Cable (2) IDE (Connector 3ea) + FDD (Connector 1ea) (1) S-ATA (3) 12VHPWR Cable x 1
80 PLUS | Gold

## Recommendations

## Recently Viewed

BUY WITH CONFIDENCE

Minimum 1 Year warranty

MONEY BACK RETURN

30-day Money Back

SECURE PAYMENT

All cards accepted

- Opens in a new window.

Ratings:☆☆☆☆☆