1/9
Gas Leaf Blowers

# HUSQVARNA 125B

12.5 N

###### Blowing Force

9.4 lbs

###### Weight

What's Included
HUSQVARNA 125B - 952 71 19‑25

#### Included

- Nozzle type
  Round+ Flat

#### Not Included

- Harness
- Vacuum Kit

#### 125B

Comfort meets performance with the Husqvarna 125B. With unbeatable performance of 470 CFM at only 9.4 lbs*, this gas blower also features a state-of-the-art ergonomic design to minimize strain on your arms and wrists. And you'll enjoy easier starting with the auto return stop switch and air purge.
Features

#### Powerful, Lightweight Design*

470 CFM for maximum blowing performance at only 9.4 lbs

View more

#### Ergonomic Balanced Design

Balanced for less strain on your arms, shoulders and back

View more

#### Quick Start with Air Purge

Air purge removes air from carburetor and fuel system for easy starting

View more

#### Simple Starting

Stop switch automatically resets to ON so blower is ready for next use

View more

#### Adjustable Tube Length

Easily adjust the blowing tube length for maximum performance

View more

#### Multi-Speed Control

Variable speed throttle with cruise control option for easier handling

View more
Specifications
Compare specifications and features with similar Husqvarna products.
Compare

#### 28cc, handheld blower SKU: 952 71 19‑25
Equipment | 28cc, handheld blower SKU: 952 71 19‑25
Nozzle type | Round+ Flat
Harness | Not included
Vacuum Kit | No
Emission |
Exhaust emissions (CO2 EU V) | 1,392 g/kWh
Engine |
Cylinder displacement | 1.7 cu.inch
Power output | 1.1 hp
Fuel tank volume | 16.91 fl oz
Fuel consumption | 575 g/kWh
Maximum power speed | 8,000 rpm
Idling speed | 3,000 rpm
Electrode gap | 0.024 in
Engine Family CARB | Not Certified for CARB
Capacity |
Air flow in housing | 470 cfm
Air flow in pipe | 425 cfm
Air speed (flat nozzle) | 170 mph
Air speed (round nozzle) | 130 mph
Blowing Force | 12.5 N
Air speed | 170 mph
Dimensions |
Weight | 9.4 lbs
Product size height | 13.4 in
Product size length | 14.9 in
Product size width | 8.1 in
Tube diameter | 2.559 in
Tube length | 25.236 in
Sound and noise |
Sound pressure level at operators ear | 94 dB(A)
Sound power level, measured | 109 dB(A)
Sound power level, guaranteed (LWA) | 112 dB(A)
Vibration |
Equivalent vibration level (ahv, eq) handle | 11.1 m/s²

Reviews
Services

For Homeowners

##### Husqvarna Care™

Get the most out of your equipment with Husqvarna Care™.

For Professionals

##### Husqvarna Financing Solutions

Find the right financing solutions for your commercial or residential outdoor power equipment needs, including zero turn lawn mowers, chainsaws, string trimmers, leaf blowers, snow blowers, string trimmers, and more.

Owner support
Manuals, handbooks, spare parts, guides, and related information for 125B can be found in the product support.
Product support for 125B

#### For 125B

Leaf Blower Attachments

#### Gutter kit

5.0
(1)

### You May Also Be Interested In

(2)
Battery Accessories

#### Battery bag

(No reviews)
Leaf Blower Attachments

#### Nozzle

1.0
(1)

#### You May Also Like

Products & Innovations
Convenience of interchangeable battery products
Learn more
About leaf blowers
Buying Advice
Leaf Blower Buying Guide
Products & Innovations
200 Series Battery Products
How-To's & Guides
Battery Runtime Chart

## Related Content

Buying Advice

##### Things to keep in mind when buying a leaf blower

Stories & Inspiration

##### All seasons lawn care tips and maintenance schedule

Testimonials

##### Why do landscaping companies switch to Husqvarna?

Stories & Inspiration

##### 9 simple tips for your fall lawn care

Golf courses

##### Golf course autonomous mowing and turf care

Stories & Inspiration

##### Winter lawn care and yard maintenance tips

How-To's & Guides

##### What is ethanol free gas and why is ethanol bad for your small engine outdoor power equipment?

Showing 7 of 7